{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["工作表1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"工作表1","index":0,"n_rows":10,"n_cols":8,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[null,"M1(系統更新)",null,null,"選配",150000,300000,"台"]
[null,"M1+M4(1:1)系統+主機",null,null,"選配",300000,650000,"台"]
[null,"M1+M4(2:1)系統+主機",null,null,"選配",300000,600000,"台"]
[null,"每±1停",null,"以15F為基底","選配",3000,6200,"台"]
[null,"殘盲系統",null,"僅線路更換(明鏡、按鈕、光幕、光電管預留)","選配",7627.5,35000,"台"]
[null,"刷卡機系統",null,"僅線路更換(刷卡機子留用)","選配",4430.16,15800,"台"]
[null,"緊急用功能",null,"僅線路更換","選配",0,17000,"台"]
[null,"能量回饋",null,null,"選配",14822.6,40000,"台"]
[null,"雙出入口",null,"僅線路更換(硬體無變更)","選配",7500,15000,"台"]
[null,"ARD自動平層裝置",null,"僅電池(接線)","選配",7156.8,39000,"台"]