{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["目錄","A-1車廂意匠","A-2車廂內裝","A-3車廂外部","A-4控制與其他"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"目錄","index":0,"n_rows":5,"n_cols":1,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,1]]}
["目錄"]
["A-1車廂意匠"]
["A-2車廂內裝"]
["A-3車廂外部"]
["A-4控制與其他"]

{"sheet":"A-1車廂意匠","index":1,"n_rows":12,"n_cols":15,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,7]]}
["A-1 車廂意匠"]
["序號","名稱","編號","規格/備註","配置","成本(NT)","定價","單位","備註","定價*0.75","利潤","%","定價*0.8","利潤","%"]
[1,"車廂意匠","MA002","吊頂：MB005(鑽石銀烤漆+發紋不銹鋼+乳白透光板)\n兩側側板：彩妝鋼板ML001+彩妝鋼板ML002\n後側側板：彩妝鋼板ML001+彩妝鋼板ML002\n前側側板：發紋不銹鋼\n轎門：彩妝鋼板ML002\n地板：PVC(MD001)","標配",8527.68,0,"台","客梯",{"$f":"G3*0.75","v":0},{"$f":"G3-F3","v":-8527.68},{"$f":"K3/F3","v":-1},{"$f":"G3*0.8","v":0},{"$f":"M3-F3","v":-8527.68},{"$f":"N3/F3","v":-1}]
[2,"車廂意匠","MA006","吊頂：MB010(鏡面不銹鋼、透光軟膜)\n兩側側板：鏡面不銹鋼蝕刻鍍黑鈦\n後側側板：鏡面不銹鋼鍍黑鈦+彩妝鋼板 ML005\n前側側板：鏡面不銹鋼鍍黑鈦\n轎門：鏡面不銹鋼蝕刻鍍黑鈦\n地板：大理石(MD011)","選配",67840.125724644298,120000,"台","客梯",{"$f":"G4*0.75","v":90000},{"$f":"G4-F4","v":52159.874275355702},{"$f":"K4/F4","v":0.76886464637561203},{"$f":"G4*0.8","v":96000},{"$f":"M4-F4","v":28159.874275355702},{"$f":"N4/F4","v":0.41509171710048964}]
[3,"車廂意匠","MA005","吊顶：MB009(钻石银烤漆+乳白透光板)\n两侧侧板：彩妆钢板ML002\n后侧侧板：发纹不锈钢+镜面不锈钢\n前侧侧板：发纹不锈钢\n轿门：彩妆钢板ML002\n地板：PVC(MD001)","選配",1532.0237777284799,16000,"台","客梯",12000,14467.97622227152,9.4437021360876514,12800,11267.97622227152,7.354961708870122]
[4,"車廂意匠","MA007","吊顶：MB012(镜面不锈钢、乳白透光板)\n两侧侧板：发纹不锈钢+镜面不锈钢\n后侧侧板：发纹不锈钢+镜面不锈钢\n前侧侧板：发纹不锈钢\n轿门：发纹不锈钢\n地板：PVC(MD005)","選配",12502.538739821835,33600,"台","客梯",25200,21097.461260178163,1.6874541802442604,26880,14377.461260178165,1.1499633441954085]
[5,"車廂意匠","MA008","吊顶：MB011(镜面不锈钢镀黑钛、乳白透光板)\n两侧侧板：镜面不锈钢镀黑钛+防火板\n后侧侧板：镜面不锈钢镀黑钛+防火板\n前侧侧板：镜面不锈钢镀黑钛\n轿门：镜面不锈钢镀黑钛\n地板：PVC(MD013)","選配",0,150000,"台","客梯",112500,150000,{"$error":"#DIV/0!"},120000,120000,{"$error":"#DIV/0!"}]
[6,"車廂意匠","MA017","吊顶：MB010(RAL9005砂纹+乳白透光板)\n两侧侧板：烤漆RAL9003砂纹+镜面不锈钢镀黑钛\n后侧侧板：烤漆RAL9003砂纹+镜面不锈钢镀黑钛\n前侧侧板：烤漆RAL9003砂纹\n轿门：烤漆RAL9003砂纹\n地板：PVC(MD005)","選配",2640.96,27300,"台","小電梯",20475,24659.040000000001,9.3371501272264634,21840,19199.04,7.2697201017811706]
[7,"車廂意匠","MA018","吊顶：MB013(RAL9003砂纹+LED灯板)\n两侧侧板：烤漆RAL9005砂纹+烤漆RAL9003砂纹+\n          镜面不锈钢镀黑钛\n后侧侧板：烤漆RAL9003砂纹+镜面不锈钢镀黑钛\n前侧侧板：烤漆RAL9003砂纹\n轿门：烤漆RAL9003砂纹\n地板：PVC(MD005)","選配",0,10000,"台","小電梯",7500,10000,{"$error":"#DIV/0!"},8000,8000,{"$error":"#DIV/0!"}]
[8,"車廂意匠","MA019","吊顶：MB014(RAL9003砂纹+LED灯板)\n两侧侧板：彩妆钢板ML002+镜面不锈钢\n后侧侧板：彩妆钢板ML002+镜面不锈钢\n前侧侧板：发纹不锈钢\n轿门：彩妆钢板ML002\n地板：PVC(MD006)","標配",17842.5,"-","台","小電梯",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[9,"車廂意匠","MA020","吊顶：MB015(烤漆RAL1015+烤漆RAL9005+\n      LED方灯)\n两侧侧板：彩妆钢板ML006\n后侧侧板：彩妆钢板ML006+镜面饰条\n前侧侧板：发纹不锈钢\n轿门：彩妆钢板ML006\n地板：PVC(MD001)","標配",19651.5,"-","台","小電梯",{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"},{"$error":"#VALUE!"}]
[10,"車廂意匠","MA021","吊顶：MB011(镜面不锈钢镀黑钛+乳白透光板)\n两侧侧板：镜面不锈钢镀黑钛+蚀刻香槟金镀色\n后侧侧板：镜面不锈钢镀黑钛+蚀刻香槟金镀色\n前侧侧板：镜面不锈钢镀黑钛\n轿门：镜面不锈钢镀黑钛\n地板：PVC(MD006)","選配",45692.639999999999,92000,"台","小電梯",69000,46307.360000000001,1.013453370170776,73600,27907.360000000001,0.61076269613662071]

{"sheet":"A-2車廂內裝","index":2,"n_rows":208,"n_cols":7,"rows_kept":208,"cut":false,"hidden":false,"merged":[[0,0,0,6],[141,1,146,1],[147,1,152,1],[134,1,135,1],[95,1,102,1],[103,1,112,1],[116,1,123,1],[124,1,133,1]]}
["A-2 車廂內裝"]
["序號","名稱","編號","規格/備註","配置","成本(NT)","定價"]
["A-2-1天井"]
[1,"天井","MB001","黑色烤漆、乳白透光板","標配",1440,5000]
[2,"天井","MB002","黑色烤漆、乳白透光板","標配",1438.4393541501165,5000]
[3,"天井","MB003","烤漆鋼板、深灰烤漆鋼板、LED方燈","標配",0]
[4,"天井","MB004","香檳色烤漆鋼板、乳白透光板、筒燈","標配",1400.0485685259646,2800]
[5,"天井","MB005","鑽石銀烤漆鋼板邊框、發紋不銹鋼、乳白透光板、筒燈","選配",5203.4237003112748,10500]
[6,"天井","MB006","鏡面不銹鋼、乳白透光板","選配",4676.1646505490453,10000]
[7,"天井","MB007","黑色烤漆鋼板邊框、黑鈦鏡面不銹鋼、乳白透光板、筒燈","選配",6145.9174873843649,13000]
[8,"天井","MB008","鑽石銀烤漆鋼板邊框、鏡面不銹鋼、乳白透光板、筒燈","選配",6145.9174873843649,13000]
[9,"天井","MB009","鑽石銀烤漆鋼板、乳白透光板","選配",4006.4048561946911,8400]
[10,"天井","MB010","鏡面不銹鋼、透光軟膜","選配",23924.241924541471,45000]
[11,"天井","MB011","鏡面不銹鋼鍍黑鈦、乳白透光板","選配",20217.992217850304,45000]
[12,"天井","MB012","鏡面不銹鋼、乳白透光板","標配",4006.4048561946911,8400]
[13,"天井","MB002","SUS304-1.2t發紋不銹鋼（標準：依巨龍標準）","加價",4006.4048561946911,8400]
[14,"天井","MB009","SUS304-1.3t發紋不銹鋼（標準：依巨龍標準）","加價",4006.4048561946911,8400]
[15,"天井","MB003","SUS304-1.4t發紋不銹鋼（標準：依巨龍標準）","加價",7251.4115044248147,12500]
[16,"天井","MB001","SUS304-1.5t發紋不銹鋼（標準：依巨龍標準）","加價",4006.4048561946911,8400]
[17,"天井","MB004","SUS304-1.6t發紋不銹鋼（標準：依巨龍標準）","加價",5628.9081803097597,9500]
[18,"天井","MB002","材質-SUS304-1.5t發紋不銹鋼\n（標準：依巨龍標準）","加價",4927.8779731194754,9500]
[19,"天井","MB009","材質-SUS304-1.6t發紋不銹鋼\n（標準：依巨龍標準）","加價",4927.8779731194754,9500]
[20,"天井","MB003","材質-SUS304-1.7t發紋不銹鋼\n（標準：依巨龍標準）","加價",8919.2361504424953,15500]
[21,"天井","MB001","材質-SUS304-1.8t發紋不銹鋼\n（標準：依巨龍標準）","加價",4927.8779731194754,9500]
[22,"天井","MB004","材質-SUS304-1.9t發紋不銹鋼\n（標準：依巨龍標準）","加價",6923.5570617809854,12500]
[23,"天井","MB002","材質-SUS304-1.5t鏡面不銹鋼\n（標準：依巨龍標準）","加價",5363.41587660396,11500]
[24,"天井","MB009","材質-SUS304-1.6t鏡面不銹鋼\n（標準：依巨龍標準）","加價",5363.41587660396,11500]
[25,"天井","MB003","材質-SUS304-1.7t鏡面不銹鋼\n（標準：依巨龍標準）","加價",9698.7628871681391,17500]
[26,"天井","MB001","材質-SUS304-1.8t鏡面不銹鋼\n（標準：依巨龍標準）","加價",5363.41587660396,11500]
[27,"天井","MB004","材質-SUS304-1.9t鏡面不銹鋼\n（標準：依巨龍標準）","加價",7042.9334236725599,12500]
["A-2-2地板"]
[28,"地板","MD001","PVC","標配",0]
[29,"地板","MD002","PVC","標配",0]
[30,"地板","MD003","PVC","標配",0]
[31,"地板","MD004","PVC","選配",2720.7295964601794,5200]
[32,"地板","MD005","PVC","選配",2720.7295964601794,5200]
[33,"地板","MD006","PVC","選配",2720.7295964601799,5200]
[34,"地板","MD007","PVC","選配",2720.7295964601794,5200]
[35,"地板","MD008","PVC","選配",2720.7295964601794,5200]
[36,"地板","MD009","PVC","選配",1999.158371681418,4200]
[37,"地板","MD010","PVC","選配",3147.112592920359,6500]
[38,"地板","MD011","大理石","選配",16910.073744807556,35000]
[39,"地板","MD012","大理石","選配",16910.073744807556,35000]
[40,"地板地磚貼付BY業主","客梯","P6~P24人 ",null,null,0]
[41,"地板 花紋不鏽鋼板 ","客梯","P6~P13人 (一片式)",null,{"$f":"G45*0.6","v":11772},19620]
[42,"地板 花紋不鏽鋼板 ","客梯","P15人 (一片式)",null,{"$f":"G46*0.6","v":13554},22590]
[43,"地板 花紋不鏽鋼板 ","客梯","P17~P24人 (僅接合式)",null,20898,34830]
[44,"地板_大理石貼付預留","小電梯","P6~P8人",null,5400,9000]
[45,"地板_大理石貼付預留","客梯","P9人",null,8100,13500]
[46,"地板_大理石貼付預留","客梯","P10人(10停)(120M(含)以下)",null,21222,35370]
[47,"地板_大理石貼付預留","客梯","P11人(10停)(120M(含)以下)",null,21816,36360]
[48,"地板_大理石貼付預留","客梯","P12~15人(10停)(60~105m)",null,19602,32670]
[49,"地板_大理石貼付預留","客梯","P17人(60~105m)",null,8046,13410]
[50,"地板_大理石貼付預留","客梯","P20~24人(任何速度)",null,8478,14130]
[51,"地板_大理石貼付預留","客梯","P13人(120M)",null,7668,12780]
[52,"地板_大理石貼付預留","客梯","P15人(20停)(120M)",null,68256,113760]
[53,"地板_大理石貼付預留","客梯","P17人(120M)",null,7452,12420]
[54,"地板_大理石貼付預留","客梯","P13~17人(150M)",null,8316,13860]
[55,"地板_石英磚貼付預留(10mm)","客梯","P6~P24人 ",null,5886,9810]
[56,"地板_大理石貼付預留","客梯","P6~P24人(無機房用)",null,5508,9180]
[57,"地板 花紋不鏽鋼板 (SH)","貨梯","1000kg以內 ",null,12312,20520]
[58,"地板 花紋不鏽鋼板 (SH)","貨梯","1500~2000kg ",null,27810,46350]
[59,"地板 花紋不鏽鋼板 (SH)","貨梯","2500~3000kg ",null,57942,96570]
[60,"地板_車廂地毯(P-11人(含)以下)","客梯",null,null,1836,3060]
[61,"地板_車廂地毯(P-12人(含)以上)","客梯",null,null,2214,3690]
[62,"地板_3M地毯(P-11人(含)以下)","客梯",null,null,2214,3690]
[63,"地板_3M地毯(P-12人(含)以上)","客梯",null,null,2970,4950]
["A-2-3操縱盤"]
[64,"操縱盤","ME001","主操縱盤","標配",0]
[65,"操縱盤","ME002","主操縱盤","選配",0,2500]
[66,"操縱盤","ME003","主操縱盤","選配",57.982300884955805,2500]
[67,"操縱盤","ME004","主操縱盤","選配",151.64601769911465,2500]
[68,"操縱盤","ME005","主操縱盤在ME001基礎上追加語音呼梯","選配",2029.3805309734485,3990]
[69,"操縱盤","ME006","側邊一體式操縱盤","選配",4370.9734513274352,8500]
[70,"操縱盤","ME007","側邊一體式操縱盤在ME006基礎上追加盲文點字板","選配",4518.1592920354051,8700]
[71,"操縱盤","ME008","一體式前側板用","選配",4616.2831858406998,8900]
[72,"操縱盤","ME009","一體式前側板用在ME008基礎上追加盲文點字板","選配",4767.84,9600]
[73,"操縱盤","ME010","外掛式殘障用","選配",4089.9823008849539,8300]
[74,"操縱盤","ME011","嵌入式殘障用","選配",4140.382300884954,8800]
[75,"操縱盤","ME012","外掛式附顯示殘障用","選配",4971.9823008849453,10000]
[76,"操縱盤","ME013","嵌入式附顯示殘障用","選配",4921.5823008849457,10000]
[77,"操縱盤","ME014","在ME002基礎上追加盲文點字板","選配",154.9911504424779,1000]
[78,"操縱盤","ME015","在ME003基礎上追加盲文點字板","選配",54.191150442477003,3500]
[79,"操縱盤","ME016","在ME001基礎上追加電話機鍵盤","選配",1033.2,2500]
[80,"操縱盤","ME017","在ME002基礎上追加電話機鍵盤","選配",1036.9911504424815,2500]
[81,"操縱盤","ME018","在ME003基礎上追加電話機鍵盤","選配",1087.3911504424814,2500]
["A-2-4扶手"]
[82,"扶手","MC001","不銹鋼扁平扶手","選配",1789.4230088495578,2500]
[83,"扶手","MC002","不銹鋼圓形扶手","選配",1342.0672566371684,2500]
[84,"扶手","MC003","不銹鋼彎管扶手","選配",1789.4230088495578,2500]
[85,"扶手","MC004","不銹鋼紅木扶手","選配",2236.7787610619475,4000]
[86,"扶手","MC005","鏡面黑鈦扶手","選配",2268,5000]
[87,"扶手鍍鈦(遠東特殊色)",null,"僅鍍鈦加工費",null,1500,1350]
["A-2-5 車廂門與層門(轎門/層門)"]
[88,"轎門2100mm （標準：噴塗或彩粧鋼板）",null,"SUS304-1.5t發紋不銹鋼","加價",2754,5200]
[89,"轎門2100mm\n（標準：噴塗或彩粧鋼板）",null,"SUS304-1.2t發紋不銹鋼","加價",2292,4800]
[90,null,null,"SUS304-1.5t發紋不銹鋼 鍍鈦","加價",7106.3343716814179,11000]
[91,null,null,"SUS304-1.5t鏡面不銹鋼","加價",3110.9925663716817,9470]
[92,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",7590.6542867256449,13250]
[93,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",6517.2966371681441,13250]
[94,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",8775.2746194690153,16500]
[95,null,null,"四周包邊玻璃轎門SUS304-1.2t發紋不銹鋼","加價",12343.380530973482,30500]
[96,null,null,"四周包邊玻璃轎門SUS304-1.5t鏡面不銹鋼","加價",15376.300884955755,39500]
[97,"層門2100mm\n（標準：噴塗Q235A-1.5t）",null,"SUS304-1.5t發紋不銹鋼","加價",3396.7842690265516,5200]
[98,null,null,"噴塗Q235A-1.2t","加價",-239.05752212389365,0]
[99,null,null,"SUS304-1.2t發紋不銹鋼","加價",2729.2081699115056,4500]
[100,null,null,"SUS304-1.5t發紋不銹鋼 鍍鈦","加價",6224.1653946902406,9500]
[101,null,null,"SUS304-1.5t鏡面不銹鋼","加價",3527.6815433628312,7800]
[102,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",6708.4853097344849,12000]
[103,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",5654.76225132744,12000]
[104,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",7893.1056424778544,15000]
[105,null,null,"四周包邊玻璃層門SUS304-1.2t發紋不銹鋼","加價",15610.619469026518,29000]
[106,null,null,"四周包邊玻璃層門SUS304-1.5t鏡面不銹鋼","加價",21587.256637168182,38000]
[107,"廂門/層門加高200(標準：SUS304-1.5t發紋不銹鋼，高：2100)",null,"SUS304-1.2t發紋不銹鋼","加價",-212.49557522123894,2500]
[108,"廂門/層門加高200(標準：SUS304-1.5t發紋不銹鋼，高：2100)",null,"SUS304-1.5t發紋不銹鋼","加價",392.69182300884944,2500]
[109,"轎門2300mm （標準：噴塗或彩粧鋼板）",null,"SUS304-1.5t發紋不銹鋼","加價",3147,7700]
[110,"轎門2300mm\n（標準：噴塗或彩粧鋼板）",null,"SUS304-1.2t發紋不銹鋼","加價",2685,7300]
[111,null,null,"SUS304-1.5t發紋不銹鋼 鍍鈦","加價",7499,13500]
[112,null,null,"SUS304-1.5t鏡面不銹鋼","加價",3531,11970]
[113,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",8011,15750]
[114,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",6910,15750]
[115,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",9168,19000]
[116,null,null,"四周包邊玻璃轎門SUS304-1.2t發紋不銹鋼","加價",12736,33000]
[117,null,null,"四周包邊玻璃轎門SUS304-1.5t鏡面不銹鋼","加價",15769,42000]
[118,"層門2300mm\n（標準：噴塗Q235A-1.5t）",null,"SUS304-1.5t發紋不銹鋼","加價",3396.7842690265516,7700]
[119,null,null,"噴塗Q235A-1.2t","加價",3158,0]
[120,null,null,"SUS304-1.2t發紋不銹鋼","加價",6126.208169911506,7000]
[121,null,null,"SUS304-1.5t發紋不銹鋼 鍍鈦","加價",9621.1653946902406,12000]
[122,null,null,"SUS304-1.5t鏡面不銹鋼","加價",6924.6815433628308,10300]
[123,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",10105.485309734486,14500]
[124,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",9051.76225132744,14500]
[125,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",11290.105642477854,17500]
[126,null,null,"四周包邊玻璃層門SUS304-1.2t發紋不銹鋼","加價",19007.619469026518,31500]
[127,null,null,"四周包邊玻璃層門SUS304-1.5t鏡面不銹鋼","加價",24984.256637168182,40500]
[128,"臨時層門",null,"冷軋板噴塗1.2t高度：2100","加價",1498.7737911504421,5200]
[129,null,null,"冷軋板噴塗1.2t高度：2300","加價",1590.4018831858425,5400]
[130,"追加臨時廂門 (烤漆)",null,"冷軋板噴塗1.2t高度：2100","加價",{"$f":"G137*0.6","v":3120},5200]
[131,"追加臨時廂門 (烤漆)",null,"冷軋板噴塗1.2t高度：2300","加價",{"$f":"G138*0.6","v":3240},5400]
[132,"廂門層門加高200(標準：噴塗Q235A-1.5t)",null,"冷軋板噴塗1.2t","加價",-148.7469026548674,2500]
[133,"廂門層門加高200(標準：噴塗Q235A-1.5t)",null,"冷軋板噴塗1.5t","加價",130.89727433628315,2500]
["A-2-6 轎壁(車廂側板)"]
[134,"轎壁_P6-P9人乘\n（前側+左右側+後側+車廂門）\n（標準：烤漆/彩妝）\n",null,"SUS304-1.5t 髮紋不銹鋼",null,{"$f":"G134*0.6","v":24300},25200]
[135,null,null,"SUS304-1.5t 髮紋不銹鋼 鍍鈦",null,{"$f":"G135*0.6","v":3120},57750]
[136,null,null,"SUS304-1.5t鏡面不銹鋼","加價",1570.7672920353959,40000]
[137,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",14856.840637168139,66000]
[138,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",13393.171115044244,53000]
[139,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",20187.929628318554,86000]
[140,"轎壁_大梯\n（前側+左右側+後側+車廂門）\n（標準：烤漆/彩妝）",null,"SUS304-1.5t 髮紋不銹鋼","加價",{"$f":"G148*0.6","v":16695},27825]
[141,null,null,"SUS304-1.5t 髮紋不銹鋼 鍍鈦","加價",{"$f":"G149*0.6","v":54180},90300]
[142,null,null,"SUS304-1.5t鏡面不銹鋼","加價",35280,58800]
[143,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",57600,96000]
[144,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",44730,74550]
[145,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",71190,118650]
[146,"轎廂淨高加高200（含加重） （標準：SUS304-1.5t發紋不銹鋼，淨高：2300）",null,"SUS304-1.5t發紋不銹鋼","加價",12600,21000]
[147,"車廂特殊裝潢\n（標準：SUS304-1.5t發紋不銹鋼，淨高：2300）",null,"3側板中間片鏡面不銹鋼SUS304-1.5t，\n其中後側板鏡面不銹鋼SUS304-1.5t需及閘同寬","加價",13250.374088495581,22000]
[148,"側板單片特殊(烤漆→不鏽鋼)",null,"(烤漆→不鏽鋼髮紋)",null,{"$f":"G156*0.6","v":2484},4140]
[149,"側板單片特殊(烤漆→不鏽鋼)",null,"(烤漆→鏡面不鏽鋼)",null,{"$f":"G157*0.6","v":3510},5850]
[150,"側板單片特殊",null,"(烤漆→不鏽鋼髮紋 鍍鈦)",null,4212,7020]
[151,"側板單片特殊",null,"(烤漆→鏡面 不鏽鋼 鍍鈦)",null,5022,8370]
[152,"側板單片特殊",null,"(烤漆→鏡面 不鏽鋼 蝕刻)",null,5022,8370]
[153,"車廂前側 RT PANEL(髮紋不鏽鋼)",null,"P6~24人(不含廂門)",null,3240,5400]
[154,"車廂前側 RT PANEL(髮紋不鏽鋼鍍鈦)",null,"P6~24人(不含廂門)",null,9072,15120]
[155,"車廂前側 RT PANEL(鏡面不鏽鋼)",null,"P6~24人(不含廂門)",null,7074,11790]
[156,"OPB(前)側&CPI  烤漆→髮紋不鏽鋼",null,"P6~24人(不含廂門)",null,3456,5760]
[157,"OPB(前)側&CPI 烤漆→仿鍍鈦",null,"P6~24人(不含廂門)",null,2484,4140]
[158,"側板單片特殊",null,"不鏽鋼髮紋(遠東特殊色)",null,16400,14760]
[159,"側板單片特殊(CE→SH-E(遠東特殊色))",null,"不鏽鋼蝕刻(遠東特殊色)",null,23300,20970]
[160,"側板單片特殊(CE→SM(遠東特殊色))",null,"鏡面不鏽鋼(遠東特殊色)",null,18100,16290]
[161,"側板單片特殊(CE→SM-E(遠東特殊色))",null,"CE→SM-E(遠東特殊色)",null,26600,23940]
[162,"車廂前側 RT PANEL(SH鍍鈦遠東特殊色)",null,"P6~24人(不含廂門)",null,27300,24570]
[163,"車廂前側 RT PANEL(SM鍍鈦遠東特殊色)",null,"P6~24人(不含廂門)",null,37900,34110]
["A-2-7 其他車廂內裝配件"]
[164,"二合一光幕(標準門高2100)",null,null,"加價",4906.1946902654699,11000]
[165,"紫外線殺菌燈（型號：TL-16W）P社已有",null,null,"加價",2217.6,5700]
[166,"風扇出風口",null,null,"加價",252,1500]
[167,"SHARP清淨機（臺灣）",null,null,"加價",27512,45000]
[168,"冷氣（臺灣）",null,null,"加價",38024,65000]
[169,"副操作盤",null,null,"加價",5095.4399999999996,13000]
[170,"語音合成裝置",null,"語音報站器","加價",1033.2,4200]
[171,"車廂攝影機",null,null,"加價",1338.0530973451337,12000]
[172,"CCTV配線預留",null,"5C FV線材(標準)","加價",null,13000]
[173,"無線遠端對講系統",null,null,"加價",3978,7500]
[174,"殘障電梯(殘障OPB、殘障IND、殘障扶手、後側鏡面、語音合成)",null,"二、超過十層樓之各層樓地板面積之和達500平方公尺者需設置。","加價",7627.5,35000]
[175,"開門延長",null,"三、超過十層樓之部分為樓梯間、昇降機間、機械室、裝飾塔、屋頂窗及其他類似用途之建築物不需設置。","加價",80.64,1000]
[176,"刷卡機系統",null,"MCTC-IC-A2","加價",4430.16,12000]
[177,"多媒體屏",null,"13寸","加價",14616,53000]
[178,"車廂側板附壁鉤",null,"P6~P24人","加價",{"$f":"G187*0.6","v":5400},9000]
[179,"側板附壁鉤及保護掛毯(牛仔布)",null,"P6~P12人","加價",{"$f":"G188*0.6","v":14958},24930]
[180,"側板附壁鉤及保護掛毯(牛仔布)",null,"P13~P20人","加價",17172,28620]
[181,"側板附壁鉤及保護掛毯(牛仔布)",null,"P24人","加價",19386,32310]
[182,"明鏡嵌入式(僅車廂後側)預留10mm",null,"P6~P24人(不包含鏡子,單純因應側板特殊所需加工及設計費)","加價",4860,8100]
[183,"明鏡嵌入式(車廂三側)預留10mm",null,"P6~P24人(不包含鏡子,單純因應側板特殊所需加工及設計費)","加價",9558,15930]
[184,"凸面鏡",null,"千鳥,展望有殘障時加計","加價",864,1440]
[185,"半身明鏡　　　　　　　　　　",null,null,"加價",3186,5310]
[186,"中間片全身明鏡　　　",null,null,"加價",3186,5310]
[187,"車廂內法特殊",null,"客梯P6~P24人","加價",9450,15750]
[188,"車廂內法特殊",null,"貨梯-1000kg~2000kg","加價",15606,26010]
[189,"車廂內法特殊",null,"貨梯-2500kg~3000kg","加價",20196,33660]
[190,"車廂附防撞板  不鏽鋼",null,"P6~P12人","加價",15984,26640]
[191,"車廂附防撞板  不鏽鋼",null,"P13~P17人","加價",19224,32040]
[192,"車廂附防撞板  不鏽鋼",null,"P20~P24人","加價",20466,34110]
[193,"車廂附防撞板  (橡膠)",null,"F-1000kg","加價",34020,56700]
[194,"車廂附防撞板  (橡膠)",null,"F-1500kg~2000kg","加價",39096,65160]
[195,"車廂附防撞板  (橡膠)",null,"F-2500kg~3000kg","加價",48330,80550]
[196,"車廂附防撞板  不鏽鋼",null,"F-1000kg","加價",23274,38790]
[197,"車廂附防撞板  不鏽鋼",null,"F-1500kg~2000kg","加價",28944,48240]
[198,"車廂附防撞板  不鏽鋼",null,"F-2500kg~3000kg","加價",33372,55620]
[199,"車廂預留裝潢重量",null,null,"加價",null,150]

{"sheet":"A-3車廂外部","index":3,"n_rows":114,"n_cols":8,"rows_kept":114,"cut":false,"hidden":false,"merged":[[0,0,0,7],[100,1,101,1],[102,1,103,1]]}
["A-3 車廂外部"]
["序號","名稱","編號","規格/備註","配置","成本(NT)","定價","單位"]
["A-3-1 小門框"]
[1,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t發紋不銹鋼","加價",641.3966442477855,1500,"停"]
[2,"小門框(標準：噴塗Q235A-1.5t)\n",null,"噴塗Q235A-1.2t","加價",-42.499115044247787,0,"停"]
[3,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.2t發紋不銹鋼","加價",556.31341592920353,1300,"停"]
[4,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t鏡面不銹鋼","加價",844.28741946902403,2300,"停"]
[5,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",1433.3251539823018,3500,"停"]
[6,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",1164.9857415929189,5000,"停"]
[7,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",1727.844021238941,7500,"停"]
[8,"小型門框 髮紋不鏽鋼 鍍鈦",null,"2P-CO ≦OP-800~1100",null,{"$f":"G11*0.6","v":1242},2070,"停"]
[9,"小型門框 鏡面不鏽鋼",null,"2P-CO ≦OP-800~1100",null,{"$f":"G12*0.6","v":1188},1980,"停"]
[10,"小型門框 鏡面不鏽鋼 鍍鈦",null,"2P-CO ≦OP-800~1100",null,1674,2790,"停"]
[11,"小型門框 髮紋不鏽鋼",null,"2P-CO≦OP-800~1100*2300H",null,{"$f":"G14*0.6","v":378},630,"停"]
[12,"小型門框 仿鍍鈦烤漆",null,"2P-CO ≦OP-800~1100",null,1350,2250,"停"]
[13,"大型門框 髮紋不鏽鋼HH=2100 A=240",null,"OP-800~1100  A值≦380",null,6426,10710,"停"]
[14,"大型門框 髮紋不鏽鋼鍍鈦 HH=2100 A=240",null,"OP-800~1100  A值≦380",null,10476,17460,"停"]
[15,"大型門框 鏡面不鏽鋼 HH=2100 A=240",null,"OP-800~1100  A值≦380",null,8532,14220,"停"]
[16,"大型門框 鏡面不鏽鋼 鍍鈦 HH=2100 A=240",null,"OP-800~1100  A值≦380",null,13068,21780,"停"]
[17,"大型門框 仿鍍鈦烤漆 HH=2100 A=240",null,"OP-800~1100  A值≦380",null,56160,93600,"停"]
[18,"小型門框附幕板 髮紋不鏽鋼",null,"OP-800~1100 全高≦3000",null,7290,12150,"停"]
[19,"小型門框附幕板 髮紋不鏽鋼 鍍鈦",null,"OP-800~1100 全高≦3000",null,11124,18540,"停"]
[20,"小型門框附幕板 鏡面不鏽鋼",null,"OP-800~1100 全高≦3000",null,9072,15120,"停"]
[21,"小型門框附幕板 鏡面不鏽鋼 鍍鈦",null,"OP-800~1100 全高≦3000",null,12744,21240,"停"]
[22,"小框附幕板  仿鍍鈦烤漆",null,"OP-800~1100 全高≦3000",null,7830,13050,"停"]
[23,"大型門框附幕板 髮紋不鏽鋼",null,"OP-800~1100 全高≦3000",null,15714,26190,"停"]
[24,"大型門框附幕板 髮紋不鏽鋼 鍍鈦",null,"OP-800~1100 全高≦3000",null,20682,34470,"停"]
[25,"大型門框附幕板 鏡面不鏽鋼",null,"OP-800~1100 全高≦3000",null,17442,29070,"停"]
[26,"大型門框附幕板 鏡面不鏽鋼 鍍鈦",null,"OP-800~1100 全高≦3000",null,22356,37260,"停"]
[27,"大框附幕板  仿鍍鈦烤漆",null,"OP-800~1100  A值≦380",null,12852,21420,"停"]
[28,"一體式門框",null,"OP-800~1100全高≦3000",null,12000,5580,"停"]
[29,"小型門框 髮紋不鏽鋼 鍍鈦",null,"2S-2P  OP-1100~1200W",null,{"$f":"G32*0.6","v":2376},3960,"停"]
[30,"小型門框 鏡面不鏽鋼",null,"2S-2P  OP-1100~1200W",null,{"$f":"G33*0.6","v":2052},3420,"停"]
[31,"小型門框 髮紋不鏽鋼 鍍鈦",null,"2S-2P  OP-1100~1200W",null,2376,3960,"停"]
[32,"大型門框 髮紋不鏽鋼",null,"2S-1100.1200  A值≦380",null,6372,10620,"停"]
[33,"大型門框 髮紋不鏽鋼 鍍鈦",null,"2S-1100.1200  A值≦380",null,11016,18360,"停"]
[34,"大型門框 鏡面不鏽鋼",null,"2S-1100.1200  A值≦380",null,9990,16650,"停"]
[35,"大型門框 鏡面不鏽鋼　鍍鈦",null,"2S-1100.1200  A值≦380",null,13392,22320,"停"]
[36,"大型門框 髮紋不鏽鋼",null,"2S-1400~1700W  A值≦380",null,7614,12690,"停"]
[37,"大型門框 髮紋不鏽鋼",null,"4C-1700~2300W  A值≦380",null,11772,19620,"停"]
[null,"小型門框 SH鍍鈦(遠東特殊色)",null,"2P-CO ≦OP-800~1100",null,{"$f":"G41*0.6","v":2214},3690,{"$f":"F41-G41","v":-1476}]
[null,"小型門框 SM鍍鈦(遠東特殊色)",null,"2P-CO ≦OP-800~1100",null,{"$f":"G42*0.6","v":2592},4320,-1728]
[null,"小型門框  亂紋鍍鈦(遠東特殊色)",null,"2P-CO ≦OP-800~1100",null,4698,7830,-3132]
[null,"小型門框  霧珠鍍鈦(遠東特殊色)",null,"2P-CO ≦OP-800~1100",null,4806,8010,-3204]
[null,"大型門框 SH鍍鈦(遠東特殊色)",null,"OP-800~1100  A值≦380",null,16902,28170,-11268]
[null,"大型門框 SM鍍鈦(遠東特殊色)",null,"OP-800~1100  A值≦380",null,19494,32490,-12996]
[null,"大型門框  亂紋鍍鈦(遠東特殊色)",null,"OP-800~1100  A值≦380",null,20682,34470,-13788]
[null,"大型門框  霧珠鍍鈦(遠東特殊色)",null,"OP-800~1100  A值≦380",null,20898,34830,-13932]
[null,"小框附幕板 SH鍍鈦(遠東特殊色)",null,"OP-800~1100 全高≦3000",null,15552,25920,-10368]
[null,"小框附幕板 SM鍍鈦(遠東特殊色)",null,"OP-800~1100 全高≦3000",null,17064,28440,-11376]
[null,"小框附幕板  亂紋鍍鈦(遠東特殊色)",null,"OP-800~1100 全高≦3000",null,17874,29790,-11916]
[null,"小框附幕板  霧珠鍍鈦(遠東特殊色)",null,"OP-800~1100 全高≦3000",null,18036,30060,-12024]
[null,"大框附幕板 SH鍍鈦(遠東特殊色)",null,"OP-800~900 全高≦3000",null,29808,49680,-19872]
[null,"大框附幕板 SM鍍鈦(遠東特殊色)",null,"OP-800~900 全高≦3000",null,31428,52380,-20952]
[null,"大框附幕板 SH鍍鈦(遠東特殊色)",null,"OP-1000~1100全高≦3000",null,30402,50670,-20268]
[null,"大框附幕板 SM鍍鈦(遠東特殊色)",null,"OP-1000~1100全高≦3000",null,33966,56610,-22644]
[null,"大框附幕板  亂紋鍍鈦(遠東特殊色)",null,"OP-800~900  A值≦380",null,33264,55440,-22176]
[null,"大框附幕板  亂紋鍍鈦(遠東特殊色)",null,"OP-1000~1100  A值≦380",null,36126,60210,-24084]
[null,"大框附幕板  霧珠鍍鈦(遠東特殊色)",null,"OP-800~900  A值≦380",null,33534,55890,-22356]
[null,"大框附幕板  霧珠鍍鈦(遠東特殊色)",null,"OP-1000~1100  A值≦380",null,36396,60660,-24264]
[null,"小型門框 SH鍍鈦(遠東特殊色)",null,"2S-2P  OP-1100~1200W",null,4806,8010,-3204]
[null,"小型門框 SM鍍鈦(遠東特殊色)",null,"2S-2P  OP-1100~1200W",null,5508,9180,{"$f":"F62-G62","v":-3672}]
[null,"大型門框 SH鍍鈦(遠東特殊色)",null,"2S-1100.1200  A值≦380",null,18144,30240,{"$f":"F63-G63","v":-12096}]
[null,"大型門框 SM鍍鈦(遠東特殊色)",null,"2S-1100.1200  A值≦380",null,20520,34200,{"$f":"F64-G64","v":-13680}]
["A-3-2 外呼(乘場指示器)"]
[38,"外呼","MF001","不銹鋼有底盒","標配",0,null,"停"]
[39,"外呼","MF002","並聯不銹鋼有底盒","選配",789.45132743362797,1600,"停"]
[40,"外呼","MF003","不銹鋼無底盒","選配",0,null,"停"]
[41,"外呼","MF004","並聯不銹鋼無底盒","選配",227.46902654867264,525,"停"]
[42,"外呼","MF005","液晶無底盒","選配",762.6902654867265,1600,"停"]
[43,"外呼","MF006","液晶無底盒","選配",762.6902654867265,1800,"停"]
[44,"外呼","MF007","殘障有底盒附盲文點字板","選配",414.79646017699127,1000,"停"]
[45,"外呼","MF008","殘障並聯有底盒附盲文點字板","選配",1239.9292035398205,2500,"停"]
[46,"外呼","MF009","殘障並聯手勢呼梯有底盒附盲文點字板","選配",1342.5132743362847,2700,"停"]
[47,"外呼","MF010","手勢呼梯有底盒","選配",499.539823008849,1050,"停"]
[48,"外呼","MF011","殘障無底盒附盲文點字板和MF012搭配用","選配",13.380530973451334,500,"停"]
[49,"外呼","MF012","殘障無底盒和MF011搭配用","選配",303.29203539823015,500,"停"]
[50,"外呼","MF013","無接觸式外呼","選配",3269.3097345132733,4500,"停"]
[51,"外呼","MF014","殘障+手勢呼梯有底盒附盲文點字板","選配",517.38053097344846,1500,"停"]
[52,"外呼","MF015","殘障有底盒和MF001搭配用","選配",334.51327433628313,1000,"停"]
[53,"外呼","MF016","殘障有底盒","選配",365.73451327433611,1000,"停"]
[54,"外呼","MF017","殘障手勢呼梯有底盒","選配",463.85840707964553,1000,"停"]
[55,"外呼","MF018","手勢呼梯有底盒附盲文點字板","選配",102.5840707964604,400,"停"]
[56,"外呼","MF019","並聯殘障有底盒附盲文點字板，左側","選配",1373.7345132743371,2800,"停"]
[57,"外呼","MF020","並聯殘障有底盒附盲文點字板，右側","選配",1373.7345132743371,2800,"停"]
[58,"外呼","MF021","無底盒","選配",160.56637168141577,400,"停"]
[59,"外呼","MF022","無底盒帶手勢呼梯","選配",182.86725663716851,400,"停"]
[60,"群管裡(2台聯動)",null,null,"選配",{"$f":"G88*0.6","v":4740},7900,"群"]
[61,"群管理 (3~8台/群)",null,"3~8台群管理(無群管理盤)","選配",{"$f":"G89*0.6","v":33780},56300,"群"]
[62,"人流管控(群)",null,"僅限一層樓(一般為大廳)","選配",null,"特殊詢價","群"]
["A-3-3 到站燈"]
[63,"到站燈","MG001",null,"選配",1110.5840707964594,2500,"停"]
[64,"到站燈","MG002",null,"選配",1110.5840707964594,2500,"停"]
[65,"到站燈","MG003",null,"選配",2872.3539823008882,6000,"停"]
[66,"到站燈","MG004",null,"選配",1436.1769911504421,2900,"停"]
[67,"到站燈","MG005",null,"選配",1855.4336283185864,4000,"停"]
[68,"到站燈","MG006",null,"選配",2368.3539823008882,5500,"停"]
["A-3-4 門開方式與門"]
[69,"2P-CO→2S-2P(台)",null,"P6~24人(OP≦1100)","加價",{"$f":"G99*0.6","v":4800},8000,"台"]
[70,"2P-CO→2S-2P(停)",null,"P6~24人(OP≦1100)","加價",{"$f":"G100*0.6","v":3000},5000,"停"]
[71,"貫通門-轎廂（轎門標準SUS304-1.5t）",null,"SUS304-1.5t","加價",15469.677876106171,85000,"台"]
[72,null,null,"冷軋板噴塗1.5t","加價",13089.727433628315,80000,"台"]
[73,"貫通門-乘場（層門門框標準Q235A-1.5t）",null,"冷軋板噴塗1.5t","加價",4164.9132743362798,9000,"停"]
[74,null,null,"SUS304-1.5t","加價",8151.3302654867402,15000,"停"]
[75,"千鳥型",null,"P9人","加價",{"$f":"G105*0.6","v":7800},13000,"台"]
[76,"千鳥型",null,"P10~P11人","加價",{"$f":"G106*0.6","v":9600},16000,"台"]
[77,"千鳥型",null,"P12~P15人","加價",9000,15000,"台"]
[78,"千鳥型",null,"P17~P24人","加價",79200,132000,"台"]
[79,"L型千鳥",null,"P9人","加價",195000,325000,"台"]
[80,"L型千鳥",null,"P10~P11人","加價",216000,360000,"台"]
[81,"L型千鳥",null,"P12~P15人","加價",204000,340000,"台"]
[82,"千鳥型",null,"貨梯1000kg~2000kg ","加價",90000,150000,"台"]
[83,"千鳥型",null,"貨梯2500kg~3000kg","加價",120000,200000,"台"]
[87,"防火門(停)(2P-CO)",null,"不鏽鋼","加價",15600,26000,"停"]

{"sheet":"A-4控制與其他","index":4,"n_rows":48,"n_cols":7,"rows_kept":48,"cut":false,"hidden":false,"merged":[[0,0,0,6]]}
["A-4 控制與其他"]
["序號","名稱","編號","規格/備註","配置","成本(NT)","定價"]
["A-4-1 功能與配置"]
[1,"專用運轉",null,"操作電梯，可提供客戶做專用運轉(例：看來車廂人滿了,直接經過外面叫車之樓層，直接到達服務樓層","加價",{"$f":"G4*0.6","v":720},1200]
[2,"車廂追加到樓鈴",null,"到樓鈴: 電子","加價",{"$f":"G5*0.6","v":1500},2500]
[3,"乘場追加到樓鈴",null,"到樓鈴: 電子","加價",780,1300]
[4,"對講機配線至管理員室以100M計(不含配管)　　　　　　　　　　",null,null,"加價",10500,17500]
[5,"對講機線材100M計　　　　　　　　　　",null,null,"加價",6720,11200]
[6,"車廂預留電話機接點",null,"僅接點預留","加價",8040,13400]
[7,"追加電話機(工廠配合留孔)",null,null,"加價",420,700]
[8,"追加電話機(工事現地配合鑽孔)",null,"針對現地配合的人工費用","加價",4200,7000]
[9,"車廂預留刷卡機接點",null,"僅接點預留","加價",6000,10000]
[10,"車廂預留刷卡機接點+面板開孔",null,"僅接點預留&面板留孔","加價",9480,15800]
[11,"遠隔監控 (組)",null,"1~7台/組 (配賦於第1台)","加價",9480,15800]
[12,"遠隔監控工事配線費(EAS)",null,null,"加價",3780,6300]
[13,"物聯網(BY工務購買)",null,"1~4台/組用, 5~8台/2組","加價",10860,18100]
[14,"廂內監控(需搭配物聯網)",null,"物聯網費用需另計","加價",116820,194700]
[15,"直話機系統",null,"與車廂內\"緊急呼叫\"共用按鈕\n1.按下3秒內,為一般緊急呼叫,可與升降道外對講\n2.按著超過3秒以上,則直接撥通電話至設定的第一組號碼(一般來說可設置6組號碼)，無人接聽時往下一組號碼撥號\n(需請客戶申請市話，方能用電話線接進去，需預先錄製語音)\n適用:EAS,VAG","加價",9480,15800]
[16,"火警受信運轉",null,"WL432","加價",4334.4000000000005,6300]
[17,"火災管制",null,"火災管制：當兩台電梯聯動時，其中一台為緊急用電梯，則隔壁台需有火災管制功能","加價",{"$f":"G20*0.6","v":2880},4800]
[18,"緊急用",null,"緊急用：一、建築物高度超過十層樓以上部分之最大一層樓地板面積，在1500平方公尺以下者，至少應設置一座：超過1500平方公尺時，每達3000平方公尺，增設一座。","加價",{"$f":"G21*0.6","v":10200},17000]
[19,"ARD",null,"四、超過十層樓之各層樓地板面積之和未達500平方公尺者不需設置。","加價",7156.8,30000]
[20,"停機操作",null,null,"加價",100.8,500]
[21,"滿載直駛",null,"操作盤檢修增加直駛開關非標加價","加價",1008,3000]
[22,"能量回饋",null,null,"加價",14822.64,42000]
[23,"對重附安全鉗（包含限速器等）",null,"P8-P15","加價",15610.619469026518,42000]
[24,"對重附安全鉗（包含限速器等）",null,"P17",null,{"$f":"G27*0.6","v":37800},63000]
[25,"對重附安全鉗（包含限速器等）",null,"P24",null,{"$f":"G28*0.6","v":44100},73500]
[26,"井道頂部追加防沖梁",null,null,"加價",2520,6500]
[27,"人臉識別",null,null,"加價",{"$f":"G30*0.6","v":39000},65000]
[null,"地震感知器",null,null,null,40000,40000]
["A-4-2 OH與樓高"]
[28,"OH ≧7.5M",null,"P6~P11人","加價",{"$f":"G33*0.6","v":9300},15500]
[29,"OH ≧7.5M",null,"P12~P15人","加價",{"$f":"G34*0.6","v":10140},16900]
[30,"OH ≧7.5M",null,"P17~P24人","加價",12120,20200]
[31,"OH ≧7.5M",null,"B-750~1000kg ","加價",11040,18400]
[32,"OH ≧7.5M",null,"F-1000kg ","加價",12420,20700]
[33,"OH ≧7.5M",null,"F-1500~2000kg ","加價",15300,25500]
[34,"OH ≧7.5M",null,"F-2500~3000kg ","加價",21180,35300]
[35,"OH 超過6M",null,null,"加價",3780,6300]
[36,"OH>5M,追加吊樑施工",null,"僅VAG無機房機種","加價",3780,6300]
[37,"樓高 ≧ 6M",null,"P6~P11人","加價",8280,13800]
[38,"樓高 ≧ 6M",null,"P12~P15人","加價",9060,15100]
[39,"樓高 ≧ 6M",null,"P17~P24人","加價",11160,18600]
[40,"樓高 ≧ 6M",null,"B-750~1000kg ","加價",10080,16800]
[41,"樓高 ≧ 6M",null,"F-1000kg ","加價",11520,19200]
[42,"樓高 ≧ 6M",null,"F-1500~2000kg ","加價",14340,23900]
[43,"樓高 ≧ 6M",null,"F-2500~3000kg ","加價",20280,33800]