{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["價審單","OPTION表","附表一"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"價審單","index":0,"n_rows":34,"n_cols":15,"rows_kept":34,"cut":false,"hidden":false,"merged":[[4,6,6,9],[6,4,7,4],[6,5,7,5],[1,1,1,2],[0,0,0,9],[1,5,3,9],[2,3,2,4],[3,1,3,2],[25,0,28,0],[29,0,30,0],[31,0,31,1],[8,0,8,4],[16,0,16,9],[8,5,8,9],[23,5,23,9],[23,0,23,2],[31,5,31,9],[15,0,15,2]]}
["價     審     單"]
["卷       號","M220276",null,"營業員","林易增","特記事項：\n1、60萬 破價77.9% 內含1萬介紹費，扣除介紹費總價59萬 破價76.6%。。\n2、。。\n3、。。",{"$nulls":5},"未稅(單價)","未稅(複價)","未稅(單價)","未稅(複價)"]
["客戶名稱","大田土木包工業","案件名稱","陳正得",{"$nulls":7},"未稅(單價)","未稅(複價)","未稅(單價)","未稅(複價)"]
["工地地址","台南市中西區西賢二街109巷5號旁",null,"詢價單號",{"$nulls":7},"未稅(單價)","未稅(複價)","未稅(單價)","未稅(複價)"]
["預定成交日","112/4/13","預訂交期","112/11/30","罰則","0/1000天","1.業務員權限>=80%以上；<80-75%呈至業務協理審核；<75%以下呈至總經理審核，並附上《附表一》。\n2.如有訂金保證金(函)、履約保證金(函)、保固保證金(函)需呈至顧問審核.",{"$nulls":4},"未稅(單價)","未稅(複價)","未稅(單價)","未稅(複價)"]
["總台數",{"$f":"SUM(D11:D15)","v":1},"保證金或保函",0,"破價%","批示售價",{"$nulls":5},"未稅(單價)","未稅(複價)","未稅(單價)","未稅(複價)"]
["牌價總額",{"$f":"E16+E24","v":770500},"售價總額",600000,{"$f":"D7/B7","v":0.77871512005191434},{"$nulls":6},"未稅(單價)","未稅(複價)","未稅(單價)","未稅(複價)"]
["破價總額",{"$f":"D7-B7","v":-170500},"破價(台)",{"$f":"B8/B6","v":-170500}]
["整機單價",{"$nulls":4},"業務部作業區"]
["項次","規  格","單價","數量","複價","金額(含稅)","價審%","配賦(含稅)","毛利(含稅)","備  註",null,"未稅(單價)","未稅(複價)","未稅(單價)","未稅(複價)"]
[1,"MAH100-6*5-2S45",732000,1,{"$f":"D11*C11","v":732000},{"$nulls":6},{"$f":"ROUND(F11/D11/1.05,-3)","v":0},{"$f":"L11*D11","v":0},1950000,1950000]
[2,null,null,null,{"$f":"D12*C12","v":0},{"$nulls":6},{"$f":"ROUND(F12/D12/1.05,-3)","v":{"$error":"#DIV/0!"}},{"$f":"L12*D12","v":{"$error":"#DIV/0!"}},1979000,1979000]
[3,null,null,null,0]
[4,null,null,null,0]
[5,null,null,null,0]
[null,null,null,"小計",{"$f":"SUM(E11:E15)","v":732000}]
["OPTION加價"]
["項次","選配規格","單價","數量","複價","項次","選配規格","單價","數量","複價",null,{"$f":"ROUND(F18/#REF!/1.05,-3)","v":{"$error":"#VALUE!"}},{"$f":"L18*#REF!","v":{"$error":"#VALUE!"}},2023000,2023000]
[1,"大理石貼付預留",9500,1,{"$f":"C19*D19","v":9500},6,null,null,null,{"$f":"H19*I19","v":0}]
[2,"MA017轎廂",26000,1,{"$f":"C20*D20","v":26000},7,null,null,null,{"$f":"H20*I20","v":0}]
[3,"扶手",3000,1,3000,8,null,null,null,0]
[4,null,null,null,0,9,null,null,null,0]
[5,null,null,null,0,10,null,null,null,0]
["加價價格請參考表下OPTION表",null,null,"小計",{"$f":"SUM(E19:E23,J19:J23)","v":38500},"藍字部分營業必須填寫資料，黑字部分由業務部填寫"]
["付款辦法","款別","比列","金額","票期","批示比例"]
["材料","1、訂金",0.2,{"$f":"C26*D7","v":120000},"電匯"]
[null,"2、貨到工地款",0.5,{"$f":"C27*D7","v":300000},"電匯"]
[null,null,null,{"$f":"C28*D7","v":0}]
[null,null,null,{"$f":"C29*D7","v":0}]
["安裝","3、安裝完畢款",0.2,{"$f":"C30*D7","v":120000},"電匯"]
[null,"4、驗收款",0.1,{"$f":"C31*D7","v":60000},"電匯"]
["合計",null,{"$f":"SUM(C26:C31)","v":0.99999999999999989},{"$f":"SUM(D26:D31)","v":600000}]
["總經理",null,"業務部\n協理",null,"業務部\n承辦人",null,"區經理",null,"營業員","林易增"]
[{"$nulls":9},"版次：1.1"]

{"sheet":"OPTION表","index":1,"n_rows":1059,"n_cols":12,"rows_kept":1059,"cut":false,"hidden":false,"merged":[[877,11,878,11],[880,11,885,11],[890,11,893,11],[805,11,810,11],[819,11,820,11],[842,4,842,5],[858,11,861,11],[862,11,865,11],[875,11,876,11],[782,11,784,11],[785,11,787,11],[789,11,791,11],[792,11,795,11],[797,11,799,11],[800,11,803,11],[716,4,716,5],[717,4,717,5],[718,4,718,5],[735,11,736,11],[738,11,739,11],[779,11,781,11],[710,4,710,5],[711,4,711,5],[712,4,712,5],[713,4,713,5],[714,4,714,5],[715,4,715,5],[608,11,635,11],[677,11,679,11],[682,11,683,11],[687,11,690,11],[691,11,694,11],[698,11,699,11],[535,11,540,11],[543,11,545,11],[564,11,565,11],[566,11,568,11],[569,11,571,11],[595,5,596,5],[595,11,597,11],[477,11,479,11],[480,11,482,11],[483,11,486,11],[487,11,490,11],[491,11,494,11],[495,11,498,11],[455,11,458,11],[459,11,462,11],[463,11,466,11],[467,11,470,11],[471,11,473,11],[474,11,476,11],[429,11,432,11],[433,11,436,11],[437,11,440,11],[441,11,444,11],[447,11,450,11],[451,11,454,11],[405,11,408,11],[409,11,412,11],[413,11,416,11],[417,11,420,11],[421,11,424,11],[425,11,428,11],[383,11,385,11],[386,11,388,11],[390,11,391,11],[393,11,396,11],[397,11,400,11],[401,11,404,11],[368,11,369,11],[370,11,371,11],[372,11,374,11],[375,11,376,11],[377,11,379,11],[380,11,382,11],[348,11,353,11],[354,11,359,11],[360,11,361,11],[362,11,363,11],[364,11,365,11],[366,11,367,11],[336,11,337,11],[338,11,339,11],[340,11,341,11],[342,11,343,11],[344,11,345,11],[346,11,347,11],[268,11,269,11],[270,11,273,11],[274,11,276,11],[290,11,291,11],[292,11,293,11],[294,11,296,11],[250,11,251,11],[252,11,253,11],[254,11,255,11],[256,11,259,11],[260,11,261,11],[262,11,267,11],[208,11,214,11],[224,11,225,11],[226,11,231,11],[232,11,239,11],[240,11,247,11],[248,11,249,11],[175,11,178,11],[181,11,185,11],[186,11,191,11],[192,11,193,11],[203,11,204,11],[206,11,207,11],[144,11,146,11],[150,11,155,11],[156,11,158,11],[159,11,161,11],[163,11,170,11],[171,11,174,11],[115,11,116,11],[119,11,123,11],[124,11,126,11],[127,11,129,11],[135,11,140,11],[141,11,143,11],[68,11,69,11],[71,11,73,11],[75,11,80,11],[106,11,108,11],[109,11,111,11],[112,11,114,11],[23,11,24,11],[26,11,27,11],[32,11,34,11],[0,7,2,7],[0,8,2,8],[0,9,2,9],[0,10,2,10],[0,11,2,11],[11,11,12,11],[0,1,2,1],[0,2,2,2],[0,3,2,3],[0,4,2,4],[0,5,2,5],[0,6,2,6],[13,11,18,11],[19,11,20,11],[21,11,22,11]]}
[null,"代號\n111(上)","用途","規調表\n仕樣代碼","品 名","110(下)規格.仕樣","單位","111(上)牌價","110(下)牌價","牌價差異","牌價差異比率","備                              註"]
[]
[]
[]
[null,"3C9200","P",288,"客貨用(PF梯) W≦1/4荷重","單次載貨重≦1/4荷重","台",8900,8500,{"$f":"H5-I5","v":400},{"$f":"IF(I5>0,(H5-I5)/I5,-(H5-I5)/I5)","v":4.7058823529411764E-2},"1.僅FLOOR強度結構配合.\n2.不含SILL&地板材質變更."]
[{"$nulls":4},"-",null,null,0]
[null,"3F3000","F",3,"單次載貨重 (W≦1/2荷重)","F-1000~2000kg","台",7400,7200,{"$f":"H7-I7","v":200},{"$f":"IF(I7>0,(H7-I7)/I7,-(H7-I7)/I7)","v":2.7777777777777776E-2}]
[null,"3F3200","F",3,"單次載貨重 (W＞1/2荷重)","F-1000kg","台",9700,9400,{"$f":"H8-I8","v":300},{"$f":"IF(I8>0,(H8-I8)/I8,-(H8-I8)/I8)","v":3.1914893617021274E-2}]
[null,"3F3300","F",3,"單次載貨重 (W＞1/2荷重)","F-1500kg","台",14200,13800,{"$f":"H9-I9","v":400},{"$f":"IF(I9>0,(H9-I9)/I9,-(H9-I9)/I9)","v":2.8985507246376812E-2}]
[null,"3F3400","F",3,"單次載貨重 (W＞1/2荷重)","F-2000kg","台",27800,27100,{"$f":"H10-I10","v":700},{"$f":"IF(I10>0,(H10-I10)/I10,-(H10-I10)/I10)","v":2.5830258302583026E-2}]
[]
[null,"7C7700","P",4255,"≧24L 加計(台)(任何速度)","採60C鐵芯CABLE","台",53700,53200,{"$f":"H12-I12","v":500},{"$f":"IF(I12>0,(H12-I12)/I12,-(H12-I12)/I12)","v":9.3984962406015032E-3},"1.鐵芯CABLE:採60C鐵芯CABLE"]
[null,"7C7800","P",4255,"≧24L 加計(樓)(任何速度)","採60C鐵芯CABLE","樓",2900,2700,200,7.407407407407407E-2]
[null,"3C7600","P",4255,"COMP CHAIN (台)","P8~P11人 (60m 10停) ","台",13700,13500,200,1.4814814814814815E-2,"1.適用:行程≧30m以上加計\n2.60m≧10停以上加計(90.105m MI已內含)\n3.(例) P15*12-CO60\n         ⊕17,800/台+ 1,400/停*2停=⊕20,600/台"]
[null,"3C7700","P",4255,"COMP CHAIN (樓)","± 1停 (P8~P11 60m) ","樓",900,900,0,0]
[null,"3C7800","P",4255,"COMP CHAIN (台)","P12~P17人 (60m 10停) ","台",17800,17600,200,1.1363636363636364E-2]
[null,"3C7900","P",4255,"COMP CHAIN (樓)","± 1停 (P12~P17 60m) ","樓",1400,1400,0,0]
[null,"3C8000","P",4255,"COMP CHAIN (台)","P20~P24人 (60m 10停) ","台",23600,23300,300,1.2875536480686695E-2]
[null,"3C8100","P",4255,"COMP CHAIN (樓)","± 1停 (P20~P24 60m) ","樓",2200,2200,0,0]
[null,"3B0700","B",4255,"COMP CHAIN (台)","B-750~1000kg(45~60m 10停) ","台",17700,17500,200,1.1428571428571429E-2,"1.適用:行程≧30m以上加計\n2.≧10停以上加計"]
[null,"3B0750","B",4255,"COMP CHAIN (樓)","B-750~1000kg +1停","樓",1400,1400,0,0]
[null,"3F2000","F",4255,"COMP CHAIN (台)","F-1000~2000kg(45~60m 10停) ","台",17800,17600,200,1.1363636363636364E-2,"1.適用:行程≧30m以上加計\n2.≧10停以上加計"]
[null,"3F2100","F",4255,"COMP CHAIN (樓)","F-1000~2000kg +1停","樓",2100,2100,0,0]
[null,"3F2200","F",4255,"COMP CHAIN (台)","F-2500~3000kg(45~60m 10停) ","台",23500,23300,200,8.5836909871244635E-3,"1.適用:行程≧30m以上加計\n2.≧10停以上加計"]
[null,"3F2300","F",4255,"COMP CHAIN (樓)","F-2500~3000kg +1停","樓",2100,2100,0,0]
[]
[null,"4C3000","P",6,"2P-CO→2S-2P(台)","P6~24人(OP≦1100)","台",10400,7200,{"$f":"H27-I27","v":3200},{"$f":"IF(I27>0,(H27-I27)/I27,-(H27-I27)/I27)","v":0.44444444444444442},"標準仕樣: 標準OP*EH-2100\n                 門框AS-1X(SH),出入口門(IP)"]
[null,"4C3100","P",6,"2P-CO→2S-2P(停)","P6~24人(OP≦1100)","停",5400,7800,-2400,-0.30769230769230771]
[null,"3C5000","P",282,"千鳥型(EAS人乘需另加計CWT側落)","P9人","台",128900,120600,8300,6.8822553897180769E-2,"不含RAIL跳級,含帶鎖門刀追加"]
[null,"3C5100","P",282,"千鳥型(EAS人乘需另加計CWT側落)","P10~P11人","台",157500,151500,6000,3.9603960396039604E-2,"含CAGE RAIL:T-8K→T-13K,含帶鎖門刀追加"]
[null,"3C5200","P",282,"千鳥型(EAS人乘需另加計CWT側落)","P12~P15人","台",139200,131400,7800,5.9360730593607303E-2,"含CWT RAIL:T-5K→T-8K,,含帶鎖門刀追加"]
[null,"3C5300","P",282,"千鳥型(EAS人乘需另加計CWT側落)","P17~P24人","台",128900,120600,8300,6.8822553897180769E-2,"不含RAIL跳級,含帶鎖門刀追加"]
[null,"3C5050","P",282,"L型千鳥(其他相關需另計)","P9人","台",282700,268500,{"$f":"H33-I33","v":14200},5.2886405959031657E-2,"報價不含2S-2P,CWT側落式,需以OPTION另計\n報價含帶鎖門刀追加\nP9人:含RAIL 8K*5K→8K*8K(10停)\nP10~P11人:含RAIL 8K*5K→13K*8K(10停)\nP12~P15人:含RAIL 13K*5K→13K*8K(10停)"]
[null,"3C5150","P",282,"L型千鳥(其他相關需另計)","P10~P11人","台",314900,302000,{"$f":"H34-I34","v":12900},4.2715231788079469E-2]
[null,"3C5250","P",282,"L型千鳥(其他相關需另計)","P12~P15人","台",297400,283300,{"$f":"H35-I35","v":14100},4.9770561242499116E-2]
[null,"3B0800","B",282,"千鳥型&THROUGH","B-750~1000kg ","台",157900,148300,9600,6.4733648010788944E-2,"1.含車廂出入口配合&立組工時追加\n2.含SUB OPB等電氣品追加 (RAIL不跳級計)"]
[null,"4F3000","F",282,"千鳥型","F-1000kg~2000kg ","台",135400,129100,6300,4.8799380325329204E-2]
[null,"4F3100","F",282,"千鳥型","F-2500kg~3000kg","台",179400,170800,{"$f":"H38-I38","v":8600},5.0351288056206089E-2]
[null,"B00100","P.B",282,"出入口防落網(UAS1-06千鳥選用)","2*樓數-停數","停",5400,5400,0,0,"UAS1-06千鳥無法規劃帶鎖門刀"]
[null,"Y24700","F",282,"出入口防落板(F梯千鳥選用)\n(以施作面積M²計算加價)","{(行程*2)-[(停數-1)*\n(EH+0.4)]}*(OP+0.1)\n*1000元/M²","M²",1000,1000,{"$f":"H40-I40","v":0},0,"1.{(行程*2)- [(停數-1)*(EH+0.4)]}*(OP+0.1)*1000元/M²\n2.加價1000元為防落板面積每平方公尺施作費用"]
[]
["新增","3C9450","P",280,"GUIDE SHOE→GUIDE ROLLER","EAS-P8~24人","台",57200,null,{"$f":"H42-I42","v":57200},{"$f":"IF(I42>0,(H42-I42)/I42,-(H42-I42)/I42)","v":{"$error":"#DIV/0!"}}]
[]
[null,"7C0100","P.B.F",8,"DUP (2台聯動)",null,"群",6800,6800,{"$f":"H44-I44","v":0},{"$f":"IF(I44>0,(H44-I44)/I44,-(H44-I44)/I44)","v":0},"配賦予聯動第1台,而聯動第2台不配賦."]
[null,"7C0200","P.B",8,"FT-2 群管理 (3~8台/群)","3~8台群管理(無群管理盤)","群",53400,51400,{"$f":"H45-I45","v":2000},{"$f":"IF(I45>0,(H45-I45)/I45,-(H45-I45)/I45)","v":3.8910505836575876E-2},"配賦於NO.1號機,另IND應採HALL-LANT,費用另計\n2.IND應採HALL-LANT,費用另計"]
[null,"7C0400","P",8,"群管理切離1台單獨運轉",null,"台",8900,8800,{"$f":"H46-I46","v":100},{"$f":"IF(I46>0,(H46-I46)/I46,-(H46-I46)/I46)","v":1.1363636363636364E-2},"僅配賦予切離號機."]
[]
[null,"7C6900","P",9,"EAS電源電壓380V(控盤對應)","EAS-P6~P11人(60m)","台",5300,4600,{"$f":"H48-I48","v":700},{"$f":"IF(I48>0,(H48-I48)/I48,-(H48-I48)/I48)","v":0.15217391304347827}]
[null,"7C6950","P",9,"EAS電源電壓220V(主機,控盤對應)","EAS-P8~P11人(90m)","台",23900,18400,5500,{"$f":"IF(I49>0,(H49-I49)/I49,-(H49-I49)/I49)","v":0.29891304347826086},"主機以大(GSD-MM)代小(GSD-MM1)"]
[null,"7C7300","P",9,"電源電壓380V(扣除TRANS 7KVA)","VAG-P6~15人(60m)","台",-21600,-21000,-600,{"$f":"IF(I50>0,(H50-I50)/I50,-(H50-I50)/I50)","v":-2.8571428571428571E-2},"扣除降壓TRANS.(MI已內附加計7KVA TRANS)"]
[null,"7C7350","P",9,"電源電壓220V(追加TRANS 12KVA)","VAG-P8~P15人(90,105m)","台",37200,33300,3900,0.11711711711711711,"追加昇壓TRANS:容量12KVA"]
[null,"7C7400","P.B.F",203,"追加能源回饋裝置 (Regen 11KW)","EAS-P12~P24人(60m)","台",43700,37900,5800,0.15303430079155672]
[null,"7C7410","P.B.F",203,"追加能源回饋裝置 (Regen 11KW)","EAS-P8~P15人(90,105m)","台",43700,37900,5800,0.15303430079155672]
[null,"7C7420","P.B.F",203,"追加能源回饋裝置 (Regen 22KW)","EAS-P17~P20人(90,105m)","台",55900,48500,7400,0.15257731958762888]
[null,"7C7430","P.B.F",203,"追加能源回饋裝置 (Regen 22KW)","EAS-P13~P17人(120m)","台",55900,48500,7400,0.15257731958762888]
[null,"7C7440","P.B.F",203,"追加能源回饋裝置 (Regen 22KW)","EAS-P13~P17人(150m)","台",55900,48500,7400,0.15257731958762888]
[null,"G02300","P.B.F",334,"變相器借用費用(含運費)",null,"台",7700,7700,0,0]
[null,"F03800","P.B.F",333,"變壓器借用費用(含運費)",null,"台",7700,7700,0,0]
[null,"7F1100","F",9,"電源電壓220V(追加TRANS 20KVA)","F-1500kg~2000kg","台",36500,33100,3400,0.1027190332326284]
[null,"7F1200","F",9,"電源電壓220V(追加TRANS 25KVA)","F-2500kg~3000kg","台",52200,51300,900,1.7543859649122806E-2]
[]
[null,"4C8900","P","10.11.52","明鏡嵌入式(僅車廂後側)預留10mm","P6~P24人","台",8700,8000,{"$f":"H62-I62","v":700},8.7499999999999994E-2]
[null,"4C8950","P","10.11.52","明鏡嵌入式(車廂三側)預留10mm","P6~P24人","台",17300,16000,1300,8.1250000000000003E-2]
[null,"4C4100","P",10.11,"車廂內法特殊","P6~P24人","台",17000,15700,1300,8.2802547770700632E-2]
[null,"4B1500","B",10.11,"車廂內法特殊","B-750~1000kg ","台",28000,26000,2000,7.6923076923076927E-2]
[null,"4F5000","F",10.11,"車廂內法特殊","F-1000kg~2000kg","台",28200,26300,1900,7.2243346007604556E-2]
[null,"4F5100","F",10.11,"車廂內法特殊","F-2500kg~3000kg","台",36400,33800,2600,7.6923076923076927E-2]
[]
[null,"4C4000","P",157,"天井加高 ⊕200mm","側板(CE)選用","台",8700,8600,{"$f":"H69-I69","v":100},1.1627906976744186E-2,"1.車廂側板&廂門(CE),天井型式(標準)\n2.廂門高度:EH-2100"]
[null,"Y07800","P",157,"天井加高 ⊕400mm","側板(CE)選用","台",34400,34400,0,0]
[null,"Y08100","P",157,"天井加高 ⊕300mm","側板(CE)選用","台",28400,28400,0,{"$f":"IF(I71>0,(H71-I71)/I71,-(H71-I71)/I71)","v":0}]
[null,"4C4010","P",157,"天井加高 ⊕200mm","側板(SH or SM)選用","台",32300,26700,5600,0.20973782771535582,"1.車廂側板材質特殊,需OPTION另計\n2.廂門高度:EH-2100"]
[null,"4C4020","P",157,"天井加高 ⊕200mm","側板(SH.SM鍍鈦金)選用","台",32300,28200,4100,0.1453900709219858]
[null,"4C4030","P",157,"天井加高 ⊕200mm","側板(SH.SM鍍鈦遠東)選用","台",61000,55900,5100,9.1234347048300538E-2]
[]
[null,"4C3200","P","12,13","OP-800→OP-900 (台)","P6~12人(車廂標準式樣)","台",5200,5000,{"$f":"H76-I76","v":200},0.04,"車廂標準式樣: 車廂前側,兩後側&廂門(CE)\n乘場標準式樣: 小型門框 SH 1.2T NSSC180, H.DR(IP)\n1.僅乘場.車廂開門尺寸變更費用\n  (乘場門框型式,材質及車廂使用材質,需另議加計)\n2.天井淨高2300mm(標準)\n3.OPB型式: KF-D型式(SM)"]
[null,"4C3300","P","12,13","OP-800→OP-900 (停)","P6~12人(乘場標準式樣)","停",500,400,100,0.25]
[null,"4C3400","P","12,13","OP-900→OP-1000 (台)","P13~15人(車廂標準式樣)","台",4600,4500,100,2.2222222222222223E-2]
[null,"4C3500","P","12,13","OP-900→OP-1000 (停)","P13~15人(乘場標準式樣)","停",2400,6300,-3900,-0.61904761904761907]
[null,"4C3600","P","12,13","OP-1000→OP-1100 (台)","P17~20人(車廂標準式樣)","台",3400,4000,-600,-0.15]
[null,"4C3700","P","12,13","OP-1000→OP-1100 (停)","P17~20人(乘場標準式樣)","停",600,1000,-400,-0.4]
[null,"4C3800","P","12,13","EH-2100→EH-2300 (台)","側板(CE)選用","台",8100,10900,-2800,-0.25688073394495414,"含天井加高⊕200mm加計"]
[null,"4C3900","P","12,13","EH-2100→EH-2300 (停)","H.DR(IP)選用","停",1300,900,400,0.44444444444444442]
[null,"4C3910","P","12,13","EH-2100→EH-2300 (台)","側板(SH or SM)選用","台",31800,28600,3200,0.11188811188811189,"含天井加高⊕200mm加計,側板材質特殊,需OPTION另計"]
[null,"4C3920","P","12,13","EH-2100→EH-2300 (停)","H.DR(SH or SM)選用","停",4300,2600,1700,0.65384615384615385,"乘場部品材質特殊,需OPTION另計"]
[null,"4C3930","P","12,13","EH-2100→EH-2300 (台)","側板(SH.SM鍍鈦金)選用","台",34900,30400,4500,0.14802631578947367,"含天井加高⊕200mm加計,側板材質特殊,需OPTION另計"]
[null,"4C3940","P","12,13","EH-2100→EH-2300 (停)","H.DR(SH.SM鍍鈦金)選用","停",5500,3900,1600,0.41025641025641024,"乘場部品材質特殊,需OPTION另計"]
[null,"4C3950","P","12,13","EH-2100→EH-2300 (台)","側板(SH.SM鍍鈦遠東)選用","台",66100,60700,5400,8.8962108731466233E-2,"含天井加高⊕200mm加計,側板材質特殊,需OPTION另計"]
[null,"4C3960","P","12,13","EH-2100→EH-2300 (停)","H.DR(SH.SM鍍鈦遠東)選用","停",7000,6300,700,0.1111111111111111,"乘場部品材質特殊,需OPTION另計"]
[null,"4B1000","B","12,13,157","天井加高⊕200mm(EH-2300) (台)","側板(CE)選用","台",10300,10100,200,1.9801980198019802E-2]
[null,"4B1010","B","12,13,157","天井加高⊕200mm(EH-2300) (停)","H.DR(IP)選用","停",3600,2500,1100,0.44]
[null,"4B1100","B","12,13,157","天井加高⊕200mm(EH-2300) (台)","側板(SH or SM)選用","台",43500,36900,6600,0.17886178861788618,"側板材質特殊,需OPTION另計"]
[null,"4B1110","B","12,13,157","天井加高⊕200mm(EH-2300) (停)","H.DR(SH or SM)選用","停",7200,5100,2100,0.41176470588235292,"乘場部品材質特殊,需OPTION另計"]
[null,"4B1200","B","12,13,157","天井加高⊕200mm(EH-2300) (台)","側板(SH.SM鍍鈦金)選用","台",71300,63100,8200,0.12995245641838352,"側板材質特殊,需OPTION另計"]
[null,"4B1210","B","12,13,157","天井加高⊕200mm(EH-2300) (停)","H.DR(SH.SM鍍鈦金)選用","停",6200,5200,1000,0.19230769230769232,"乘場部品材質特殊,需OPTION另計"]
[null,"4B1300","B","12,13,157","天井加高⊕200mm(EH-2300) (台)","側板(SH.SM鍍鈦遠東)選用","台",90900,83000,7900,9.5180722891566261E-2,"側板材質特殊,需OPTION另計"]
[null,"4B1310","B","12,13,157","天井加高⊕200mm(EH-2300) (停)","H.DR(SH.SM鍍鈦遠東)選用","停",8900,7900,1000,0.12658227848101267,"乘場部品材質特殊,需OPTION另計"]
[null,"4F1000","F","12,13,157","天井加高⊕200mm(EH-2300) (台)","F-1000~2000kg","台",31200,30300,{"$f":"H98-I98","v":900},2.9702970297029702E-2]
[null,"4F1100","F","12,13,157","天井加高⊕200mm(EH-2300) (停)","F-1000~2000kg","停",11600,6800,{"$f":"H99-I99","v":4800},0.70588235294117652]
[null,"4F1200","F","12,13,157","天井加高⊕200mm(EH-2500) (台)","F-2500kg~3000kg","台",82500,66500,{"$f":"H100-I100","v":16000},0.24060150375939848]
[null,"4F1300","F","12,13,157","天井加高⊕200mm(EH-2500) (停)","F-2500kg~3000kg","停",23900,15500,{"$f":"H101-I101","v":8400},0.54193548387096779]
[]
[null,"Y01100","P.B.F",298,"鋼骨結構配合費用(P-12~24人)","P12~P24人 (60m~105m 10停)","台",20200,20200,{"$f":"H103-I103","v":0},{"$f":"IF(I103>0,(H103-I103)/I103,-(H103-I103)/I103)","v":0},"工程定芯(台),防火披覆清潔(10停),\n配合IND固定(10停) "]
[null,"Y01200","P.B.F",298,"鋼骨結構配合費用(P-12~24人)","±1停","樓",1000,1000,{"$f":"H104-I104","v":0},0]
[null,"Y02200","P",298,"鋼骨結構(停)(UAS1-06)",null,"樓",1000,1000,{"$f":"H105-I105","v":0},0]
[]
[null,"3C4000","P",155,"CWT附WEDGE(台)","P6~P15人 (60m 6停)","台",42900,42100,{"$f":"H107-I107","v":800},1.9002375296912115E-2,"1.CWT FRAME變更及追加GOV&ROPE等\n2.含CWT RAIL: T-5K → T-8K"]
[null,"3C4100","P",155,"CWT附WEDGE(台)","P8~P15人 (90,105m 10停)","台",47600,46800,800,1.7094017094017096E-2]
[null,"3C4200","P",155,"CWT附WEDGE(樓)"," ± 1停  (60m,90,105m)","樓",1700,1300,400,0.30769230769230771]
[null,"3C4300","P",155,"CWT附WEDGE(台)","P17人 (60m 6停)","台",58100,57800,300,5.1903114186851208E-3,"1.CWT FRAME變更及追加GOV&ROPE等\n2.含CWT RAIL:T-8K → T-13K"]
[null,"3C4400","P",155,"CWT附WEDGE(台)","P17人 (90,105m 10停)","台",72700,72400,300,4.1436464088397788E-3]
[null,"3C4500","P",155,"CWT附WEDGE(樓)"," ± 1停  (60m,90,105m)","樓",3700,3300,400,0.12121212121212122]
[null,"3C4600","P",155,"CWT附WEDGE(台)","P20~P24人 (60m 6停)","台",65400,64900,500,7.7041602465331279E-3,"1.CWT FRAME變更及追加GOV&ROPE等\n2.含CWT RAIL:T-13K → T-18K(賽維拉BE)"]
[null,"3C4700","P",155,"CWT附WEDGE(台)","P20~P24人 (90,105m 10停)","台",88000,87000,1000,1.1494252873563218E-2]
[null,"3C4800","P",155,"CWT附WEDGE(樓)"," ± 1停  (60m,90,105m)","樓",4500,4300,200,4.6511627906976744E-2]
[null,"3S6000","P",155,"CWT附WEDGE(台)","UAS-P8人 (60m 6停)","台",78800,79800,-1000,-1.2531328320802004E-2,"1.CWT FRAME變更及追加GOV&ROPE等\n2.含CWT RAIL: T-5K → T-8K & SUB WT改鑄鐵式\n"]
[null,"3S6100","P",155,"CWT附WEDGE(樓)","UAS-P8人 ± 1停","樓",1100,1200,-100,-8.3333333333333329E-2]
[null,"3C3200","P",155,"CWT附WEDGE(台)","P6~P15人(無機房用)","台",86800,65800,{"$f":"H118-I118","v":21000},{"$f":"IF(I118>0,(H118-I118)/I118,-(H118-I118)/I118)","v":0.31914893617021278},"含混用式SUB WT→全部改鑄鐵式"]
[]
[null,"1C0100","P",16.170000000000002,"小型門框 SH鍍鈦(金色)","2P-CO ≦OP-800~1100","停",3100,2100,{"$f":"H120-I120","v":1000},0.47619047619047616,"標準小型門框SH素材:為(NSSC180)1.2T板材\n1.小型門框SM素材:為(日新)板材\n2.小型門框SH鍍鈦素材:(唐榮)板於國內加工鍍鈦\n3.小型門框SM鍍鈦素材:(日新)板於國內加工鍍鈦\n4.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"1C0150","P",16.170000000000002,"小型門框 SH鍍鈦(遠東特殊色)","2P-CO ≦OP-800~1100","停",4900,3900,1000,0.25641025641025639]
[null,"1C0200","P",16.170000000000002,"小型門框 SM","2P-CO ≦OP-800~1100","停",2600,1700,900,0.52941176470588236]
[null,"1C0300","P",16.170000000000002,"小型門框 SM鍍鈦(金色)","2P-CO ≦OP-800~1100","停",3700,2800,900,0.32142857142857145]
[null,"1C0350","P",16.170000000000002,"小型門框 SM鍍鈦(遠東特殊色)","2P-CO ≦OP-800~1100","停",5400,4400,1000,0.22727272727272727]
[null,"1C4000","P",16.170000000000002,"小型門框  亂紋板","2P-CO ≦OP-800~1100","停",4400,3500,900,0.25714285714285712,"1.(遠東)亂紋板: V-00\n2.(遠東)亂紋鍍鈦(金色): V-01 \n3.(遠東)亂紋鍍鈦(特殊色): V-02~V-05"]
[null,"1C4020","P",16.170000000000002,"小型門框  亂紋鍍鈦(金色)","2P-CO ≦OP-800~1100","停",5900,5000,900,0.18]
[null,"1C4040","P",16.170000000000002,"小型門框  亂紋鍍鈦(遠東特殊色)","2P-CO ≦OP-800~1100","停",8900,8000,900,0.1125]
[null,"1C4100","P",16.170000000000002,"小型門框  霧珠板","2P-CO ≦OP-800~1100","停",4600,3700,900,0.24324324324324326,"1.(遠東)霧珠板: B-00\n2.(遠東)霧珠鍍鈦(金色): B-01 \n3.(遠東)霧珠鍍鈦(特殊色): B-02~B-05"]
[null,"1C4120","P",16.170000000000002,"小型門框  霧珠鍍鈦(金色)","2P-CO ≦OP-800~1100","停",6100,5200,900,0.17307692307692307]
[null,"1C4140","P",16.170000000000002,"小型門框  霧珠鍍鈦(遠東特殊色)","2P-CO ≦OP-800~1100","停",9100,8200,900,0.10975609756097561]
[null,"1C2100","P","16.17.314","小型門框(SH)指定SUS#304","2P-CO≦OP-800~1100*2300H","停",600,500,100,0.2,"小型門框指定SUS#304: 為國內(唐榮)1.5T板材"]
[null,"1C0360","P",16.170000000000002,"小型門框 IP(仿鍍鈦烤漆)","2P-CO ≦OP-800~1100","停",1700,1100,{"$f":"H132-I132","v":600},0.54545454545454541,"仿古咖色, 仿黑色, 仿古銅色, 仿金色."]
[null,"1C0370","P",16.170000000000002,"小型門框 SH(壓克力烤漆)","2P-CO ≦OP-800~1100","停",3400,3300,{"$f":"H133-I133","v":100},{"$f":"IF(I133>0,(H133-I133)/I133,-(H133-I133)/I133)","v":3.0303030303030304E-2}]
[null,"1C0380","P",16.170000000000002,"小型門框 SH(仿鍍鈦烤漆)","2P-CO ≦OP-800~1100","停",3800,3700,{"$f":"H134-I134","v":100},{"$f":"IF(I134>0,(H134-I134)/I134,-(H134-I134)/I134)","v":2.7027027027027029E-2}]
[null,"Y03900","P",16.170000000000002,"隱藏式門框(無門框)","門框前緣鎖附角鐵以遮縫隙","停",700,700,{"$f":"H135-I135","v":0},{"$f":"IF(I135>0,(H135-I135)/I135,-(H135-I135)/I135)","v":0},"隱藏式門框前緣鎖附角鐵,業主裝潢時再移除"]
[null,"1C0800","P",18.190000000000001,"大型門框 SH","OP-800~1100  A值≦380","停",13300,10200,3100,0.30392156862745096,"1.大型門框SH素材:為國內(唐榮)板材\n2.大型門框SM素材:為(日新)板材\n3.大型門框SH鍍鈦素材:(唐榮)板於國內加工鍍鈦\n4.大型門框SM鍍鈦素材:(日新)板於國內加工鍍鈦\n5.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"1C0900","P",18.190000000000001,"大型門框 SH鍍鈦(金色)","OP-800~1100  A值≦380","停",20400,17100,3300,0.19298245614035087]
[null,"1C0950","P",18.190000000000001,"大型門框 SH鍍鈦(遠東特殊色)","OP-800~1100  A值≦380","停",32300,29000,3300,0.11379310344827587]
[null,"1C1000","P",18.190000000000001,"大型門框 SM","OP-800~1100  A值≦380","停",17500,14200,3300,0.23239436619718309]
[null,"1C1100","P",18.190000000000001,"大型門框 SM鍍鈦(金色)","OP-800~1100  A值≦380","停",24400,21400,3000,0.14018691588785046]
[null,"1C1150","P",18.190000000000001,"大型門框 SM鍍鈦(遠東特殊色)","OP-800~1100  A值≦380","停",36300,33300,3000,9.0090090090090086E-2]
[null,"1C4400","P",18.190000000000001,"大型門框  亂紋板","OP-800~1100  A值≦380","停",20700,17700,3000,0.16949152542372881,"1.(遠東)亂紋板: V-00\n2.(遠東)亂紋鍍鈦(金色): V-01 \n3.(遠東)亂紋鍍鈦(特殊色): V-02~V-05"]
[null,"1C4420","P",18.190000000000001,"大型門框  亂紋鍍鈦(金色)","OP-800~1100  A值≦380","停",27300,24300,3000,0.12345679012345678]
[null,"1C4440","P",18.190000000000001,"大型門框  亂紋鍍鈦(遠東特殊色)","OP-800~1100  A值≦380","停",39100,36100,3000,8.3102493074792241E-2]
[null,"1C4500","P",18.190000000000001,"大型門框  霧珠板","OP-800~1100  A值≦380","停",21400,18400,3000,0.16304347826086957,"1.(遠東)霧珠板: B-00\n2.(遠東)霧珠鍍鈦(金色): B-01 \n3.(遠東)霧珠鍍鈦(特殊色): B-02~B-05"]
[null,"1C4520","P",18.190000000000001,"大型門框  霧珠鍍鈦(金色)","OP-800~1100  A值≦380","停",27700,24700,3000,0.1214574898785425]
[null,"1C4540","P",18.190000000000001,"大型門框  霧珠鍍鈦(遠東特殊色)","OP-800~1100  A值≦380","停",39500,36500,3000,8.2191780821917804E-2]
[null,"1C1160","P",18.190000000000001,"大型門框 IP(仿鍍鈦烤漆)","OP-800~1100  A值≦380","停",9100,8700,{"$f":"H148-I148","v":400},{"$f":"IF(I148>0,(H148-I148)/I148,-(H148-I148)/I148)","v":4.5977011494252873E-2},"仿古咖色, 仿黑色, 仿古銅色, 仿金色."]
[null,"1C2200","P",18.190000000000001,"(CO)配合防火門,大框包覆小框加工費","2P-CO:工廠已組立好","停",2900,2700,{"$f":"H149-I149","v":200},{"$f":"IF(I149>0,(H149-I149)/I149,-(H149-I149)/I149)","v":7.407407407407407E-2},"防火門及大型門框加價需以OPTION另計"]
[null,"Y23900","P.B",18.190000000000001,"(2S)配合防火門,大框包覆小框加工費","2S-2P:工廠未組立","停",10900,10700,200,1.8691588785046728E-2,"防火門及大型門框加價需以OPTION另計"]
[null,"1C0400","P",335.33600000000001,"小型門框附幕板 SH","OP-800~1100 全高≦3000","停",14200,13300,900,6.7669172932330823E-2,"小型門框附幕板: 含HF-LM3顯示器\n1.小型門框附幕板SH素材:為國內(唐榮)板材\n2.小型門框附幕板SM素材:為(日新)板材\n3.小框附幕板SH鍍鈦素材:(唐榮)板於國內加工鍍鈦\n4.小框附幕板SM鍍鈦素材:(日新)板於國內加工鍍鈦\n5.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"1C0500","P",335.33600000000001,"小型門框附幕板 SH鍍鈦(金色)","OP-800~1100 全高≦3000","停",21300,19200,2100,0.109375]
[null,"1C0550","P",335.33600000000001,"小框附幕板 SH鍍鈦(遠東特殊色)","OP-800~1100 全高≦3000","停",29900,27300,2600,9.5238095238095233E-2]
[null,"1C0600","P",335.33600000000001,"小型門框附幕板 SM","OP-800~1100 全高≦3000","停",16000,14900,1100,7.3825503355704702E-2]
[null,"1C0700","P",335.33600000000001,"小型門框附幕板 SM鍍鈦(金色)","OP-800~1100 全高≦3000","停",23700,21400,2300,0.10747663551401869]
[null,"1C0750","P",335.33600000000001,"小框附幕板 SM鍍鈦(遠東特殊色)","OP-800~1100 全高≦3000","停",31800,29700,2100,7.0707070707070704E-2]
[null,"1C4200","P",335.33600000000001,"小型門框附幕板  亂紋板","OP-800~1100 全高≦3000","停",20900,18800,2100,0.11170212765957446,"1.(遠東)亂紋板: V-00\n2.(遠東)亂紋鍍鈦(金色): V-01 \n3.(遠東)亂紋鍍鈦(特殊色): V-02~V-05"]
[null,"1C4220","P",335.33600000000001,"小型門框附幕板  亂紋鍍鈦(金色)","OP-800~1100 全高≦3000","停",25800,23500,2300,9.7872340425531917E-2]
[null,"1C4240","P",335.33600000000001,"小框附幕板  亂紋鍍鈦(遠東特殊色)","OP-800~1100 全高≦3000","停",33800,31600,2200,6.9620253164556958E-2]
[null,"1C4300","P",335.33600000000001,"小型門框附幕板  霧珠板","OP-800~1100 全高≦3000","停",21200,19000,2200,0.11578947368421053,"1.(遠東)霧珠板: B-00\n2.(遠東)霧珠鍍鈦(金色): B-01 \n3.(遠東)霧珠鍍鈦(特殊色): B-02~B-05"]
[null,"1C4320","P",335.33600000000001,"小型門框附幕板  霧珠鍍鈦(金色)","OP-800~1100 全高≦3000","停",25900,23700,2200,9.2827004219409287E-2]
[null,"1C4340","P",335.33600000000001,"小框附幕板  霧珠鍍鈦(遠東特殊色)","OP-800~1100 全高≦3000","停",34200,31800,2400,7.5471698113207544E-2]
[null,"1C0760","P",335.33600000000001,"小框附幕板  IP(仿鍍鈦烤漆)","OP-800~1100 全高≦3000","停",14300,13400,{"$f":"H163-I163","v":900},{"$f":"IF(I163>0,(H163-I163)/I163,-(H163-I163)/I163)","v":6.7164179104477612E-2},"仿古咖色, 仿黑色, 仿古銅色, 仿金色."]
[null,"1C1200","P",21.23,"大型門框附幕板 SH","OP-800~1100 全高≦3000","停",27800,23400,4400,0.18803418803418803,"大型門框附幕板: 含HF-LM3顯示器\n1.大型門框附幕板SH素材:為國內(唐榮)板材\n2.大型門框附幕板SM素材:為(日新)板材\n3.大框附幕板SH鍍鈦素材:(唐榮)板於國內加工鍍鈦\n4.大框附幕板SM鍍鈦素材:(日新)板於國內加工鍍鈦\n5.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"1C1300","P",21.23,"大型門框附幕板 SH鍍鈦(金色)","OP-800~1100 全高≦3000","停",37000,32100,4900,0.15264797507788161]
[null,"1C1350","P",21.23,"大框附幕板 SH鍍鈦(遠東特殊色)","OP-800~900 全高≦3000","停",53700,48900,4800,9.815950920245399E-2]
[null,"1C1400","P",21.23,"大型門框附幕板 SM","OP-800~1100 全高≦3000","停",32600,28000,4600,0.16428571428571428]
[null,"1C1500","P",21.23,"大型門框附幕板 SM鍍鈦(金色)","OP-800~1100 全高≦3000","停",41800,36800,5000,0.1358695652173913]
[null,"1C1550","P",21.23,"大框附幕板 SM鍍鈦(遠東特殊色)","OP-800~900 全高≦3000","停",58600,53500,5100,9.5327102803738323E-2]
[null,"1C1750","P",21.23,"大框附幕板 SH鍍鈦(遠東特殊色)","OP-1000~1100全高≦3000","停",58400,53500,4900,{"$f":"IF(I170>0,(H170-I170)/I170,-(H170-I170)/I170)","v":9.1588785046728974E-2}]
[null,"1C1950","P",21.23,"大框附幕板 SM鍍鈦(遠東特殊色)","OP-1000~1100全高≦3000","停",63800,58000,5800,0.1]
[null,"1C4600","P",21.23,"大型門框附幕板  亂紋板","OP-800~1100  A值≦380","停",36800,32100,4700,0.14641744548286603,"1.(遠東)亂紋板: V-00\n2.(遠東)亂紋鍍鈦(金色): V-01 \n3.(遠東)亂紋鍍鈦(特殊色): V-02~V-05\n4.[遠東]特殊色: 計有咖啡. 黑色. 古銅. 古咖"]
[null,"1C4620","P",21.23,"大型門框附幕板  亂紋鍍鈦(金色)","OP-800~1100  A值≦380","停",45500,40800,4700,0.11519607843137254]
[null,"1C4640","P",21.23,"大框附幕板  亂紋鍍鈦(遠東特殊色)","OP-800~900  A值≦380","停",62300,57600,4700,8.1597222222222224E-2]
[null,"1C4660","P",21.23,"大框附幕板  亂紋鍍鈦(遠東特殊色)","OP-1000~1100  A值≦380","停",67900,62700,5200,8.2934609250398722E-2]
[null,"1C4700","P",21.23,"大型門框附幕板  霧珠板","OP-800~1100  A值≦380","停",37200,32700,4500,0.13761467889908258,"1.(遠東)霧珠板: B-00\n2.(遠東)霧珠鍍鈦(金色): B-01 \n3.(遠東)霧珠鍍鈦(特殊色): B-02~B-05\n4.[遠東]特殊色: 計有咖啡. 黑色. 古銅. 古咖"]
[null,"1C4720","P",21.23,"大型門框附幕板  霧珠鍍鈦(金色)","OP-800~1100  A值≦380","停",46000,41300,4700,0.11380145278450363]
[null,"1C4740","P",21.23,"大框附幕板  霧珠鍍鈦(遠東特殊色)","OP-800~900  A值≦380","停",62700,58000,4700,8.1034482758620685E-2]
[null,"1C4760","P",21.23,"大框附幕板  霧珠鍍鈦(遠東特殊色)","OP-1000~1100  A值≦380","停",68400,63200,5200,8.2278481012658222E-2]
[null,"1C1960","P",21.23,"大框附幕板  IP(仿鍍鈦烤漆)","OP-800~1100  A值≦380","停",21300,21000,{"$f":"H180-I180","v":300},{"$f":"IF(I180>0,(H180-I180)/I180,-(H180-I180)/I180)","v":1.4285714285714285E-2},"仿古咖色, 仿黑色, 仿古銅色, 仿金色."]
[null,"1C2000","P","21.23.335.336","面一式門框","OP-800~1100全高≦3000","停",5400,5400,0,0,"要先加計大(小)框附幕板的底價"]
[null,"1B0100","B",16.170000000000002,"小型門框 SH鍍鈦(金色)","2S-2P  OP-1100~1200W","停",4700,3900,800,0.20512820512820512,"小型門框SH素材:為國內(唐榮)板材\n1.小型門框SM素材:為(日新)板材\n2.小型門框SH鍍鈦素材:(唐榮)板於國內加工鍍鈦\n3.小型門框SM鍍鈦素材:(日新)板於國內加工鍍鈦\n4.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"1B0110","B",16.170000000000002,"小型門框 SH鍍鈦(遠東特殊色)","2S-2P  OP-1100~1200W","停",9100,8300,800,9.6385542168674704E-2]
[null,"1B0200","B",16.170000000000002,"小型門框 SM","2S-2P  OP-1100~1200W","停",3800,2900,{"$f":"H184-I184","v":900},0.31034482758620691]
[null,"1B0210","B",16.170000000000002,"小型門框 SM鍍鈦(金色)","2S-2P  OP-1100~1200W","停",5900,5000,{"$f":"H185-I185","v":900},0.18]
[null,"1B0220","B",16.170000000000002,"小型門框 SM鍍鈦(遠東特殊色)","2S-2P  OP-1100~1200W","停",10300,9400,{"$f":"H186-I186","v":900},9.5744680851063829E-2]
[null,"1B0300","B",18.190000000000001,"大型門框 SH","2S-1100.1200  A值≦380","停",15100,11300,3800,0.33628318584070799,"大型門框SH素材:為國內(唐榮)板材\n1.大型門框SM素材:為(日新)板材\n2.大型門框SH鍍鈦素材:(唐榮)板於國內加工鍍鈦\n3.大型門框SM鍍鈦素材:(日新)板於國內加工鍍鈦\n4.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"1B0310","B",18.190000000000001,"大型門框 SH鍍鈦(金色)","2S-1100.1200  A值≦380","停",23700,19700,4000,0.20304568527918782]
[null,"1B0320","B",18.190000000000001,"大型門框 SH鍍鈦(遠東特殊色)","2S-1100.1200  A值≦380","停",37100,33000,4100,0.12424242424242424]
[null,"1B0400","B",18.190000000000001,"大型門框 SM","2S-1100.1200  A值≦380","停",21000,16700,{"$f":"H190-I190","v":4300},0.25748502994011974]
[null,"1B0410","B",18.190000000000001,"大型門框 SM鍍鈦(金色)","2S-1100.1200  A值≦380","停",27200,22900,{"$f":"H191-I191","v":4300},0.18777292576419213]
[null,"1B0420","B",18.190000000000001,"大型門框 SM鍍鈦(遠東特殊色)","2S-1100.1200  A值≦380","停",40500,36200,{"$f":"H192-I192","v":4300},0.11878453038674033]
[null,"1F0300","F",18.190000000000001,"大型門框 SH","2S-1400~1700W  A值≦380","停",15800,13200,{"$f":"H193-I193","v":2600},0.19696969696969696]
[null,"1F0400","F",18.190000000000001,"大型門框 SH","4C-1700~2300W  A值≦380","停",24500,20400,{"$f":"H194-I194","v":4100},0.20098039215686275]
[]
[null,"2C3000","P",316,"防火門(台)(2P-CO)(含FMS拉線測試)",null,"台",12400,12200,{"$f":"H196-I196","v":200},1.6393442622950821E-2,"含火災管制追加.含火警總機→FMS線材,拉線測試."]
[null,"2C3150","P.B",316,"防火門(台)(2S-2P)(含FMS拉線測試)",null,"台",12400,12200,200,1.6393442622950821E-2,"含火災管制追加.含火警總機→FMS線材,拉線測試."]
["修改","2C3100","P",316,"防火門(停)(非IP)(2P-CO)",null,"停",21100,20600,500,2.4271844660194174E-2,"1.不含材質變更之差價"]
["新增","2C3110","P",316,"防火門(停)(指定IP)(2P-CO)",null,"停",30500,null,30500,{"$error":"#DIV/0!"},"1.不含材質變更之差價"]
["修改","2C3200","P.B",316,"防火門(停)(非IP)(2S-2P)",null,"停",22800,22400,400,1.7857142857142856E-2,"1.不含材質變更之差價"]
["新增","2C3210","P.B",316,"防火門(停)(指定IP)(2S-2P)",null,"停",32300,null,32300,{"$error":"#DIV/0!"},"1.不含材質變更之差價"]
[null,"2C2600","P.B.F",24,"製作烤漆色板(壓克力漆)",null,"台",2500,2500,0,0]
[null,"2C2610","P.B.F",24,"製作烤漆色板(金屬漆)",null,"台",3800,3800,0,0]
[null,"2C1900","P",24,"出入口門  金屬漆 (外包)","2P-CO ≦OP-800~900","停",3500,3500,0,0,"依金屬漆型錄: 124M~129M\n新增 4種金屬漆型號: J020, J122, J147, J191"]
[null,"2C2000","P",24,"出入口門  金屬漆 (外包)","2P-CO ≦OP-1000~1100","停",4200,4200,0,0]
[null,"2C2050","P",24,"出入口門  金屬漆 (自製)","2P-CO ≦OP-800~1100","停",1100,1000,{"$f":"H206-I206","v":100},0.1,"僅有 4種金屬漆型號: J020, J122, J147, J191"]
[null,"2C2060","P",24,"出入口門  (仿鍍鈦烤漆)","2P-CO ≦OP-800~900","停",3500,3500,{"$f":"H207-I207","v":0},0,"(M042): 仿鍍鈦古咖色, (M043): 仿鍍鈦黑色\n(M044): 仿鍍鈦古銅色, (M046): 仿鍍鈦金色"]
[null,"2C2070","P",24,"出入口門  (仿鍍鈦烤漆)","2P-CO ≦OP-1000~1100","停",4200,4200,{"$f":"H208-I208","v":0},0]
[null,"2C2700","P",105.10599999999999,"新品臨時門(三角key)(IP)","OP-800~900W × EH-2100","停",5800,5700,{"$f":"H209-I209","v":100},1.7543859649122806E-2,"(1)下述情況不能選用整修型臨時門:2S-2P,防火門,\n     面一式門框,隱藏式門框(上門框後退非20mm),廂門.\n"]
[null,"2C2710","P",105.10599999999999,"新品臨時門(三角key)(IP)","OP-800~900W × EH-2300","停",6500,6500,0,0]
[null,"2C2720","P",105.10599999999999,"新品臨時門(三角key)(IP)","OP-1000~1100W × EH-2100","停",8000,7800,{"$f":"H211-I211","v":200},{"$f":"IF(I211>0,(H211-I211)/I211,-(H211-I211)/I211)","v":2.564102564102564E-2}]
[null,"2C2730","P",105.10599999999999,"新品臨時門(三角key)(IP)","OP-1000~1100W × EH-2300","停",9100,8900,{"$f":"H212-I212","v":200},{"$f":"IF(I212>0,(H212-I212)/I212,-(H212-I212)/I212)","v":2.247191011235955E-2}]
[null,"2C2740","P",105.10599999999999,"整修型臨時門(三角key)(鍍鋅鋼板)","OP-800~900W × EH-2100","停",4400,4300,{"$f":"H213-I213","v":100},{"$f":"IF(I213>0,(H213-I213)/I213,-(H213-I213)/I213)","v":2.3255813953488372E-2}]
[null,"2C2750","P",105.10599999999999,"整修型臨時門(三角key)(鍍鋅鋼板)","OP-800~900W × EH-2300","停",5300,5100,200,3.9215686274509803E-2]
[null,"2C2760","P",105.10599999999999,"整修型臨時門(三角key)(鍍鋅鋼板)","(僅)OP-1000W × EH-2300","停",5900,5700,{"$f":"H215-I215","v":200},{"$f":"IF(I215>0,(H215-I215)/I215,-(H215-I215)/I215)","v":3.5087719298245612E-2}]
[null,"2C2770","P",86,"出入口門 (無取付三角key)","OP-800W~900W","停",2300,1800,{"$f":"H216-I216","v":500},{"$f":"IF(I216>0,(H216-I216)/I216,-(H216-I216)/I216)","v":0.27777777777777779}]
[null,"2C2780","P",86,"出入口門 (無取付三角key)","OP-1000W~1100W","停",3200,3000,{"$f":"H217-I217","v":200},{"$f":"IF(I217>0,(H217-I217)/I217,-(H217-I217)/I217)","v":6.6666666666666666E-2}]
[null,"2B0510","B",105.10599999999999,"追加乘場臨時門(三角key)(IP)","2S-2P OP=1100~1200","停",7800,7700,100,1.2987012987012988E-2,"塗裝:底漆(NO.40)"]
[null,"2C3300","P",108,"乘場臨時門(IP)(防火功能)","2P-CO ≦OP-800~900","停",15700,15400,{"$f":"H219-I219","v":300},{"$f":"IF(I219>0,(H219-I219)/I219,-(H219-I219)/I219)","v":1.948051948051948E-2}]
[null,"2C3310","P",108,"乘場臨時門(IP)(防火功能)","2P-CO ≦OP-1000~1100","停",16600,16200,{"$f":"H220-I220","v":400},{"$f":"IF(I220>0,(H220-I220)/I220,-(H220-I220)/I220)","v":2.4691358024691357E-2}]
[null,"2C3340","P",108,"乘場臨時門(IP)(防火功能)","2S-2P ≦OP-800~900","停",18800,18300,{"$f":"H221-I221","v":500},{"$f":"IF(I221>0,(H221-I221)/I221,-(H221-I221)/I221)","v":2.7322404371584699E-2}]
[null,"2C3350","P",108,"乘場臨時門(IP)(防火功能)","2S-2P ≦OP-1000~1100","停",19400,19000,{"$f":"H222-I222","v":400},{"$f":"IF(I222>0,(H222-I222)/I222,-(H222-I222)/I222)","v":2.1052631578947368E-2}]
[null,"2C1700","P",22,"出入口門  CE ","2P-CO ≦OP-800~900","停",1000,500,500,1,"素材1片(4*8)/停計算"]
[null,"2C1800","P",22,"出入口門  CE ","2P-CO ≦OP-1000~1100","停",4400,4200,200,4.7619047619047616E-2,"素材2片(4*8)/停計算"]
[null,"2C0100","P",26,"出入口門  SH","2P-CO ≦OP-800~900","停",6800,4300,2500,0.58139534883720934,"素材:為(唐榮)板材.(標準為1.5T)"]
[null,"2C0500","P",26,"出入口門  SH","2P-CO ≦OP-1000~1100","停",9100,6500,2600,0.4]
[null,"2C0200","P",26,"出入口門  SH鍍鈦(金色)","2P-CO ≦OP-800~900","停",11200,9000,2200,0.24444444444444444,"1.素材:為(唐榮)板材再加工鍍鈦.(標準為1.5T)\n2.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"2C0250","P",26,"出入口門  SH鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",20100,17900,2200,0.12290502793296089]
[null,"2C0590","P",26,"出入口門  SH鍍鈦(金色)","2P-CO ≦OP-1000","停",13000,10600,2400,0.22641509433962265]
[null,"2C0600","P",26,"出入口門  SH鍍鈦(金色)","2P-CO ≦OP-1100","停",15800,12800,{"$f":"H230-I230","v":3000},{"$f":"IF(I230>0,(H230-I230)/I230,-(H230-I230)/I230)","v":0.234375}]
[null,"2C0640","P",26,"出入口門  SH鍍鈦(遠東特殊色)","2P-CO ≦OP-1000","停",21800,19500,2300,0.11794871794871795]
[null,"2C0650","P",26,"出入口門  SH鍍鈦(遠東特殊色)","2P-CO ≦OP-1100","停",27600,24700,{"$f":"H232-I232","v":2900},{"$f":"IF(I232>0,(H232-I232)/I232,-(H232-I232)/I232)","v":0.11740890688259109}]
[null,"2C5000","P",26,"出入口門  亂紋板","2P-CO ≦OP-800~900","停",11800,9400,2400,0.25531914893617019,"1.(遠東)亂紋板: V-00\n2.(遠東)亂紋鍍鈦(金色): V-01 \n3.(遠東)亂紋鍍鈦(特殊色): V-02~V-05\n4.[遠東]特殊色: 計有咖啡. 黑色. 古銅. 古咖"]
[null,"2C5020","P",26,"出入口門  亂紋鍍鈦(金色)","2P-CO ≦OP-800~900","停",16000,13600,2400,0.17647058823529413]
[null,"2C5040","P",26,"出入口門  亂紋鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",24900,22500,2400,0.10666666666666667]
[null,"2C5100","P",26,"出入口門  亂紋板","2P-CO ≦OP-1000~1100","停",16800,13600,3200,0.23529411764705882]
[null,"2C5110","P",26,"出入口門  亂紋鍍鈦(金色)","2P-CO ≦OP-1000","停",17300,16000,{"$f":"H237-I237","v":1300},{"$f":"IF(I237>0,(H237-I237)/I237,-(H237-I237)/I237)","v":8.1250000000000003E-2}]
[null,"2C5120","P",26,"出入口門  亂紋鍍鈦(金色)","2P-CO ≦OP-1100","停",22300,19100,3200,0.16753926701570682]
[null,"2C5130","P",26,"出入口門  亂紋鍍鈦(遠東特殊色)","2P-CO ≦OP-1000","停",26100,24800,{"$f":"H239-I239","v":1300},{"$f":"IF(I239>0,(H239-I239)/I239,-(H239-I239)/I239)","v":5.2419354838709679E-2}]
[null,"2C5140","P",26,"出入口門  亂紋鍍鈦(遠東特殊色)","2P-CO ≦OP-1100","停",34200,31000,3200,0.1032258064516129]
[null,"2C5200","P",26,"出入口門  霧珠板","2P-CO ≦OP-800~900","停",12100,9700,2400,0.24742268041237114,"1.(遠東)霧珠板: B-00\n2.(遠東)霧珠鍍鈦(金色): B-01 \n3.(遠東)霧珠鍍鈦(特殊色): B-02~B-05\n4.[遠東]特殊色: 計有咖啡. 黑色. 古銅. 古咖"]
[null,"2C5220","P",26,"出入口門  霧珠鍍鈦(金色)","2P-CO ≦OP-800~900","停",16300,13900,2400,0.17266187050359713]
[null,"2C5240","P",26,"出入口門  霧珠鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",25200,22800,2400,0.10526315789473684]
[null,"2C5300","P",26,"出入口門  霧珠板","2P-CO ≦OP-1000~1100","停",17300,14000,3300,{"$f":"IF(I244>0,(H244-I244)/I244,-(H244-I244)/I244)","v":0.23571428571428571}]
[null,"2C5310","P",26,"出入口門  霧珠鍍鈦(金色)","2P-CO ≦OP-1000","停",17700,16400,{"$f":"H245-I245","v":1300},{"$f":"IF(I245>0,(H245-I245)/I245,-(H245-I245)/I245)","v":7.926829268292683E-2}]
[null,"2C5320","P",26,"出入口門  霧珠鍍鈦(金色)","2P-CO ≦OP-1100","停",22700,19500,3200,0.1641025641025641]
[null,"2C5330","P",26,"出入口門  霧珠鍍鈦(遠東特殊色)","2P-CO ≦OP-1000","停",26500,25200,1300,{"$f":"IF(I247>0,(H247-I247)/I247,-(H247-I247)/I247)","v":5.1587301587301584E-2}]
[null,"2C5340","P",26,"出入口門  霧珠鍍鈦(遠東特殊色)","2P-CO ≦OP-1100","停",34600,31500,3100,9.841269841269841E-2]
[null,"2C6100","P",26,"出入口門 1D加工鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",35900,33300,2600,7.8078078078078081E-2,"遠東1D型號：DR-04,11,19,20,DR-25~30"]
[null,"2C6150","P",26,"出入口門 1D加工鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","停",39800,37000,2800,7.567567567567568E-2]
[null,"2C6200","P",26,"出入口門 2D加工鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",43600,41000,2600,6.3414634146341464E-2,"遠東2D型號：2D-01~03,2D-07~09"]
[null,"2C6250","P",26,"出入口門 2D加工鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","停",47400,44600,2800,6.2780269058295965E-2]
[null,"2C6300","P",26,"出入口門 3D加工鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",51300,48700,2600,5.3388090349075976E-2,"遠東3D型號：3D-04~06"]
[null,"2C6350","P",26,"出入口門 3D加工鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","停",55200,52400,2800,5.3435114503816793E-2]
[null,"2C0300","P",27,"出入口門  SE ","2P-CO ≦OP-800~900","停",9300,6800,2500,0.36764705882352944,"素材:為(唐榮)板材再加工蝕刻.(標準為1.5T)"]
[null,"2C0700","P",27,"出入口門  SE ","2P-CO ≦OP-1000~1100","停",11700,9100,2600,0.2857142857142857]
[null,"2C0400","P",27,"出入口門  SE鍍鈦(金色)","2P-CO ≦OP-800~900","停",15000,12500,2500,0.2,"1.素材:為(唐榮)板材再加工蝕刻.鍍鈦.(標準為1.5T)\n2.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"2C0450","P",27,"出入口門  SE鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",25900,23500,2400,0.10212765957446808]
[null,"2C0800","P",27,"出入口門  SE鍍鈦(金色)","2P-CO ≦OP-1000~1100","停",17500,14900,2600,0.17449664429530201]
[null,"2C0850","P",27,"出入口門  SE鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","停",28900,26300,2600,9.8859315589353611E-2]
[null,"2C0900","P",266,"出入口門  SM","2P-CO ≦OP-800~900","停",8700,6100,2600,0.42622950819672129,"素材:為(日新)板材.(標準為1.5T)"]
[null,"2C1300","P",266,"出入口門  SM","2P-CO ≦OP-1000~1100","停",11200,8500,{"$f":"H262-I262","v":2700},0.31764705882352939]
[null,"2C1000","P",266,"出入口門  SM鍍鈦(金色)","2P-CO ≦OP-800~900","停",13800,11500,2300,0.2,"1.素材:為(日新)板材再加工鍍鈦.(標準為1.5T)\n2.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"2C1050","P",266,"出入口門  SM鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",22700,20300,2400,0.11822660098522167]
[null,"2C1390","P",266,"出入口門  SM鍍鈦(金色)","2P-CO ≦OP-1000","停",15200,12800,{"$f":"H265-I265","v":2400},{"$f":"IF(I265>0,(H265-I265)/I265,-(H265-I265)/I265)","v":0.1875}]
[null,"2C1400","P",266,"出入口門  SM鍍鈦(金色)","2P-CO ≦OP-1100","停",18600,15500,3100,0.2]
[null,"2C1440","P",266,"出入口門  SM鍍鈦(遠東特殊色)","2P-CO ≦OP-1000","停",24100,21700,{"$f":"H267-I267","v":2400},{"$f":"IF(I267>0,(H267-I267)/I267,-(H267-I267)/I267)","v":0.11059907834101383}]
[null,"2C1450","P",266,"出入口門  SM鍍鈦(遠東特殊色)","2P-CO ≦OP-1100","停",30500,27400,3100,0.11313868613138686]
[null,"2C1100","P",268,"出入口門  SM-E ","2P-CO ≦OP-800~900","停",11900,9300,2600,0.27956989247311825,"素材:為(日新)板材再加工蝕刻.(標準為1.5T)"]
[null,"2C1500","P",268,"出入口門  SM-E ","2P-CO ≦OP-1000~1100","停",14300,11600,2700,0.23275862068965517]
[null,"2C1200","P",268,"出入口門  SM-E鍍鈦(金色)","2P-CO ≦OP-800~900","停",17600,15000,2600,0.17333333333333334,"1.素材:為(日新)板材再加工蝕刻.鍍鈦.(標準為1.5T)\n2.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"2C1250","P",268,"出入口門  SM-E鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","停",28400,25800,2600,0.10077519379844961]
[null,"2C1600","P",268,"出入口門  SM-E鍍鈦(金色)","2P-CO ≦OP-1000~1100","停",20400,17700,2700,0.15254237288135594]
[null,"2C1650","P",268,"出入口門  SM-E鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","停",31400,28800,2600,9.0277777777777776E-2]
[null,"2C2300","P",300,"出入口門附透視窗  IP ","2P-CO ≦OP-800~900","停",8700,8000,700,8.7499999999999994E-2,"透視窗尺寸:200W*700H(標準)\nSH為標準 1.5T"]
[null,"2C2400","P",300,"出入口門附透視窗  SH  ","2P-CO ≦OP-800~900","停",17600,14300,3300,0.23076923076923078]
[null,"2C2500","P",300,"出入口門附透視窗  SM  ","2P-CO ≦OP-800~900","停",20400,17200,3200,0.18604651162790697]
[null,"2B0100","B",26,"出入口門  SH","2S-2P OP=1100~1200","停",6300,5700,600,0.10526315789473684,"素材:為(唐榮)板材.(標準為1.5T)"]
[null,"2B0110","B",26,"出入口門  SH鍍鈦(金色)","2S-2P OP=1100~1200","停",12900,12000,900,7.4999999999999997E-2,"素材:為(唐榮)板材再加工鍍鈦.(標準為1.5T)"]
[null,"2B0120","B",26,"出入口門  SH鍍鈦(遠東特殊色)","2S-2P OP=1100~1200","停",24700,23900,{"$f":"H280-I280","v":800},3.3472803347280332E-2,"素材:為(唐榮)板材再加工鍍鈦.(標準為1.5T)"]
[null,"2B0200","B",27,"出入口門  SE ","2S-2P OP=1100~1200","停",8900,8300,600,7.2289156626506021E-2,"素材:為(唐榮)板材再加工蝕刻.(標準為1.5T)"]
[null,"2B0210","B",27,"出入口門  SE鍍鈦(金色)","2S-2P OP=1100~1200","停",14700,14000,700,0.05,"素材:為國內(唐榮)板材再加工蝕刻.鍍鈦.(標準為1.5T)"]
[null,"2B0220","B",27,"出入口門  SE鍍鈦(遠東特殊色)","2S-2P OP=1100~1200","停",26100,25400,700,2.7559055118110236E-2,"素材:為國內(唐榮)板材再加工蝕刻.鍍鈦.(標準為1.5T)"]
[null,"2B0300","B",266,"出入口門  SM","2S-2P OP=1100~1200","停",8800,8200,600,7.3170731707317069E-2,"素材:為(日新)板材.(標準為1.5T)"]
[null,"2B0310","B",266,"出入口門  SM鍍鈦(金色)","2S-2P OP=1100~1200","停",15600,14800,800,5.4054054054054057E-2,"素材:為(日新)板材再加工鍍鈦.(標準為1.5T)"]
[null,"2B0320","B",266,"出入口門  SM鍍鈦(遠東特殊色)","2S-2P OP=1100~1200","停",27400,26600,800,3.007518796992481E-2,"素材:為(日新)板材再加工鍍鈦.(標準為1.5T)"]
[null,"2B0400","B",268,"出入口門  SM-E ","2S-2P OP=1100~1200","停",11900,11400,500,4.3859649122807015E-2,"素材:為(日新)板材再加工蝕刻.(標準為1.5T)"]
[null,"2B0410","B",268,"出入口門  SM-E鍍鈦(金色)","2S-2P OP=1100~1200","停",17700,17100,600,3.5087719298245612E-2,"素材:為(日新)板材再加工蝕刻.鍍鈦.(標準為1.5T)"]
[null,"2B0420","B",268,"出入口門  SM-E鍍鈦(遠東特殊色)","2S-2P OP=1100~1200","停",29100,28500,600,2.1052631578947368E-2,"素材:為(日新)板材再加工蝕刻.鍍鈦.(標準為1.5T)"]
[]
[null,"Y25100","P",38.39,"阿姆斯壯地磚BY工務","P6~P24人 ","台",4400,4400,{"$f":"H291-I291","v":0},0,"阿姆斯壯地磚厚度: 3T"]
[null,"Y25200","P",38.39,"阿姆斯壯(拼花)地磚BY工務","P6~P24人 ","台",8500,8500,0,0]
[null,"3C1000","P",38.39,"地板 花紋鋼板 (IP)","P6~P15人 (一片式)","台",6100,5900,200,3.3898305084745763E-2,"1.花紋鋼板IP厚度: 台製3.2T"]
[null,"3C1100","P",38.39,"地板 花紋鋼板 (IP)","P17~P24人 (僅接合式)","台",8700,8500,200,2.3529411764705882E-2]
[null,"3C1200","P",38.39,"地板 花紋不鏽鋼板 (SH)","P6~P13人 (一片式)","台",21700,18500,3200,0.17297297297297298,"1.花紋鋼板SH厚度: 台製3.0T (P6~13人)\n2.花紋鋼板SH厚度: 台製2.5T (P15人)\n3.花紋鋼板SH厚度: 台製3.0T (P17~24人)"]
[null,"3C1300","P",38.39,"地板 花紋不鏽鋼板 (SH)","P15人 (一片式)","台",25000,21000,4000,0.19047619047619047]
[null,"3C1400","P",38.39,"地板 花紋不鏽鋼板 (SH)","P17~P24人 (僅接合式)","台",38700,32700,6000,0.1834862385321101]
[null,"3C2000","P",38.39,"大理石貼付預留","P6~P8人","台",9500,8900,600,6.741573033707865E-2,"僅FLOOR配合大理石厚度預留"]
[null,"3C2100","P",38.39,"大理石貼付預留","P9人","台",13600,13200,400,3.0303030303030304E-2,"配合大理石厚度預留"]
[null,"3C2200","P",38.39,"大理石貼付預留","P10人(10停)(120M(含)以下)","台",35600,35000,600,1.7142857142857144E-2,"含RAIL:T-8K*T-5K→T-13K*T-5K"]
[null,"3C2300","P",38.39,"大理石貼付預留"," ± 1停  (P10人)","樓",2600,2400,200,8.3333333333333329E-2,"含RAIL:T-8K*T-5K→T-13K*T-5K"]
[null,"3C2400","P",38.39,"大理石貼付預留","P11人(10停)(120M(含)以下)","台",36300,35900,400,1.1142061281337047E-2,"含RAIL:T-8K*T-5K→T-13K*T-5K"]
[null,"3C2500","P",38.39,"大理石貼付預留"," ± 1停  (P11人)","樓",2600,2400,200,8.3333333333333329E-2,"含RAIL:T-8K*T-5K→T-13K*T-5K"]
[null,"3C2600","P",38.39,"大理石貼付預留","P12~15人(10停)(60~105m)","台",27000,26100,900,3.4482758620689655E-2,"含RAIL:T-13K*T-5K→T-13K*T-8K"]
[null,"3C2700","P",38.39,"大理石貼付預留"," ± 1停  (P12~P15人)","樓",1800,1600,200,0.125,"含RAIL:T-13K*T-5K→T-13K*T-8K"]
[null,"3C2800","P",38.39,"大理石貼付預留","P17人(60~105m)","台",14700,13400,1300,9.7014925373134331E-2,"僅FLOOR配合大理石厚度預留"]
[null,"3C2810","P",38.39,"大理石貼付預留","P20~24人(任何速度)","台",14300,14000,300,2.1428571428571429E-2,"僅FLOOR配合大理石厚度預留"]
[null,"3C2840","P",38.39,"大理石貼付預留","P13人(120M)","台",12800,12500,300,{"$f":"IF(I308>0,(H308-I308)/I308,-(H308-I308)/I308)","v":2.4E-2},"僅FLOOR配合大理石厚度預留"]
[null,"3C2850","P",38.39,"大理石貼付預留","P15人(20停)(120M)","台",94400,94100,300,3.188097768331562E-3,"含CAGE RAIL:T-13K → T-18K"]
[null,"3C2860","P",38.39,"大理石貼付預留"," ± 1停  (P15人)(120M)","樓",4500,4400,100,2.2727272727272728E-2,"含CAGE RAIL:T-13K → T-18K"]
[null,"3C2870","P",38.39,"大理石貼付預留","P17人(120M)","台",12400,12300,100,8.130081300813009E-3,"僅FLOOR配合大理石厚度預留"]
[null,"3C2880","P",38.39,"大理石貼付預留","P13~17人(150M)","台",14100,13900,200,1.4388489208633094E-2,"僅FLOOR配合大理石厚度預留"]
[null,"3C2900","P",38.39,"石英磚貼付預留(10mm)","P6~P24人 ","台",9800,9100,700,7.6923076923076927E-2,"僅FLOOR配合石英磚厚度(10mm以下)預留"]
[null,"3C3100","P",38.39,"大理石貼付預留","P6~P24人(無機房用)","台",11900,11300,600,5.3097345132743362E-2,"僅FLOOR配合大理石厚度預留"]
[null,"3B1000","B",38.39,"大理石貼付預留","B-750kg ","台",16800,16700,100,5.9880239520958087E-3,"僅FLOOR配合大理石厚度預留"]
[null,"3B1100","B",38.39,"大理石貼付預留","B-1000kg (4停)","台",36700,37200,-500,-1.3440860215053764E-2,"FLOOR配合大理石厚度預留\n含CAGE RAIL:T-13K→T-18K"]
[null,"3B1200","B",38.39,"大理石貼付預留"," ± 1停  (B-1000kg )","樓",3900,4000,-100,-2.5000000000000001E-2,"含CAGE RAIL:T-13K→T-18K"]
[null,"3F0100","F",38.39,"地板 花紋不鏽鋼板 (SH)","F-1000kg ","台",22500,16500,6000,0.36363636363636365,"接合式厚度: 3.0T (台製品)"]
[null,"3F0200","F",38.39,"地板 花紋不鏽鋼板 (SH)","F-1500~2000kg ","台",51000,37200,13800,0.37096774193548387,"接合式厚度: 4.5T (台製品)"]
[null,"3F0300","F",38.39,"地板 花紋不鏽鋼板 (SH)","F-2500~3000kg ","台",106600,80000,{"$f":"H320-I320","v":26600},0.33250000000000002,"接合式厚度: 6.0T (台製品)"]
[null,"G01000","P",38.39,"車廂地毯(P-11人(含)以下)",null,"台",3400,3400,0,0]
[null,"G01100","P",38.39,"車廂地毯(P-12人(含)以上)",null,"台",4100,4100,0,0]
[null,"E00100","P",38.39,"3M地毯(P-11人(含)以下)",null,"台",4100,4100,0,0]
[null,"E00200","P",38.39,"3M地毯(P-12人(含)以上)",null,"台",5500,5500,0,0]
[]
[null,"4C8700","P",42,"CH天井(IP→SH)(不含CH-18)","(P6~17人)CH-18除外","台",19600,15000,{"$f":"H326-I326","v":4600},0.30666666666666664]
[null,"4C8710","P",42,"CH-18天井(IP→SH)","(P6~17人)","台",35800,34500,1300,3.7681159420289857E-2,"因造型特殊,非IP材質,需有後續修飾意匠處理."]
[null,"4C8720","P",42,"天井型式 (H4) ","P12~P24人","台",16300,16100,200,{"$f":"IF(I328>0,(H328-I328)/I328,-(H328-I328)/I328)","v":1.2422360248447204E-2},"限P-12(含)以上人乘選用"]
[null,"4C8730","P",42,"天井型式 (CPD) ","P12~P24人","台",-16000,-14900,-1100,{"$f":"IF(I329>0,(H329-I329)/I329,-(H329-I329)/I329)","v":-7.3825503355704702E-2},"CPD天井: 預留170mm, 以供天井裝璜."]
[null,"4C8740","P",42,"天井型式 (A2)","P10~P24人","台",81700,38000,43700,{"$f":"IF(I330>0,(H330-I330)/I330,-(H330-I330)/I330)","v":1.1499999999999999},"(TK-ED-003+SM)"]
[null,"Y25600","P",42,"天井型式 (VIP-01)","P10~P24人","台",81700,38000,43700,{"$f":"IF(I331>0,(H331-I331)/I331,-(H331-I331)/I331)","v":1.1499999999999999},"(TK-ED-011)"]
[null,"4B1400","B",42,"B TYPE STD天井(IP→SH)","B-750~1000KG","台",15000,14300,700,4.8951048951048952E-2,"SH素材為國內(唐榮)板材"]
[null,"4F1600","F",42,"F TYPE STD天井(IP→SH)","F-1000kg","台",26000,19300,6700,0.34715025906735753,"SH素材為國內(唐榮)板材"]
[null,"4F1700","F",42,"F TYPE STD天井(IP→SH)","F-1500kg~2000kg","台",34700,24300,10400,0.4279835390946502,"SH素材為國內(唐榮)板材"]
[null,"4F1800","F",42,"F TYPE STD天井(IP→SH)","F-2500kg~3000kg","台",47200,34200,13000,0.38011695906432746,"SH素材為國內(唐榮)板材"]
[]
[null,"4C6000","P",30,"廂門   SH","2P-CO ≦OP-800~900","台",6600,4200,{"$f":"H337-I337","v":2400},0.5714285714285714,"素材:為國內(唐榮)板材"]
[null,"4C6050","P",30,"廂門   SH","2P-CO ≦OP-1000~1100","台",9200,5500,3700,0.67272727272727273]
[null,"4C6200","P",30,"廂門   SE","2P-CO ≦OP-800~900","台",9100,6800,2300,0.33823529411764708,"SH素材為(唐榮)板材於國內加工蝕刻"]
[null,"4C6250","P",30,"廂門   SE","2P-CO ≦OP-1000~1100","台",11700,7900,3800,0.48101265822784811]
[null,"4C6400","P",30,"廂門   SM","2P-CO ≦OP-800~900","台",9300,6800,2500,0.36764705882352944,"素材為(日新)板材於國內加工"]
[null,"4C6450","P",30,"廂門   SM","2P-CO ≦OP-1000~1100","台",12800,9000,3800,0.42222222222222222]
[null,"4C6600","P",30,"廂門   SM-E","2P-CO ≦OP-800~900","台",12500,10100,2400,0.23762376237623761,"素材為(日新)板材於國內加工&蝕刻"]
[null,"4C6650","P",30,"廂門   SM-E","2P-CO ≦OP-1000~1100","台",16000,12100,3900,0.32231404958677684]
[null,"4C6100","P",30,"廂門   SH 鍍鈦(金色)","2P-CO ≦OP-800~900","台",11100,9000,2100,0.23333333333333334,"SH素材為(唐榮)板材於國內加工鍍鈦"]
[null,"4C6150","P",30,"廂門   SH 鍍鈦(金色)","2P-CO ≦OP-1000~1100","台",14500,11700,2800,0.23931623931623933]
[null,"4C6160","P",30,"廂門   SH 鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","台",20100,18000,2100,0.11666666666666667,"SH素材為(唐榮)板材於國內加工鍍鈦\n[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C6170","P",30,"廂門   SH 鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","台",26300,23600,2700,0.11440677966101695]
[null,"4C4200","P",30,"廂門   亂紋板","2P-CO ≦OP-800~900","台",11400,9100,2300,0.25274725274725274,"亂紋板為(日新)板材於國內加工\n亂紋鍍鈦板為(日新)板材於國內加工&鍍鈦\n1.(遠東)亂紋板: V-00\n2.(遠東)亂紋鍍鈦(金色): V-01 \n3.(遠東)亂紋鍍鈦(特殊色): V-02~V-05\n4.[遠東]特殊色: 計有咖啡. 黑色. 古銅. 古咖"]
[null,"4C4210","P",30,"廂門   亂紋板","2P-CO ≦OP-1000~1100","台",14800,11900,2900,0.24369747899159663]
[null,"4C4220","P",30,"廂門   亂紋鍍鈦(金色)","2P-CO ≦OP-800~900","台",15600,13400,2200,0.16417910447761194]
[null,"4C4230","P",30,"廂門   亂紋鍍鈦(金色)","2P-CO ≦OP-1000~1100","台",20400,17500,2900,0.1657142857142857]
[null,"4C4240","P",30,"廂門   亂紋鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","台",24500,22200,2300,0.1036036036036036]
[null,"4C4250","P",30,"廂門   亂紋鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","台",32300,29300,3000,0.10238907849829351]
[null,"4C4300","P",30,"廂門   霧珠板","2P-CO ≦OP-800~900","台",11700,9400,2300,0.24468085106382978,"霧珠板為(日新)板材於國內加工\n霧珠鍍鈦板為(日新)板材於國內加工&鍍鈦\n1.(遠東)霧珠板: B-00\n2.(遠東)霧珠鍍鈦(金色): B-01 \n3.(遠東)霧珠鍍鈦(特殊色): B-02~B-05\n4.[遠東]特殊色: 計有咖啡. 黑色. 古銅. 古咖"]
[null,"4C4310","P",30,"廂門   霧珠板","2P-CO ≦OP-1000~1100","台",15200,12300,2900,0.23577235772357724]
[null,"4C4320","P",30,"廂門   霧珠鍍鈦(金色)","2P-CO ≦OP-800~900","台",15900,13600,2300,0.16911764705882354]
[null,"4C4330","P",30,"廂門   霧珠鍍鈦(金色)","2P-CO ≦OP-1000~1100","台",20800,17900,2900,0.16201117318435754]
[null,"4C4340","P",30,"廂門   霧珠鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","台",24800,22500,2300,0.10222222222222223]
[null,"4C4350","P",30,"廂門   霧珠鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","台",32700,29700,3000,0.10101010101010101]
[null,"4C6300","P",30,"廂門   SE 鍍鈦(金色)","2P-CO ≦OP-800~900","台",15300,13000,2300,0.17692307692307693,"SH素材為(唐榮)板材於國內加工.蝕刻&鍍鈦"]
[null,"4C6350","P",30,"廂門   SE 鍍鈦(金色)","2P-CO ≦OP-1000~1100","台",17900,14200,3700,0.26056338028169013]
[null,"4C6360","P",30,"廂門   SE 鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","台",28600,26200,2400,9.1603053435114504E-2,"SH素材為(唐榮)板材於國內加工.蝕刻&鍍鈦\n[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C6370","P",30,"廂門   SE 鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","台",32600,28800,3800,0.13194444444444445]
[null,"4C6500","P",30,"廂門   SM 鍍鈦(金色)","2P-CO ≦OP-800~900","台",13400,11200,2200,0.19642857142857142,"素材為(日新)板材於國內加工&鍍鈦"]
[null,"4C6550","P",30,"廂門   SM 鍍鈦(金色)","2P-CO ≦OP-1000~1100","台",17500,14600,2900,0.19863013698630136]
[null,"4C6560","P",30,"廂門   SM 鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","台",22300,20000,2300,0.115,"SM素材為(日新)板材於國內加工鍍鈦\n[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C6570","P",30,"廂門   SM 鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","台",29400,26500,2900,0.10943396226415095]
[null,"4C6700","P",30,"廂門   SM-E 鍍鈦(金色)","2P-CO ≦OP-800~900","台",18500,16200,2300,0.1419753086419753,"素材為(日新)板材於國內加工,蝕刻&鍍鈦"]
[null,"4C6750","P",30,"廂門   SM-E 鍍鈦(金色)","2P-CO ≦OP-1000~1100","台",22100,18300,3800,0.20765027322404372]
[null,"4C6760","P",30,"廂門   SM-E 鍍鈦(遠東特殊色)","2P-CO ≦OP-800~900","台",31700,29300,2400,8.191126279863481E-2,"SM素材為(日新)板材於國內加工蝕刻&鍍鈦\n[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C6770","P",30,"廂門   SM-E 鍍鈦(遠東特殊色)","2P-CO ≦OP-1000~1100","台",36800,32900,3900,0.11854103343465046]
[null,"4C6900","P",30,"廂門附透視窗  IP","2P-CO ≦OP-800~1100","台",5800,5200,600,0.11538461538461539,"1.透視窗標準尺寸: 200W*700H\n2.特殊開窗尺寸另予檢討"]
[null,"4C6950","P",30,"廂門附透視窗  SH","2P-CO ≦OP-800~900","台",17500,14200,3300,{"$f":"IF(I374>0,(H374-I374)/I374,-(H374-I374)/I374)","v":0.23239436619718309}]
[null,"4C7000","P",30,"廂門附透視窗  SH","2P-CO ≦OP-1000~1100","台",23900,20600,3300,0.16019417475728157]
[null,"4C7120","P",30,"廂門  IP (仿鍍鈦烤漆)","2P-CO ≦OP-800~900","台",3800,3900,{"$f":"H376-I376","v":-100},-2.564102564102564E-2,"(M042): 仿鍍鈦古咖色, (M043): 仿鍍鈦黑色\n(M044): 仿鍍鈦古銅色, (M046): 仿鍍鈦金色"]
[null,"4C7130","P",30,"廂門  IP (仿鍍鈦烤漆)","2P-CO ≦OP-1000~1100","台",4300,4400,{"$f":"H377-I377","v":-100},{"$f":"IF(I377>0,(H377-I377)/I377,-(H377-I377)/I377)","v":-2.2727272727272728E-2}]
[null,"4B0500","B",30,"B-TYPE 廂門 SH","2S-2P OP-1100~1200","台",7200,6800,400,5.8823529411764705E-2,"1.SH素材為國內(唐榮)板材\n2.SH素材為(唐榮)板材於國內加工鍍鈦\n3.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4B0510","B",30,"B-TYPE 廂門 SH鍍鈦(金色)","2S-2P OP-1100~1200","台",14000,13400,{"$f":"H379-I379","v":600},4.4776119402985072E-2]
[null,"4B0520","B",30,"B-TYPE 廂門 SH鍍鈦(遠東特殊色)","2S-2P OP-1100~1200","台",25600,25100,{"$f":"H380-I380","v":500},1.9920318725099601E-2]
[null,"4B0600","B",30,"B-TYPE 廂門 SE","2S-2P OP-1100~1200","台",9800,9400,400,4.2553191489361701E-2,"1.SH素材為(唐榮)板材於國內加工蝕刻\n2.SH素材為(唐榮)板材於國內加工.蝕刻&鍍鈦\n3.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4B0610","B",30,"B-TYPE 廂門 SE鍍鈦(金色)","2S-2P OP-1100~1200","台",15500,15200,{"$f":"H382-I382","v":300},1.9736842105263157E-2]
[null,"4B0620","B",30,"B-TYPE 廂門 SE鍍鈦(遠東特殊色)","2S-2P OP-1100~1200","台",27000,26600,{"$f":"H383-I383","v":400},1.5037593984962405E-2]
[null,"4B0700","B",30,"B-TYPE 廂門 SM","2S-2P OP-1100~1200","台",11300,10500,800,7.6190476190476197E-2,"1.SM素材為(日新)板材於國內加工\n2.SM素材為(日新)板材於國內加工鍍鈦\n3.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4B0710","B",30,"B-TYPE 廂門 SM鍍鈦(金色)","2S-2P OP-1100~1200","台",16800,16000,{"$f":"H385-I385","v":800},0.05]
[null,"4B0720","B",30,"B-TYPE 廂門 SM鍍鈦(遠東特殊色)","2S-2P OP-1100~1200","台",28400,27700,{"$f":"H386-I386","v":700},2.5270758122743681E-2]
[null,"4B0800","B",30,"B-TYPE 廂門 SM-E","2S-2P OP-1100~1200","台",14500,13700,800,5.8394160583941604E-2,"1.SM素材為(日新)板材於國內加工蝕刻\n2.SM素材為(日新)板材於國內加工.蝕刻&鍍鈦\n3.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4B0810","B",30,"B-TYPE 廂門 SM-E鍍鈦(金色)","2S-2P OP-1100~1200","台",20000,19300,{"$f":"H388-I388","v":700},3.6269430051813469E-2]
[null,"4B0820","B",30,"B-TYPE 廂門 SM-E鍍鈦(遠東特殊色)","2S-2P OP-1100~1200","台",31500,30800,{"$f":"H389-I389","v":700},2.2727272727272728E-2]
[]
[null,"4C7100","P",107,"追加臨時廂門 (IP)","2P-CO ≦OP-800~900","台",11500,11500,{"$f":"H391-I391","v":0},0,"1.塗裝:底漆(NO.40)\n2.廂門無整修型臨時門"]
[null,"4C7110","P",107,"追加臨時廂門 (IP)","2P-CO ≦OP-1000~1100","台",12700,12500,{"$f":"H392-I392","v":200},1.6E-2]
[]
[null,"4C0100","P","30.43.44.45","車廂側板&廂門  SH","P6~P9人 ","台",34900,21700,{"$f":"H394-I394","v":13200},0.60829493087557607,"1.SH素材為國內(唐榮)板材\n2.OPB側板: SH 1.2T\n3.OPB型式: KF-D型式(SM)"]
[null,"4C0150","P","30.43.44.45","車廂側板&廂門  SH","P10~P12人 ","台",43400,26600,16800,0.63157894736842102]
[null,"4C0200","P","30.43.44.45","車廂側板&廂門  SH","P13~P17人 ","台",47700,28200,19500,0.69148936170212771]
[null,"4C0250","P","30.43.44.45","車廂側板&廂門  SH","P20~P24人 ","台",54000,29500,24500,0.83050847457627119]
[null,"4C0300","P","30.43.44.45","車廂側板&廂門  SH鍍鈦(金色)","P6~P9人 ","台",73200,61500,11700,0.19024390243902439,"1.SH鍍鈦材為(唐榮)板材於國內加工鍍鈦\n2.OPB側板: SH 1.2T鍍鈦\n3.OPB型式: KF-D型式(SM鍍鈦), 按鈕鍍鈦另加計"]
[null,"4C0350","P","30.43.44.45","車廂側板&廂門  SH鍍鈦(金色)","P10~P12人 ","台",85000,70000,15000,0.21428571428571427]
[null,"4C0400","P","30.43.44.45","車廂側板&廂門  SH鍍鈦(金色)","P13~P17人 ","台",95900,79500,16400,0.20628930817610064]
[null,"4C0450","P","30.43.44.45","車廂側板&廂門  SH鍍鈦(金色)","P20~P24人 ","台",115800,95500,20300,0.21256544502617802]
[null,"4C0460","P","30.43.44.45","車廂側板&廂門  SH鍍鈦(遠東特殊色)","P6~P9人 (&R.T PANEL)","台",130700,119000,11700,9.8319327731092435E-2,"1.SH素材為(唐榮)板材於國內加工鍍鈦\n2.OPB側板: SH 1.2T鍍鈦\n3.OPB型式: KF-D型式(SM鍍鈦), 按鈕鍍鈦另加計\n4.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C0470","P","30.43.44.45","車廂側板&廂門  SH鍍鈦(遠東特殊色)","P10~P12人 (&R.T PANEL) ","台",151500,136500,15000,0.10989010989010989]
[null,"4C0480","P","30.43.44.45","車廂側板&廂門  SH鍍鈦(遠東特殊色)","P13~P17人 (&R.T PANEL) ","台",171300,154900,16400,0.10587475790832795]
[null,"4C0490","P","30.43.44.45","車廂側板&廂門  SH鍍鈦(遠東特殊色)","P20~P24人 (&R.T PANEL)","台",210500,189500,21000,0.11081794195250659]
[null,"4C1700","P","30.43.44.45","車廂側板&廂門  亂紋板","P6~P9人 ","台",78600,64900,13700,0.2110939907550077,"1.亂紋板材為(日新)板材於國內加工\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光)\n4.(遠東)亂紋板: V-00"]
[null,"4C1710","P","30.43.44.45","車廂側板&廂門  亂紋板","P10~P12人 ","台",90800,73600,17200,0.23369565217391305]
[null,"4C1720","P","30.43.44.45","車廂側板&廂門  亂紋板","P13~P17人 ","台",102200,83500,18700,0.22395209580838324]
[null,"4C1730","P","30.43.44.45","車廂側板&廂門  亂紋板","P20~P24人 ","台",122400,99500,22900,0.23015075376884422]
[null,"4C1740","P","30.43.44.45","車廂側板&廂門  亂紋鍍鈦(金色)","P6~P9人 ","台",105900,92200,13700,0.14859002169197397,"1.亂紋鍍鈦板為(日新)板材於國內加工&鍍鈦\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計\n4.(遠東)亂紋鍍鈦(金色): V-01"]
[null,"4C1750","P","30.43.44.45","車廂側板&廂門  亂紋鍍鈦(金色)","P10~P12人 ","台",122200,105000,17200,0.16380952380952382]
[null,"4C1760","P","30.43.44.45","車廂側板&廂門  亂紋鍍鈦(金色)","P13~P17人 ","台",137500,118800,18700,0.15740740740740741]
[null,"4C1770","P","30.43.44.45","車廂側板&廂門  亂紋鍍鈦(金色)","P20~P24人 ","台",163300,140500,22800,0.16227758007117438]
[null,"4C1780","P","30.43.44.45","車廂側板&廂門  亂紋鍍鈦(遠東特殊色)","P6~P9人 ","台",163600,149900,13700,9.13942628418946E-2,"1.亂紋鍍鈦板為(日新)板材於國內加工&鍍鈦\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計\n4.(遠東)亂紋鍍鈦(特殊色): V-02~V-05"]
[null,"4C1790","P","30.43.44.45","車廂側板&廂門  亂紋鍍鈦(遠東特殊色)","P10~P12人 ","台",188700,171500,17200,0.10029154518950437]
[null,"4C1792","P","30.43.44.45","車廂側板&廂門  亂紋鍍鈦(遠東特殊色)","P13~P17人 ","台",212900,194200,18700,9.6292481977342942E-2]
[null,"4C1794","P","30.43.44.45","車廂側板&廂門  亂紋鍍鈦(遠東特殊色)","P20~P24人 ","台",250600,227700,22900,0.10057092665788318]
[null,"4C1840","P","30.43.44.45","車廂側板&廂門  霧珠板","P6~P9人 ","台",80700,67000,13700,0.20447761194029851,"1.霧珠板材為(日新)板材於國內加工\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光)\n4.(遠東)霧珠板: B-00"]
[null,"4C1842","P","30.43.44.45","車廂側板&廂門  霧珠板","P10~P12人 ","台",93100,76000,17100,0.22500000000000001]
[null,"4C1844","P","30.43.44.45","車廂側板&廂門  霧珠板","P13~P17人 ","台",104700,85900,18800,0.21885913853317812]
[null,"4C1850","P","30.43.44.45","車廂側板&廂門  霧珠板","P20~P24人 ","台",125400,102500,22900,0.22341463414634147]
[null,"4C1860","P","30.43.44.45","車廂側板&廂門  霧珠鍍鈦(金色)","P6~P9人 ","台",107800,94100,13700,0.14558979808714134,"1.霧珠鍍鈦板為(日新)板材於國內加工&鍍鈦\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計\n4.(遠東)霧珠鍍鈦(金色): B-01"]
[null,"4C1870","P","30.43.44.45","車廂側板&廂門  霧珠鍍鈦(金色)","P10~P12人 ","台",124500,107300,17200,0.16029822926374651]
[null,"4C1880","P","30.43.44.45","車廂側板&廂門  霧珠鍍鈦(金色)","P13~P17人 ","台",140500,121800,18700,0.15353037766830871]
[null,"4C1890","P","30.43.44.45","車廂側板&廂門  霧珠鍍鈦(金色)","P20~P24人 ","台",166300,143500,22800,0.1588850174216028]
[null,"4C1900","P","30.43.44.45","車廂側板&廂門  霧珠鍍鈦(遠東特殊色)","P6~P9人 ","台",165500,151800,13700,9.025032938076416E-2,"1.霧珠鍍鈦板為(日新)板材於國內加工&鍍鈦\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計\n4.(遠東)霧珠鍍鈦(特殊色): B-02~B-05"]
[null,"4C1910","P","30.43.44.45","車廂側板&廂門  霧珠鍍鈦(遠東特殊色)","P10~P12人 ","台",191000,173900,17100,9.8332374928119609E-2]
[null,"4C1920","P","30.43.44.45","車廂側板&廂門  霧珠鍍鈦(遠東特殊色)","P13~P17人 ","台",215500,196800,18700,9.5020325203252029E-2]
[null,"4C1930","P","30.43.44.45","車廂側板&廂門  霧珠鍍鈦(遠東特殊色)","P20~P24人 ","台",253600,230700,22900,9.926311226701344E-2]
[null,"4C0500","P","30.43.44.45","車廂側板&廂門  SE","P6~P9人 ","台",46500,33300,13200,0.3963963963963964,"1.SH素材為國內(唐榮)板材於國內加工蝕刻\n2.前&OPB側,CPI維持SH,不作蝕刻處理\n3.OPB型式: KF-D型式(SM)(不作蝕刻)"]
[null,"4C0550","P","30.43.44.45","車廂側板&廂門  SE","P10~P12人 ","台",57800,40900,16900,0.41320293398533009]
[null,"4C0600","P","30.43.44.45","車廂側板&廂門  SE","P13~P17人 ","台",62000,42500,19500,0.45882352941176469]
[null,"4C0650","P","30.43.44.45","車廂側板&廂門  SE","P20~P24人 ","台",68200,43600,24600,0.56422018348623848]
[null,"4C0700","P","30.43.44.45","車廂側板&廂門  SE鍍鈦(金色)","P6~P9人 ","台",83300,70000,13300,0.19,"1.SH素材為(唐榮)板材於國內加工蝕刻&鍍鈦\n2.前&OPB側,CPI維持SH鍍鈦,不作蝕刻處理\n3.OPB型式: KF-D型式(SM鍍鈦)(不作蝕刻)"]
[null,"4C0750","P","30.43.44.45","車廂側板&廂門  SE鍍鈦(金色)","P10~P12人 ","台",100900,84000,16900,0.2011904761904762]
[null,"4C0800","P","30.43.44.45","車廂側板&廂門  SE鍍鈦(金色)","P13~P17人 ","台",105500,86000,19500,0.22674418604651161]
[null,"4C0850","P","30.43.44.45","車廂側板&廂門  SE鍍鈦(金色)","P20~P24人 ","台",111800,87200,24600,0.28211009174311924]
[null,"4C0860","P","30.43.44.45","車廂側板&廂門  SE鍍鈦(遠東特殊色)","P6~P9人 (&R.T PANEL)","台",160800,147500,13300,{"$f":"IF(I438>0,(H438-I438)/I438,-(H438-I438)/I438)","v":9.0169491525423723E-2},"1.SH素材為(唐榮)板材於國內加工蝕刻&鍍鈦\n2.前&OPB側,CPI維持SH鍍鈦,不作蝕刻處理\n3.3.OPB型式: KF-D型式(SM鍍鈦)(不作蝕刻)\n4.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C0870","P","30.43.44.45","車廂側板&廂門  SE鍍鈦(遠東特殊色)","P10~P12人 (&R.T PANEL) ","台",190600,174100,16500,9.4773118897185524E-2]
[null,"4C0880","P","30.43.44.45","車廂側板&廂門  SE鍍鈦(遠東特殊色)","P13~P17人 (&R.T PANEL) ","台",205000,186000,19000,0.10215053763440861]
[null,"4C0890","P","30.43.44.45","車廂側板&廂門  SE鍍鈦(遠東特殊色)","P20~P24人 (&R.T PANEL)","台",219600,195400,24200,0.12384851586489252]
[null,"4C2000","P","30.43.44.45","側板&廂門 IP(NO.40),CPD天井","P6~P9人 ","台",-14100,-13400,-700,-5.2238805970149252E-2,"1.標準仕樣: 標準OP*EH-2100\n2.天井型式: CPD天井\n3.車廂高度: 2470mm(CPD天井至地板面)\n                    預留170mm以供天井裝璜."]
[null,"4C2050","P","30.43.44.45","側板&廂門 IP(NO.40),CPD天井","P10~P12人 ","台",-16600,-16200,-400,-2.4691358024691357E-2]
[null,"4C2100","P","30.43.44.45","側板&廂門 IP(NO.40),CPD天井","P13~P17人 ","台",-19000,-17500,-1500,-8.5714285714285715E-2]
[null,"4C2150","P","30.43.44.45","側板&廂門 IP(NO.40),CPD天井","P20~P24人 ","台",-22900,-21500,-1400,-6.5116279069767441E-2]
[null,"4C2160","P","30.43.44.45","側板&廂門 IP(仿鍍鈦烤漆)","P8~P15人 ","台",18500,19000,{"$f":"H446-I446","v":-500},{"$f":"IF(I446>0,(H446-I446)/I446,-(H446-I446)/I446)","v":-2.6315789473684209E-2}]
[null,"4C2165","P","30.43.44.45","側板&廂門 IP(仿鍍鈦烤漆)","P17~P24人 ","台",25500,25900,{"$f":"H447-I447","v":-400},{"$f":"IF(I447>0,(H447-I447)/I447,-(H447-I447)/I447)","v":-1.5444015444015444E-2}]
[null,"4C0900","P","30.43.44.45","車廂側板&廂門  SM","P6~P9人 (&R. PANEL)","台",60100,45500,14600,0.3208791208791209,"1.SM素材為(日新)板材於國內加工\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光)"]
[null,"4C0950","P","30.43.44.45","車廂側板&廂門  SM","P10~P12人 (&R. PANEL) ","台",74200,55600,18600,0.3345323741007194]
[null,"4C1000","P","30.43.44.45","車廂側板&廂門  SM","P13~P17人 (&R. PANEL) ","台",76400,56900,19500,0.34270650263620389]
[null,"4C1050","P","30.43.44.45","車廂側板&廂門  SM","P20~P24人 (&R. PANEL) ","台",87400,62300,25100,0.4028892455858748]
[null,"4C1100","P","30.43.44.45","車廂側板&廂門  SM鍍鈦(金色)","P6~P9人 (&R. PANEL) ","台",86500,73900,12600,0.17050067658998647,"1.SM素材為(日新)板材於國內加工鍍鈦\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計"]
[null,"4C1150","P","30.43.44.45","車廂側板&廂門  SM鍍鈦(金色)","P10~P12人 (&R. PANEL) ","台",100700,84700,16000,0.18890200708382526]
[null,"4C1200","P","30.43.44.45","車廂側板&廂門  SM鍍鈦(金色)","P13~P17人 (&R. PANEL) ","台",113900,96300,17600,0.18276220145379024]
[null,"4C1250","P","30.43.44.45","車廂側板&廂門  SM鍍鈦(金色)","P20~P24人 (&R. PANEL) ","台",142000,119600,22400,0.18729096989966554]
[null,"4C1260","P","30.43.44.45","車廂側板&廂門  SM鍍鈦(遠東特殊色)","P6~P9人 (&R. PANEL) ","台",144100,131600,12500,9.4984802431610948E-2,"1.SM素材為(日新)板材於國內加工鍍鈦\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計\n4.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C1270","P","30.43.44.45","車廂側板&廂門  SM鍍鈦(遠東特殊色)","P10~P12人 (&R. PANEL) ","台",167300,151200,16100,0.10648148148148148]
[null,"4C1280","P","30.43.44.45","車廂側板&廂門  SM鍍鈦(遠東特殊色)","P13~P17人 (&R. PANEL) ","台",189300,171700,{"$f":"H458-I458","v":17600},0.1025043680838672]
[null,"4C1290","P","30.43.44.45","車廂側板&廂門  SM鍍鈦(遠東特殊色)","P20~P24人 (&R. PANEL) ","台",231300,208900,22400,0.10722833891814265]
[null,"4C1300","P","30.43.44.45","車廂側板&廂門  SM-E","P6~P9人 (&R. PANEL) ","台",74300,59700,14600,0.24455611390284757,"1.SM素材為(日新)板材於國內加工蝕刻\n2.OPB側板為RETURN PANEL\n3.前&OPB側,CPI維持SM,不作蝕刻處理\n4.按鈕: 橢圓形按鈕(橘光)"]
[null,"4C1350","P","30.43.44.45","車廂側板&廂門  SM-E","P10~P12人 (&R. PANEL) ","台",91400,72800,18600,0.25549450549450547]
[null,"4C1400","P","30.43.44.45","車廂側板&廂門  SM-E","P13~P17人 (&R. PANEL) ","台",93600,74000,19600,0.26486486486486488]
[null,"4C1450","P","30.43.44.45","車廂側板&廂門  SM-E","P20~P24人 (&R. PANEL) ","台",104600,79500,25100,0.31572327044025156]
[null,"4C1500","P","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(金色)","P6~P9人 (&R. PANEL) ","台",110300,95700,14600,0.15256008359456635,"1.SM素材為(日新)板材於國內加工蝕刻&鍍鈦\n2.OPB側板為RETURN PANEL\n3.前&OPB側,CPI維持SM鍍鈦,不作蝕刻處理\n4.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計"]
[null,"4C1550","P","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(金色)","P10~P12人 (&R. PANEL) ","台",133400,114800,18600,0.16202090592334495]
[null,"4C1600","P","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(金色)","P13~P17人 (&R. PANEL) ","台",137300,117700,19600,0.16652506372132542]
[null,"4C1650","P","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(金色)","P20~P24人 (&R. PANEL) ","台",150500,125500,25000,0.19920318725099601]
[null,"4C1660","P","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(遠東特殊色)","P6~P9人 (&R. PANEL) ","台",188600,174000,14600,8.39080459770115E-2,"1.SM素材為(日新)板材於國內加工蝕刻&鍍鈦\n2.OPB側板為RETURN PANEL\n3.前&OPB側,CPI維持SM鍍鈦,不作蝕刻處理\n4.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計"]
[null,"4C1670","P","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(遠東特殊色)","P10~P12人 (&R. PANEL) ","台",225300,205500,19800,9.6350364963503646E-2]
[null,"4C1680","P","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(遠東特殊色)","P13~P17人 (&R. PANEL) ","台",237300,217600,19700,9.0533088235294115E-2]
[null,"4C1690","P","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(遠東特殊色)","P20~P24人 (&R. PANEL) ","台",255500,230300,25200,0.10942249240121581]
[null,"4C7200","P","30.43.44.45","車廂意匠(VIP-01)","P10~P12人 (&R. PANEL) ","台",262600,231800,30800,0.13287316652286454,"1.OPB側板: R.T PANEL\n2.後側含亂紋鍍鈦扶手×1"]
[null,"4C7210","P","30.43.44.45","車廂意匠(VIP-01)","P13~P17人 (&R. PANEL) ","台",286600,265400,21200,7.9879427279577989E-2]
[null,"4C7220","P","30.43.44.45","車廂意匠(VIP-01)","P20~P24人 (&R. PANEL) ","台",347900,296900,51000,0.17177500842034354]
[null,"4C7250","P","30.43.44.45","車廂意匠(VIP-02)","P10~P12人 (&R. PANEL) ","台",105200,101500,3700,3.6453201970443348E-2,"1.OPB側板: R.T PANEL\n"]
[null,"4C7260","P","30.43.44.45","車廂意匠(VIP-02)","P13~P17人 (&R. PANEL) ","台",119200,115100,4100,3.5621198957428324E-2]
[null,"4C7270","P","30.43.44.45","車廂意匠(VIP-02)","P20~P24人 (&R. PANEL) ","台",142700,137000,5700,4.1605839416058395E-2]
[null,"4C7300","P","30.43.44.45","車廂意匠(VIP-03)","P10~P12人 (&R. PANEL) ","台",67000,66000,1000,1.5151515151515152E-2,"1.OPB側板: R.T PANEL\n2.後側含拋光扶手×1"]
[null,"4C7310","P","30.43.44.45","車廂意匠(VIP-03)","P13~P17人 (&R. PANEL) ","台",71300,70100,1200,1.7118402282453638E-2]
[null,"4C7320","P","30.43.44.45","車廂意匠(VIP-03)","P20~P24人 (&R. PANEL) ","台",82000,80300,1700,2.1170610211706103E-2]
[null,"4C7350","P","30.43.44.45","車廂意匠(VIP-04)","P10~P12人 (&R. PANEL) ","台",159200,152900,6300,4.1203400915631135E-2,"1.OPB側板: R.T PANEL\n2.兩側附SH壓條鍍鈦×4"]
[null,"4C7360","P","30.43.44.45","車廂意匠(VIP-04)","P13~P17人 (&R. PANEL) ","台",186300,178900,7400,4.1363890441587482E-2]
[null,"4C7370","P","30.43.44.45","車廂意匠(VIP-04)","P20~P24人 (&R. PANEL) ","台",215000,206200,8800,4.2677012609117361E-2]
[null,"4B0100","B","30.43.44.45","車廂側板&廂門  SH","B-750kg~1000kg","台",51800,48100,3700,7.6923076923076927E-2,"1.SH素材為國內(唐榮)板材\n2.OPB型式: OPY-HD2 (SH or SH鍍鈦)"]
[null,"4B0110","B","30.43.44.45","車廂側板&廂門  SH鍍鈦(金色)","B-750kg~1000kg","台",120900,98700,22200,0.22492401215805471]
[null,"4B0120","B","30.43.44.45","車廂側板&廂門  SH鍍鈦(遠東特殊色)","B-750kg ","台",198100,177500,20600,0.11605633802816902]
[null,"4B0130","B","30.43.44.45","車廂側板&廂門  SH鍍鈦(遠東特殊色)","B-1000kg ","台",212500,190400,22100,0.11607142857142858]
[null,"4B0200","B","30.43.44.45","車廂側板&廂門  SE","B-750kg~1000kg","台",62800,60300,2500,4.1459369817578771E-2,"1.SH素材為國內(唐榮)板材於國內加工蝕刻\n2.前&OPB側,CPI維持SH,不作蝕刻處理\n3.OPB型式: OPY-HD2 (SH or SH鍍鈦)"]
[null,"4B0210","B","30.43.44.45","車廂側板&廂門  SE鍍鈦(金色)","B-750kg~1000kg","台",112300,109600,2700,2.4635036496350366E-2]
[null,"4B0220","B","30.43.44.45","車廂側板&廂門  SE鍍鈦(遠東特殊色)","B-750kg ","台",184200,182000,2200,1.2087912087912088E-2]
[null,"4B0230","B","30.43.44.45","車廂側板&廂門  SE鍍鈦(遠東特殊色)","B-1000kg ","台",199400,197000,2400,1.2182741116751269E-2]
[null,"4B0300","B","30.43.44.45","車廂側板&廂門  SM","B-750kg~1000kg(R.T PANEL)","台",72800,68800,4000,5.8139534883720929E-2,"1.SM素材為(日新)板材於國內加工\n2.OPB側板為RETURN PANEL\n3.按鈕: 橢圓形按鈕(橘光)"]
[null,"4B0310","B","30.43.44.45","車廂側板&廂門  SM鍍鈦(金色)","B-750kg~1000kg(R.T PANEL)","台",155300,129200,26100,0.20201238390092879]
[null,"4B0320","B","30.43.44.45","車廂側板&廂門  SM鍍鈦(遠東特殊色)","B-750kg (R.T PANEL)","台",229200,205900,23300,0.1131617289946576]
[null,"4B0330","B","30.43.44.45","車廂側板&廂門  SM鍍鈦(遠東特殊色)","B-1000kg (R.T PANEL)","台",255800,229800,26000,0.11314186248912098]
[null,"4B0400","B","30.43.44.45","車廂側板&廂門  SM-E","B-750kg~1000kg(R.T PANEL)","台",86500,83700,2800,3.3452807646356032E-2,"1.SM素材為(日新)板材於國內加工蝕刻\n2.OPB側板為RETURN PANEL\n3.前&OPB側,CPI維持SM,不作蝕刻處理\n4.按鈕: 橢圓形按鈕(橘光)"]
[null,"4B0410","B","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(金色)","B-750kg~1000kg(R.T PANEL)","台",132600,129900,2700,2.0785219399538105E-2]
[null,"4B0420","B","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(遠東特殊色)","B-750kg (R.T PANEL)","台",202500,200400,2100,1.0479041916167664E-2]
[null,"4B0430","B","30.43.44.45","車廂側板&廂門  SM-E鍍鈦(遠東特殊色)","B-1000kg (R.T PANEL)","台",222300,219600,2700,1.2295081967213115E-2]
[]
[null,"Y00600","P",44.45,"車廂側板分割特殊","如內法特殊則不再加計","台",6800,6800,{"$f":"H501-I501","v":0},0]
[null,"Y00700","P",44.45,"側板單片特殊(CE→SH或SH-E)","CE→SH或SH-E","片",6500,4400,2100,0.47727272727272729]
[null,"Y00800","P",44.45,"側板單片特殊(CE→SM或SM-E)","CE→SM或SM-E","片",8200,5500,2700,0.49090909090909091]
[null,"Y00900","P",44.45,"側板單片特殊(CE→SH或SHE鍍鈦(金色))","CE→SH鍍鈦或SHE鍍鈦(金色)","片",9500,9300,200,2.1505376344086023E-2]
[null,"Y01000","P",44.45,"側板單片特殊(CE→SM或SME鍍鈦(金色))","CE→SM鍍鈦或SME鍍鈦(金色)","片",10900,10400,500,4.807692307692308E-2]
[null,"Y01300","P",44.45,"側板單片特殊(CE→SH(遠東特殊色))","CE→SH(遠東特殊色)","片",19100,15700,3400,{"$f":"IF(I506>0,(H506-I506)/I506,-(H506-I506)/I506)","v":0.21656050955414013}]
[null,"Y01400","P",44.45,"側板單片特殊(CE→SH-E(遠東特殊色))","CE→SH-E(遠東特殊色)","片",27300,24100,3200,{"$f":"IF(I507>0,(H507-I507)/I507,-(H507-I507)/I507)","v":0.13278008298755187}]
[null,"Y01500","P",44.45,"側板單片特殊(CE→SM(遠東特殊色))","CE→SM(遠東特殊色)","片",20500,17300,3200,{"$f":"IF(I508>0,(H508-I508)/I508,-(H508-I508)/I508)","v":0.18497109826589594}]
[null,"Y01600","P",44.45,"側板單片特殊(CE→SM-E(遠東特殊色))","CE→SM-E(遠東特殊色)","片",30000,26900,3100,{"$f":"IF(I509>0,(H509-I509)/I509,-(H509-I509)/I509)","v":0.11524163568773234}]
[]
[null,"4C9000","P",50,"後側中間片附飾條(鏡面,化粧)",null,"台",2000,1900,{"$f":"H511-I511","v":100},{"$f":"IF(I511>0,(H511-I511)/I511,-(H511-I511)/I511)","v":5.2631578947368418E-2},"標準不取付鏡面飾條"]
[]
[null,"4C4150","P",284,"車廂預留裝潢重量",null,"KG",70,40,{"$f":"H513-I513","v":30},0.75,"WT增加"]
[]
[null,"Y02400","P.B.F",52,"凸面鏡","千鳥,展望有殘障時加計","面",1600,1600,{"$f":"H515-I515","v":0},0]
[null,"E00600","P.B.F",52,"台製半身明鏡　　　　　　　　　　",null,"面",4500,4500,0,0]
[null,"E00800","P.B.F",52,"明鏡附SH鏡框　　　　　　　　　　　　　",null,"台",8200,8200,0,0]
[null,"E00900","P.B.F",52,"中間片全身明鏡　　　",null,"面",4500,4500,0,0]
[null,"E01600","P.B.F",52,"半(全)身茶鏡　　　　　　　　　　",null,"面",6000,6000,0,{"$f":"IF(I519>0,(H519-I519)/I519,-(H519-I519)/I519)","v":0},"參考BQ-E6783"]
[null,"E01700","P.B.F",52,"半(全)身灰鏡　　　　　　　　　　",null,"面",7100,7100,0,{"$f":"IF(I520>0,(H520-I520)/I520,-(H520-I520)/I520)","v":0},"參考BQ-E6783"]
[]
[null,"4C8000","P",53.55,"扁平扶手 65mm (HR-1)","P6~P24人","支",2300,2300,{"$f":"H522-I522","v":0},0]
[null,"4C8050","P",53.55,"扁平扶手 80mm (HR-2)","P6~P24人","側",5000,4900,100,2.0408163265306121E-2,"B型用扶手,  標準: 2支/側(上.下各一支)"]
[null,"4C8100","P",53.55,"扁平扶手 150mm (HR-3)","P6~P24人","支",4400,4400,0,0,"F型用扶手,  標準: 1支/側"]
[null,"4C8381","P",53.55,"不銹鋼嵌胡桃木扶手38ψ(NR-108)","P6~P24人","支",5200,5200,{"$f":"H525-I525","v":0},{"$f":"IF(I525>0,(H525-I525)/I525,-(H525-I525)/I525)","v":0}]
[null,"4C8382","P",53.55,"不銹鋼嵌栓木扶手38ψ(NR-112)","P6~P24人","支",5200,5200,{"$f":"H526-I526","v":0},{"$f":"IF(I526>0,(H526-I526)/I526,-(H526-I526)/I526)","v":0}]
[null,"4C8383","P",53.55,"不銹鋼扶手38ψ(NR-113)","P6~P24人","支",3800,3700,{"$f":"H527-I527","v":100},{"$f":"IF(I527>0,(H527-I527)/I527,-(H527-I527)/I527)","v":2.7027027027027029E-2}]
[null,"4C8384","P",53.55,"不銹鋼嵌真皮扶手38ψ(NR-125)","P6~P24人","支",7900,7900,{"$f":"H528-I528","v":0},{"$f":"IF(I528>0,(H528-I528)/I528,-(H528-I528)/I528)","v":0}]
[null,"4C8385","P",53.55,"不銹鋼圓形扶手38ψ(NR-6)","P6~P24人","支",4700,4700,{"$f":"H529-I529","v":0},{"$f":"IF(I529>0,(H529-I529)/I529,-(H529-I529)/I529)","v":0}]
[null,"4C8400","P",53.55,"扶手鍍鈦(金黃色)","僅鍍鈦加工費","支",1000,1000,0,0,"僅扶手鍍鈦加工費.(扶手依型式.另計)"]
[null,"4C8450","P",53.55,"扶手鍍鈦(遠東特殊色)","僅鍍鈦加工費","支",1400,1400,0,0,"[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C8500","P",53.55,"扶手追加抗菌塗料加工費","僅NR-108,NR-112木質可配合","支",2500,2500,{"$f":"H532-I532","v":0},{"$f":"IF(I532>0,(H532-I532)/I532,-(H532-I532)/I532)","v":0},"僅木質扶手可配合"]
[null,"4F3200","F",53.55,"扁平扶手 150mm (HR-3)","F-1000kg~2000kg","支",15100,12600,2500,0.1984126984126984,"1.F型用扶手,  標準: 1支/側"]
[null,"4F3300","F",53.55,"扁平扶手 150mm (HR-3)","F-2500kg~3000kg","支",21100,16800,{"$f":"H534-I534","v":4300},0.25595238095238093,"1.F型用扶手,  標準: 1支/側"]
[]
[null,"4C2400","P",43,"車廂前側 RT PANEL(SH)","P6~24人(不含廂門)","台",8300,6500,{"$f":"H536-I536","v":1800},0.27692307692307694,"1.SH or SH鍍鈦素材,為(唐榮)板材於國內加工鍍鈦\n2.SM or SM鍍鈦素材,為(日新)板材於國內加工鍍鈦\n3.車廂OPB側,改為 RT PANEL.\n4.按鈕: 橢圓形按鈕(橘光), 按鈕鍍鈦另加計\n5.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"4C2200","P",43,"車廂前側 RT PANEL(SH鍍鈦金色)","P6~24人(不含廂門)","台",19500,16900,2600,0.15384615384615385]
[null,"4C2220","P",43,"車廂前側 RT PANEL(SH鍍鈦遠東特殊色)","P6~24人(不含廂門)","台",30100,27700,2400,8.6642599277978335E-2]
[null,"4C2250","P",43,"車廂前側 RT PANEL(SM)","P6~24人(不含廂門)","台",14500,12000,2500,0.20833333333333334]
[null,"4C2300","P",43,"車廂前側 RT PANEL(SM鍍鈦金色)","P6~24人(不含廂門)","台",26000,22900,3100,0.13537117903930132]
[null,"4C2350","P",43,"車廂前側 RT PANEL(SM鍍鈦遠東特殊色)","P6~24人(不含廂門)","台",39300,36100,3200,8.8642659279778394E-2]
[null,"4C2170","P",43,"OPB(前)側&CPI (KF-D) CE→SH","P6~24人(不含廂門)","台",10500,6400,4100,0.640625]
[null,"4C2180","P",43,"OPB(前)側&CPI CE→IP(仿鍍鈦漆)","P6~24人(不含廂門)","台",4200,4100,{"$f":"H543-I543","v":100},{"$f":"IF(I543>0,(H543-I543)/I543,-(H543-I543)/I543)","v":2.4390243902439025E-2},"仿古咖色, 仿黑色, 仿古銅色, 仿金色."]
[null,"8C2000","P.B",56.57,"YE-HD  SH ","≦12FL","台",9300,9700,-400,-4.1237113402061855E-2,"1.僅YE-HD OPB本體. 2.面板: 2T(直角立體型)\n3.方型按鈕: EJ-ICA(紅光)(TOUCH式)\n4.殘障用: 不可行"]
[null,"8C2100","P.B",56.57,"YE-HD  SH ","13~16FL","台",11700,12000,-300,-2.5000000000000001E-2]
[null,"8C2200","P.B",56.57,"YE-HD  SH ","17FL(含)以上","台",15400,15700,-300,-1.9108280254777069E-2]
[null,"8C0600","P",56,"OPB顯示器採LCD(KF-L1)",null,"台",8300,7900,400,5.0632911392405063E-2]
[null,"8C0610","P",56,"OPB顯示器採LCD(OPY-HD2)","7.0\"全彩LCD螢幕","台",5800,6100,{"$f":"H548-I548","v":-300},-4.9180327868852458E-2]
[null,"8C0550","P",56,"KF-D SM面板鍍鈦(遠東特殊色)","非RETURN PANEL","台",4200,4200,{"$f":"H549-I549","v":0},{"$f":"IF(I549>0,(H549-I549)/I549,-(H549-I549)/I549)","v":0}]
[null,"7C9200","P",56.57,"LCD預留(追加網路訊號轉換器)","不含LCD螢幕及開孔","台",23400,23200,200,8.6206896551724137E-3,"同時有CCTV,刷卡機預留,多媒體影音需加計"]
[null,"8C5000","P",56.57,"車廂側板預留LCD螢幕開孔",null,"台",4500,4200,{"$f":"H551-I551","v":300},7.1428571428571425E-2,"外法特殊對應(請另加計內法特殊費用)"]
[null,"8C6000","P",56.57,"多媒體視訊系統 OPY-M4 (群)","側板預留LCD螢幕嵌入式","群",78500,78500,0,0,"含PC主機.19\"LCD螢幕&DVD PLAY"]
[null,"8C6100","P",56.57,"多媒體視訊系統 OPY-M4 (台)","側板預留LCD螢幕嵌入式","台",155300,154800,500,3.2299741602067182E-3,"螢幕:可動態DVD播放. 含同軸電纜以60m計"]
[null,"8C6200","P",56.57,"多媒體視訊系統 OPY-M5 (台)","側板預留LCD螢幕嵌入式","台",69800,69300,500,7.215007215007215E-3,"螢幕:僅靜態圖片播放."]
[null,"7C9420","P.B",87,"車廂內聲控(語音)叫車",null,"台",9100,8900,{"$f":"H555-I555","v":200},{"$f":"IF(I555>0,(H555-I555)/I555,-(H555-I555)/I555)","v":2.247191011235955E-2},"廠商:獨步新媒體"]
[null,"8C6300","P.B",208,"車廂內OPB非接觸按鈕","≦16FL","台",5600,5500,{"$f":"H556-I556","v":100},{"$f":"IF(I556>0,(H556-I556)/I556,-(H556-I556)/I556)","v":1.8181818181818181E-2}]
[null,"8C6350","P.B",208,"車廂內OPB非接觸按鈕","17FL(含)以上","台",11000,10900,{"$f":"H557-I557","v":100},{"$f":"IF(I557>0,(H557-I557)/I557,-(H557-I557)/I557)","v":9.1743119266055051E-3}]
[null,"Y26600","P.B",56.57,"二維條碼叫車",null,"台",10900,10900,{"$f":"H558-I558","v":0},{"$f":"IF(I558>0,(H558-I558)/I558,-(H558-I558)/I558)","v":0},"廠商:茂旭"]
[]
[null,"9C0100","P.B",60.61,"DIG-C2面板 SH鍍鈦(金色)","橢圓形按鈕: H3525TL(橘光)","停",500,500,{"$f":"H560-I560","v":0},0,"面板: 1.2T (30°立體型)(插入式), 按鈕鍍鈦另計"]
[null,"9C0150","P.B",60.61,"DIG-C2面板 SH鍍鈦(遠東特殊色)","橢圓形按鈕: H3525TL(橘光)","停",800,700,100,0.14285714285714285,"面板: 1.2T (30°立體型)(插入式), 按鈕鍍鈦另計"]
[null,"9C0200","P.B",60.61,"DIG-C2面板 SM","橢圓形按鈕: H3525TL(橘光)","停",300,300,0,0,"面板: 1.2T (30°立體型)(插入式)"]
[null,"9C0300","P.B",60.61,"DIG-C2面板 SM鍍鈦(金色)","橢圓形按鈕: H3525TL(橘光)","停",800,700,100,0.14285714285714285,"面板: 1.2T (30°立體型)(插入式), 按鈕鍍鈦另計"]
[null,"9C0350","P.B",60.61,"DIG-C2面板 SM鍍鈦(遠東特殊色)","橢圓形按鈕: H3525TL(橘光)","停",1000,1000,0,0,"面板: 1.2T (30°立體型)(插入式), 按鈕鍍鈦另計"]
[null,"9C0500","P.B",60.61,"按鈕 追加鍍鈦(金色)","橢圓形按鈕: H3525TL(橘光)","停",400,400,0,0,"1.僅按鈕追加鍍鈦加工"]
[null,"9C0600","P.B",60.61,"按鈕 追加鍍鈦(遠東特殊色)","橢圓形按鈕: H3525TL(橘光)","停",600,600,0,0]
[null,"9C0700","P.B",60.61,"DIG-C2面板  亂紋板","橢圓形按鈕: H3525TL(橘光)","停",500,400,100,0.25,"1.面板: 1.5T (30°立體型)(插入式)\n2.按鈕: 鍍鈦費用另計"]
[null,"9C0710","P.B",60.61,"DIG-C2面板  亂紋鍍鈦(金色)","橢圓形按鈕: H3525TL(橘光)","停",1000,900,100,0.1111111111111111]
[null,"9C0720","P.B",60.61,"DIG-C2面板  亂紋鍍鈦(遠東特殊色)","橢圓形按鈕: H3525TL(橘光)","停",1300,1200,100,8.3333333333333329E-2]
[null,"9C0800","P.B",60.61,"DIG-C2面板  霧珠板","橢圓形按鈕: H3525TL(橘光)","停",500,500,0,0,"1.面板: 1.5T (30°立體型)(插入式)\n2.按鈕: 鍍鈦費用另計"]
[null,"9C0810","P.B",60.61,"DIG-C2面板  霧珠鍍鈦(金色)","橢圓形按鈕: H3525TL(橘光)","停",1000,900,100,0.1111111111111111]
[null,"9C0820","P.B",60.61,"DIG-C2面板  霧珠鍍鈦(遠東特殊色)","橢圓形按鈕: H3525TL(橘光)","停",1300,1200,100,8.3333333333333329E-2]
[null,"9C1000","P.B",60.61,"DIG-CE  SH","方型Touch Button(紅光)","停",2400,2200,200,9.0909090909090912E-2,"面板: 2T (平板型)(插入式)"]
[null,"9C0360","P",60.61,"DIG-C2面板  IP(仿鍍鈦烤漆)","DIG-C2","停",300,300,{"$f":"H574-I574","v":0},0,"仿古咖色, 仿黑色, 仿古銅色, 仿金色."]
[null,"9C1400","P.B",60.61,"DIG-C2顯示器→3.5\"全彩LCD",null,"停",2400,2300,{"$f":"H575-I575","v":100},{"$f":"IF(I575>0,(H575-I575)/I575,-(H575-I575)/I575)","v":4.3478260869565216E-2}]
[null,"9C8000","P.B",60.61,"FOX IND→DIG-C2",null,"停",700,700,{"$f":"H576-I576","v":0},0]
[null,"9C8010","P.B",60.61,"FOX IND面板 SH鍍鈦(金色)","※僅面板,FOX按鈕無法鍍鈦","停",800,700,100,0.14285714285714285]
[null,"9C8020","P.B",60.61,"FOX IND面板 SH鍍鈦(遠東特殊色)","※僅面板,FOX按鈕無法鍍鈦","停",1000,1000,0,0]
[null,"9C8030","P.B",60.61,"FOX IND面板 SM","※僅面板,FOX按鈕無鏡面","停",700,600,100,0.16666666666666666]
[null,"9C8040","P.B",60.61,"FOX IND面板 SM鍍鈦(金色)","※僅面板,FOX按鈕無法鍍鈦","停",1100,1000,100,0.1]
[null,"9C8050","P.B",60.61,"FOX IND面板 SM鍍鈦(遠東特殊色)","※僅面板,FOX按鈕無法鍍鈦","停",1400,1300,100,7.6923076923076927E-2]
[null,"9C8090","P.B",60.61,"FOX IND(LED)→FOX IND(LCD)",null,"停",2000,2000,0,0]
[null,"Y03200","P.F.B",60.61,"IND 圓形面板",null,"停",1200,1200,0,0]
[null,"Y03300","P",60.61,"IND面板加長(同殘障用尺寸)",null,"停",400,400,0,0]
[null,"8C6400","P.B",208,"乘場側IND非接觸按鈕",null,"停",2000,2000,0,0]
[null,"9C8500","P.B",207,"乘場側手勢呼梯",null,"停",2000,2000,0,0]
[null,"7C9440","P.B",60.61,"目的階叫車 (群)","Max: 64組/群","群",178000,174300,3700,2.1227768215720023E-2]
[null,"7C9450","P.B",60.61,"目的階叫車 (停)","選層器取付","停",34100,34100,0,0]
[null,"7C9480","P.B",60.61,"手機叫車 (台)",null,"台",24800,24500,300,1.2244897959183673E-2]
[null,"7C9490","P.B",60.61,"手機叫車 (停)",null,"停",2000,2000,0,0]
[]
[null,"Y24800","P.B.F",63,"屏東楓港村(枋山鄉),車城鄉安裝差旅費",null,"台",20000,20000,{"$f":"H592-I592","v":0},0,"2018年4月份出貨協調會決議"]
[null,"F03300","P.B.F",63,"羅東,宜蘭,礁溪,墾丁,恆春安裝差旅費",null,"台",27000,27000,{"$f":"H593-I593","v":0},{"$f":"IF(I593>0,(H593-I593)/I593,-(H593-I593)/I593)","v":0}]
[null,"F03400","P.B.F",63,"花蓮,台東安裝差旅費+工廠運費及工事鐵籠箱回廠運費",null,"台",74900,74900,0,0,"2021年12月出貨協調會決議,增加工事鐵籠箱回廠運費"]
[null,"F03500","P.B.F",63,"金門,馬祖,澎湖安裝差旅費",null,"台",59600,59600,0,0]
[null,"Y24200","P",63,"安裝地:金門(全部費用)","含(530)保養交通及住宿費用*12個月","台",232200,230300,1900,{"$f":"IF(I596>0,(H596-I596)/I596,-(H596-I596)/I596)","v":8.250108554059922E-3},"金門及澎湖計入(530)保養交通及住宿費用*12個月,\n馬祖台數多,(530)可吸收(2018年4月份出貨協調會決議)\n含PCB凡立水處理,安裝差旅費\n離島捆包費(含工務裝箱),船運費及當地運費."]
[null,"Y24900","P",63,"安裝地:澎湖(全部費用)",null,"台",305400,303500,{"$f":"H597-I597","v":1900},{"$f":"IF(I597>0,(H597-I597)/I597,-(H597-I597)/I597)","v":6.2602965403624382E-3}]
[null,"Y24300","P",63,"安裝地:馬祖(全部費用)","船運費及當地運費BY永大","台",212100,210200,1900,{"$f":"IF(I598>0,(H598-I598)/I598,-(H598-I598)/I598)","v":9.0390104662226457E-3}]
[null,"Y24400","P",63,"安裝地:馬祖(船運費及當地運費不含)","船運費及當地運費BY業主","台",164300,162400,1900,{"$f":"IF(I599>0,(H599-I599)/I599,-(H599-I599)/I599)","v":1.1699507389162561E-2},"船運費及當地運費BY業主"]
[null,"0C9300","P",63,"離島地區(頂樓追加S.ANN KEY)","僅VAG機種適用","台",7000,7000,{"$f":"H600-I600","v":0},{"$f":"IF(I600>0,(H600-I600)/I600,-(H600-I600)/I600)","v":0},"UAY3屬控盤內移,可查看/清除TCD碼,以利維修保養."]
[]
[null,"3C5400","P",66,"後側展望 (含CWT側落式*10停)","P8~P9人(含鋼絲玻璃) ","台",164500,158000,{"$f":"H602-I602","v":6500},4.1139240506329111E-2,"(含立組工時)"]
[null,"3C5500","P",66,"後側展望 (含CWT側落式*10停)","P10~11人(含鋼絲玻璃) ","台",199800,194900,4900,2.5141097998973832E-2,"含RAIL:T-8K*T-5K→T-13K*T-8K(含立組工時)"]
[null,"3C5600","P",66,"後側展望 (含CWT側落式*10停)","P12~P15(含鋼絲玻璃)","台",174900,168800,6100,3.6137440758293837E-2,"含CWT RAIL:T-5K→T-8K(含立組工時)"]
[null,"3C5650","P",66,"後側展望 (含CWT側落式*10停)","P17~P24(含鋼絲玻璃)","台",164500,158000,6500,4.1139240506329111E-2]
[null,"3C6060","P",158,"展望梯採開放式昇降道",null,"樓",19400,19100,300,1.5706806282722512E-2,"1.開放式升降道等相關部品遮羞費用\n2.含升降道配線槽整理及蛇護管費用\n3.含作業基準器具塗裝費用"]
[null,"Y02300","P",66,"升降道塗裝粉刷",null,"台",16000,16000,0,0,"粉刷、油漆、帷幕玻璃安裝(以實際配合日計)"]
[]
[null,"Y20100","P",68.69,"按鈕 (H3525HW-O-MRSV)","(宏匠)(A1)(鏡面本色)","只",70,70,{"$f":"H609-I609","v":0},0,"使用數量:\n 1.車廂主OPB按鈕數量:(N+4)/組  (N:停數)\n   (停數+開+關+對講機按鈕+開延長)\n    殘障OPB按鈕數量:(N+3)/組  (N:停數)\n   (停數+開+關+對講機按鈕)\n 2.乘場IND按鈕數量:(2N-2)/台  (N:停數)\n    殘障IND按鈕數量:(2N-2)/台  (N:停數)\n"]
[null,"Y20200","P",68.69,"按鈕 (H3525-HY-O-MRSV)","(宏匠)(B1)(鏡面本色)","只",70,70,0,0]
[null,"Y20300","P",68.69,"按鈕 (H3525HR-O-MRSV)","(宏匠)(C1)(鏡面本色)","只",70,70,0,0]
[null,"Y20400","P",68.69,"按鈕 (H3525HW-O-MRBZ-MBZ)","(宏匠)(D1)(鏡面古銅)","只",200,200,0,0]
[null,"Y20500","P",68.69,"按鈕 (H3525HW-O-MRTB-MTB)","(宏匠)(E1)(鏡面鈦黑)","只",200,200,0,0]
[null,"Y20600","P",68.69,"按鈕 (H3525HW-O-MRTG-MTG)","(宏匠)(F1)(鏡面鈦金)","只",200,200,0,0]
[null,"Y20700","P",68.69,"按鈕 (D3025PKC-G-HLSV)","(宏匠)(A2)(髮絲本色)","只",140,140,0,0]
[null,"Y20800","P",68.69,"按鈕 (D3225PHWB-B-HLTB-HTB)","(宏匠)(B2)(髮絲本色)","只",200,200,0,0]
[null,"Y20900","P",68.69,"按鈕 (D3425PHWB-W-VBBZ-HBZ)","(宏匠)(C2)(亂紋本色)","只",270,270,0,0]
[null,"Y21000","P",68.69,"按鈕 (D3625PHKA-R-DPSV-HSV)","(宏匠)(D2)(霧珠本色)","只",200,200,0,0]
[null,"Y21100","P",68.69,"按鈕 (D3925HWB-O-HLBZ-HBZ)","(宏匠)(E2)(髮絲本色)","只",340,340,0,0]
[null,"Y21200","P",68.69,"按鈕 (D4525WB-BU-MRTG-HTG)","(宏匠)(F2)(鏡面本色)","只",410,410,0,0]
[null,"Y21300","P",68.69,"按鈕 (SQ3328HKB-G-HLSV)","(宏匠)(A3)(髮絲本色)","只",340,340,0,0]
[null,"Y21400","P",68.69,"按鈕 (SQ3328HWB-B-HLTB)","(宏匠)(B3)(髮絲鈦黑)","只",480,480,0,0]
[null,"Y21500","P",68.69,"按鈕 (SQ3328HWB-W-MRBZ)","(宏匠)(C3)(鏡面古銅)","只",610,610,0,0]
[null,"Y21600","P",68.69,"按鈕 (SQ3428HKB-R-DPSV)","(宏匠)(D3)(霧珠本色)","只",410,410,0,0]
[null,"Y21700","P",68.69,"按鈕 (SQ3428WB-O-MRSV)","(宏匠)(E3)(鏡面本色)","只",340,340,0,0]
[null,"Y21800","P",68.69,"按鈕 (SQ3428HWB-BU-DPTG)","(宏匠)(F3)(霧珠本色)","只",550,550,0,0]
[null,"Y21900","P",68.69,"按鈕 (D4025A-G-HHSV-MSV)","(宏匠)(A4)(髮絲本色)","只",410,410,0,0]
[null,"Y22000","P",68.69,"按鈕 (D4025C-B-MHTB-MTB)","(宏匠)(B4)(鏡面本色)","只",340,340,0,0]
[null,"Y22100","P",68.69,"按鈕 (D4033HWB-W-DPTG-HTG)","(宏匠)(C4)(霧珠本色)","只",410,410,0,0]
[null,"Y22200","P",68.69,"按鈕 (D4033LKB-R-DPSV-HSV)","(宏匠)(D4)(霧珠本色)","只",410,410,0,0]
[null,"Y22300","P",68.69,"按鈕 (D4533HWB-O-MRTB-HTB)","(宏匠)(E4)(鏡面本色)","只",410,410,{"$f":"H631-I631","v":0},0]
[null,"Y22400","P",68.69,"按鈕 (D5033HWB-BU-MRSV-HSV)","(宏匠)(F4)(鏡面本色)","只",480,480,{"$f":"H632-I632","v":0},0]
[null,"Y22900","P",68.69,"按鈕(D3925HWBL08-O-HLBZ-HBZ)","(E2)可鎖附牆面(髮絲古銅)","只",1100,1100,{"$f":"H633-I633","v":0},0]
[null,"Y23000","P",68.69,"按鈕(D4525WBL08-BU-MRTG-HTG)","(F2)可鎖附牆面(鏡面鈦黑)","只",1100,1100,{"$f":"H634-I634","v":0},0]
[null,"Y23100","P",68.69,"按鈕(D4533HWBL07-O-MRTB-HTB)","(E4)可鎖附牆面(鏡面鈦黑)","只",1200,1200,0,0]
[null,"Y23200","P",68.69,"按鈕(D5033HWBL07-BU-MRSV-HSV)","(F4)可鎖附牆面(鏡面鈦黑)","只",1000,1000,0,0]
[]
[null,"9C2000","P.B.F","60.68.73","HF(VF)-LM5+BL-C2(SH)","橢圓形按鈕: H3525TL(橘光)","停",2300,2200,{"$f":"H638-I638","v":100},4.5454545454545456E-2,"顯示器2T(導角平板),按鈕1.2T(30°立體型)"]
[null,"9C2200","P.B.F","60.68.73","HF(VF)-LM5+DIG-C2(SH)","橢圓形按鈕: H3525TL(橘光)","停",4100,4000,100,2.5000000000000001E-2,"顯示器2T(導角平板),按鈕1.2T(30°立體型)"]
[null,"9C2410","P.B.F","60.68.73","顯示器面板  追加鍍鈦(金色)","HF(VF)-LM5 or L-50","停",900,900,{"$f":"H640-I640","v":0},0]
[null,"9C2420","P.B.F","60.68.73","顯示器面板  追加鍍鈦(遠東特殊色)","HF(VF)-LM5 or L-50","停",1500,1500,{"$f":"H641-I641","v":0},0]
[null,"9C4000","P.B.F","60.68.73","HALL-LANT(台)",null,"台",5200,5000,200,0.04]
[null,"9C4010","P.B.F","60.68.73","HALL-LANT接點預留(停)\n(廳燈BY業主)","廳燈by(業主)","停",2500,2500,{"$f":"H643-I643","v":0},0,"[業主]:使用電壓AC 110V 20W或DC 22V 1.5W\n電源提供by(永大) → 由PANEL上取付"]
[null,"9C4300","P.B.F","60.68.73","L-50H+BL-C2  (SH)","變更為LED燈","停",4800,4600,200,4.3478260869565216E-2,"顯示器3T(導角平板),按鈕1.2T(30°立體型)"]
[null,"9C4500","P.B.F","60.68.73","L-50H+DIG-C2  (SH)","變更為LED燈","停",4800,4700,100,2.1276595744680851E-2,"顯示器3T(導角平板),按鈕1.2T(30°立體型)"]
[null,"9C4700","P.B.F","60.68.73","L-51H+BL-C2  (SH)","變更為LED燈","停",10200,10500,-300,-2.8571428571428571E-2,"顯示器(圓筒無面板),按鈕1.2T(30°立體型)"]
[null,"9C4900","P.B.F","60.68.73","L-51H+DIG-C2  (SH)","變更為LED燈","停",10200,10600,-400,-3.7735849056603772E-2,"顯示器(圓筒無面板),按鈕1.2T(30°立體型)"]
[null,"9C5100","P.B.F","60.68.73","L-52H+BL-C2  (SH)","變更為LED燈","停",4900,4800,100,2.0833333333333332E-2,"顯示器(圓筒無面板),按鈕1.2T(30°立體型)"]
[null,"9C5300","P.B.F","60.68.73","L-52H+DIG-C2  (SH)","變更為LED燈","停",5100,5100,0,0,"顯示器(圓筒無面板),按鈕1.2T(30°立體型)"]
[null,"9C6800","P.B.F","60.68.73","L-61+BL-C2  (SM)",null,"停",7800,7700,100,1.2987012987012988E-2,"面板: 鏡面3T(壓克力 35W×350H), 按鈕1.5T(30°立體型)"]
[null,"9C7000","P.B.F","60.68.73","L-61+DIG-C2  (SM)",null,"停",8000,7900,100,{"$f":"IF(I651>0,(H651-I651)/I651,-(H651-I651)/I651)","v":1.2658227848101266E-2},"面板: 鏡面3T(壓克力 35W×350H), 按鈕1.5T(30°立體型)"]
[null,"9C7200","P.B.F","60.68.73","L-63+BL-C2  (SM)",null,"停",7800,7700,100,1.2987012987012988E-2]
[null,"9C7400","P.B.F","60.68.73","L-63+DIG-C2  (SM)",null,"停",8000,7900,100,1.2658227848101266E-2]
[null,"9C8200","P.B.F","60.68.73","L-50H(SH)+FOX IND(SH)",null,"停",5000,4800,200,4.1666666666666664E-2]
[null,"9C8250","P.B.F","60.68.73","L-51H(無面板)+FOX IND(SH)",null,"停",10400,10700,-300,-2.8037383177570093E-2]
[null,"9C8300","P.B.F","60.68.73","L-52H(無面板)+FOX IND(SH)",null,"停",4700,4700,0,0]
[null,"9C8350","P.B.F","60.68.73","L-61(SM)+FOX IND(SM)","※僅面板,FOX按鈕無鏡面","停",8100,8000,100,1.2500000000000001E-2]
[null,"9C8450","P.B.F","60.68.73","L-63(SM)+FOX IND(SM)","※僅面板,FOX按鈕無鏡面","停",7900,7800,100,1.282051282051282E-2]
[null,"9C8400","P.B.F","60.68.73","L-62(亂紋)+BL-C2  (SH)",null,"停",5400,5300,{"$f":"H659-I659","v":100},{"$f":"IF(I659>0,(H659-I659)/I659,-(H659-I659)/I659)","v":1.8867924528301886E-2}]
[]
[null,"7C1400","P",79,"專用運轉",null,"台",1200,1100,{"$f":"H661-I661","v":100},{"$f":"IF(I661>0,(H661-I661)/I661,-(H661-I661)/I661)","v":9.0909090909090912E-2}]
[null,"7C1300","P",79,"ATT功能",null,"台",3900,3000,{"$f":"H662-I662","v":900},0.3,"操作開關取付於OPB SW BOX內"]
[]
[null,"7C5000","P.B.F",80,"車廂追加到樓鈴","到樓鈴: 電子CHIME","台",2400,2300,{"$f":"H664-I664","v":100},4.3478260869565216E-2,"電子音發聲,取付於C.J BOX內"]
[null,"9C4100","P.B.F",80,"乘場追加到樓鈴","到樓鈴: 電子CHIME","停",1200,1100,{"$f":"H665-I665","v":100},9.0909090909090912E-2,"電子音發聲,取付於POCKET內"]
[]
[null,"2C2800","P.B.F",81,"紅外線光幕+內縮型機械SHOE","千鳥型需加計2次","台",15000,15300,{"$f":"H667-I667","v":-300},-1.9607843137254902E-2,"光幕: 採CEDES光幕"]
[]
[null,"7C1000","P.B",82,"火警受信",null,"台",2600,2500,{"$f":"H669-I669","v":100},0.04]
[null,"7C1100","P.B",82,"火災管制",null,"台",4300,4100,{"$f":"H670-I670","v":200},4.878048780487805E-2]
[null,"7C1200","P.B",82,"緊急用",null,"台",16400,15300,{"$f":"H671-I671","v":1100},7.1895424836601302E-2]
[]
[null,"4C7900","P",162,"車廂側板附壁鉤","P6~P24人","台",8900,8700,{"$f":"H673-I673","v":200},2.2988505747126436E-2,"取付高度:距地面2100mm(不含保護壁毯)"]
[null,"Y03600","P",162,"側板附壁鉤及保護掛毯(牛仔布)","P6~P12人","台",26700,26500,{"$f":"H674-I674","v":200},7.5471698113207548E-3,"壁毯為三側(牛仔布)"]
[null,"Y03700","P",162,"側板附壁鉤及保護掛毯(牛仔布)","P13~P20人","台",30800,30500,{"$f":"H675-I675","v":300},{"$f":"IF(I675>0,(H675-I675)/I675,-(H675-I675)/I675)","v":9.8360655737704927E-3},"壁毯為三側(牛仔布)"]
[null,"Y03800","P",162,"側板附壁鉤及保護掛毯(牛仔布)","P24人","台",34800,34600,{"$f":"H676-I676","v":200},{"$f":"IF(I676>0,(H676-I676)/I676,-(H676-I676)/I676)","v":5.7803468208092483E-3},"壁毯為三側(牛仔布)"]
[]
[null,"8C1000","P.B.F",163,"SUB OPY-HD2  (SH) ","≦12FL","台",9400,8300,{"$f":"H678-I678","v":1100},0.13253012048192772,"1.僅追加SUB OPB本體.\n2.面板: 1.5T(直角立體型)\n3.圓形按鈕: H3525(橘光)(PUSH式)"]
[null,"8C1100","P.B.F",163,"SUB OPY-HD2  (SH) ","13~16FL","台",10400,9100,{"$f":"H679-I679","v":1300},0.14285714285714285]
[null,"8C1200","P.B.F",163,"SUB OPY-HD2  (SH) ","17FL(含)以上","台",11300,10100,{"$f":"H680-I680","v":1200},0.11881188118811881]
[]
[null,"7C7500","P.B.F",176,"CCTV配線預留","5C FV線材(標準)","台",13400,13400,{"$f":"H682-I682","v":0},{"$f":"IF(I682>0,(H682-I682)/I682,-(H682-I682)/I682)","v":0},"標準長度:預留予CPI FRAME上. L=80m計"]
[null,"7C7600","P.B.F",176,"CCTV配線預留(台)(12FL計)","12芯同軸電纜","台",34200,34100,{"$f":"H683-I683","v":100},2.9325513196480938E-3]
[null,"7C7650","P.B.F",176,"CCTV配線預留(停)","12芯同軸電纜","樓",1500,1500,{"$f":"H684-I684","v":0},0]
[]
[null,"7C5500","P.B.F",177,"追加PARKING SW","取付於基準階IND面板","台",600,500,{"$f":"H686-I686","v":100},0.2,"一般取付於[1FL] IND面板上"]
[]
[null,"8C3500","P.B",178,"殘障OPB面板  SH鍍鈦(金色)","僅面板鍍鈦費(殘障功能另計)","台",2500,2000,{"$f":"H688-I688","v":500},0.25,"1.僅殘障OPB面板鍍鈦加工費(殘障功能另計)\n2.[遠東]特殊色: 計有咖啡. 古銅. 古咖. 黑色"]
[null,"8C3600","P.B",178,"殘障OPB面板  SH鍍鈦(遠東特殊色)","僅面板鍍鈦費(殘障功能另計)","台",3500,3000,500,0.16666666666666666]
[null,"8C3700","P.B",178,"殘障OPB面板  SM鍍鈦(金色)","僅面板鍍鈦費(殘障功能另計)","台",3400,2900,500,0.17241379310344829]
[null,"8C3800","P.B",178,"殘障OPB面板  SM鍍鈦(遠東特殊色)","僅面板鍍鈦費(殘障功能另計)","台",4200,3700,500,0.13513513513513514]
[null,"7C3000","P.B",178,"殘障用 (台)(12FL(含)以下)","橢圓形按鈕:H3525TL","台",34600,33600,1000,2.976190476190476E-2,"1.含主殘障OPB(嵌入式) & 語音合成追加.\n2.含(賽福特)標準光幕, NR-113扶手*2側\n3.主OPB,IND盲人點字板(硬質PVC)追加\n4.IND面板: SH(1.2T), (30°立體型插入式)"]
[null,"7C3100","P.B",178,"殘障用 (台)(13-20FL)","橢圓形按鈕:H3525TL","台",39700,38500,1200,3.1168831168831169E-2]
[null,"7C3150","P.B",178,"殘障用 (台)(21-30FL)","橢圓形按鈕:H3525TL","台",43500,42100,1400,3.3254156769596199E-2]
[null,"7C3400","P.B",178,"殘障用 (停)2019殘障法規","殘障DIG-C2 (SH)","停",1900,1800,100,5.5555555555555552E-2]
[]
[null,"7C1500","P.B",179,"自家發管制",null,"台",3300,3300,{"$f":"H697-I697","v":0},0]
[]
[null,"7C1600","P.B",180,"地震管制運轉(單獨or同一機房NO.1)","單獨or同一機房(NO.1)","台",14400,14200,{"$f":"H699-I699","v":200},1.4084507042253521E-2,"1.單獨 (一般用or緊急用均同)\n2.同一機房共用1組地震管制器"]
[null,"7C1700","P.B",180,"地震管制運轉(同一機房其它號機)","同一機房(其它號機)","台",5700,5500,{"$f":"H700-I700","v":200},3.6363636363636362E-2]
[]
[null,"7C2000","P.B",181,"B.G.M","含SPEAKER","台",5400,5300,{"$f":"H702-I702","v":100},1.8867924528301886E-2,"OPB內不附音量調節鈕"]
[]
[null,"7C4600","P.B",182,"語音合成",null,"台",4600,4500,{"$f":"H704-I704","v":100},2.2222222222222223E-2,"標準:國台語發音(Ver2.1),特殊須另錄音加價"]
[]
[null,"F00300","P.B.F",183,"對講機配線至管理員室以100M計(不含配管)　　　　　　　　　　",null,"台",16500,15000,{"$f":"H706-I706","v":1500},0.1]
[null,"Y02800","P.B.F",183,"對講機線材100M計　　　　　　　　　　",null,"台",11200,9700,{"$f":"H707-I707","v":1500},0.15463917525773196,"永大提供線材業主自行拉線處理"]
[]
[null,"7C4700","P.B",185,"追加盲人點字板 ","硬質PVC (標準)","台",800,800,{"$f":"H709-I709","v":0},0,"標準:僅主OPB.IND貼付(殘障OPB.IND不貼付)"]
[]
[null,"F08100","P.B.F",186,"監視盤(EAS,VAG)(第壹台)(1台/組)",null,"台",27500,26700,{"$f":"H711-I711","v":800},{"$f":"IF(I711>0,(H711-I711)/I711,-(H711-I711)/I711)","v":2.9962546816479401E-2},"監視盤尺寸: 500W × 650H × 150D"]
[null,"F08200","P.B.F",186,"監視盤(EAS,VAG)(第壹台)(2台/組)",null,"台",35400,34500,900,2.6086956521739129E-2,"監視盤尺寸: 500W × 650H × 150D"]
[null,"F08300","P.B.F",186,"監視盤(EAS,VAG)(第壹台)(3台/組)",null,"台",43200,42400,800,1.8867924528301886E-2,"監視盤尺寸: 500W × 650H × 150D"]
[null,"F08400","P.B.F",186,"監視盤(EAS,VAG)(第壹台)(4台/組)",null,"台",51100,50200,900,1.7928286852589643E-2,"監視盤尺寸: 500W × 650H × 150D"]
[null,"F08500","P.B.F",186,"監視盤(EAS,VAG)(第壹台)(5台/組)",null,"台",59300,58200,1100,1.8900343642611683E-2,"監視盤尺寸: 575W × 650H × 150D"]
[null,"F08600","P.B.F",186,"監視盤(EAS,VAG)(第壹台)(6台/組)",null,"台",67400,66400,1000,1.5060240963855422E-2,"監視盤尺寸: 650W × 650H × 150D"]
[null,"F08700","P.B.F",186,"監視盤(EAS,VAG)(第壹台)(7台/組)",null,"台",75800,74600,1200,1.6085790884718499E-2,"監視盤尺寸: 575W × 800H × 150D"]
[null,"F08800","P.B.F",186,"監視盤(EAS,VAG)(第壹台)(8台/組)",null,"台",83700,82400,1300,1.5776699029126214E-2,"監視盤尺寸: 575W × 800H × 150D"]
[null,"7C2400","P.B.F",186,"監視盤(EAS,VAG)(第2台以後)",null,"台",1800,1800,{"$f":"H719-I719","v":0},0]
[null,"Y03100","P.B.F",186,"監視盤線材費100M ",null,"台",23200,21100,2100,9.9526066350710901E-2]
[null,"F00100","P.B.F",186,"監視盤配線與人工費用以100M計(不含配管)　　　",null,"台",33800,31800,2000,6.2893081761006289E-2,"(含對講機拉線至管理室費用)"]
[null,"Y07000","P.B.F",210,"協檢費用扣除(竣檢方式:不檢)",null,"台",-2000,-2000,0,0]
[null,"Y07100","P.B.F",601,"清安費用",null,"式",5000,5000,0,0]
[null,"Y07200","P.B.F",601,"工程保險",null,"式",3000,3000,0,0]
[null,"Y07300","P.B.F",601,"配合人工費(工事後續雜項配合)",null,"工",5300,5300,0,0]
[null,"Y07400","P.B.F",601,"許可證費用",null,"式",1260,1260,0,0]
[null,"Y07500","P.B.F",601,"佣金(工程備佣金)",null,"式",5000,5000,0,0]
[null,"Y07600","P.B.F",601,"捐贈費",null,"式",5000,5000,0,0]
[null,"Y07700","P.B.F",601,"廠驗費",null,"式",5000,5000,0,0]
[null,"Y07900","P.B.F",601,"其他配合費用",null,"式",5000,5000,0,0]
[null,"Y08300","P.B.F",601,"配合人工費(服務後續雜項配合)",null,"工",7400,7400,{"$f":"H731-I731","v":0},{"$f":"IF(I731>0,(H731-I731)/I731,-(H731-I731)/I731)","v":0}]
[]
[null,"7C2100","P.B",187,"ALP(15KW(含)以下)","P6~24-60m,P8~15-90,105m\nB-750~1000kg(45m,60m)","台",41300,41200,{"$f":"H733-I733","v":100},2.4271844660194173E-3,"15KW(含)以下: P6~24-CO60m, P8~15-CO90,105m\n                            B-750~1000kg(45m,60m)"]
[null,"7C2150","P",187,"ALP(15KW以上)","P17~24-90,105m, P13~17-120.150m","台",48900,48700,{"$f":"H734-I734","v":200},4.1067761806981521E-3,"15KW以上: P17~24-CO90,105m, P13~17-CO120.150m"]
[]
[null,"7C2200","P.B.F",188,"YECM (群)","僅需加計於第一台","群",116900,115500,{"$f":"H736-I736","v":1400},1.2121212121212121E-2,"含PC主機,22\"LCD螢幕,印表機(取消),UPS,\n  &TRANS(YECM) I/O BOX---等"]
[null,"7C2300","P.B.F",188,"YECM (台)","每台電梯皆需加計","台",18300,17900,400,2.23463687150838E-2]
[null,"F06200","P.B.F",188,"YECM線材100米(含拉線人工)","需搭配另計對講機拉線工程","台",27100,27100,0,0,"3C隔離線  47元/米 "]
[null,"Y25400","P.B.F",188,"YES1 (群)","僅需加計於第一台","群",201700,200700,1000,{"$f":"IF(I739>0,(H739-I739)/I739,-(H739-I739)/I739)","v":4.9825610363726956E-3}]
[null,"7C2350","P.B.F",188,"YES1 (台)","每台電梯皆需加計","台",13400,12800,600,{"$f":"IF(I740>0,(H740-I740)/I740,-(H740-I740)/I740)","v":4.6875E-2}]
[null,"Y25500","P.B.F",188,"YES1光纖100米(多模6C)(含拉線人工)","需搭配另計對講機拉線工程","台",31600,31600,0,{"$f":"IF(I741>0,(H741-I741)/I741,-(H741-I741)/I741)","v":0}]
[]
[null,"7C5200","P.B",195,"滿員自動通過不停運轉","FULL LOAD BY PASS","台",2800,2800,{"$f":"H743-I743","v":0},0]
[]
[null,"7C5900","P.B",196,"車廂預留電話機接點","僅接點預留","台",6700,6300,{"$f":"H745-I745","v":400},6.3492063492063489E-2,"不含電話機&按裝 [BY(工務or業主)]"]
[null,"Y25300","P.B",196,"追加電話機(工廠配合留孔)",null,"台",700,700,{"$f":"H746-I746","v":0},0,"只有電話機,預留接點另計"]
[null,"Y23700","P.B",196,"追加電話機(工事現地配合鑽孔)",null,"台",6000,6000,{"$f":"H747-I747","v":0},0,"只有電話機,預留接點另計"]
[]
[null,"7C5700","P.B.F",197,"車廂預留刷卡機接點","僅接點預留","台",11600,11400,{"$f":"H749-I749","v":200},1.7543859649122806E-2,"不含刷卡機&磁卡 [BY業主]"]
[null,"7C5710","P.B.F",197,"車廂預留刷卡機接點+面板開孔","僅接點預留&面板留孔","台",14200,14000,{"$f":"H750-I750","v":200},{"$f":"IF(I750>0,(H750-I750)/I750,-(H750-I750)/I750)","v":1.4285714285714285E-2}]
[null,"7C5800","P.B",197,"車廂設置(永大牌)刷卡機","含感應式刷卡機&磁卡","台",12300,12300,{"$f":"H751-I751","v":0},0,"感應式刷卡機(茂迪AR-829E),磁卡(50片/台)"]
[]
[null,"7C2600","P.B.F",198,"遠隔監控 (組)","1~7台/組 (配賦於第1台)","台",15800,15500,{"$f":"H753-I753","v":300},1.935483870967742E-2,"適用:7台以內/組 (2~6號機不配賦)"]
[null,"A03800","P.B.F",198,"遠隔監控工事配線費(EAS)",null,"台",5300,5300,0,0,"工務配合費(業主未將電話線拉至機房時)"]
[null,"7C2700","P.B",198,"物聯網(BY工務購買)","1~4台/組用, 5~8台/2組","組",17800,17700,100,5.6497175141242938E-3]
[null,"7C9400","P.B",198,"廂內監控(需搭配物聯網)","物聯網費用需另計","台",187900,187900,0,0]
[null,"7C9410","P.B",198,"人臉辨識(群)","人臉辨識機by業主,永大提供通訊協議","群",78800,78800,0,0,"人臉辨識機by業主,永大提供通訊協議"]
[null,"7C9415","P.B",198,"人臉辨識(台)","PC板及配線","台",1400,1400,{"$f":"H758-I758","v":0},{"$f":"IF(I758>0,(H758-I758)/I758,-(H758-I758)/I758)","v":0}]
[null,"7C9460","P.B",198,"人流管控(群)","僅限一層樓(一般為大廳)","群",178000,174300,3700,2.1227768215720023E-2]
[null,"7C9500","P.B",198,"APS絕對定位系統(台)(含20停)",null,"台",27800,27300,500,1.8315018315018316E-2]
[null,"7C9510","P.B",198,"APS絕對定位系統 ± 1(停)",null,"停",1400,1400,0,0]
[null,"7C9520","P.B",198,"保安模式",null,"台",110500,109100,1400,1.2832263978001834E-2]
[null,"7C9540","P.B",198,"緊急可視系統",null,"台",40900,40900,0,0]
[null,"7C9100","P.B.F",198,"直話機系統","適用:EAS,VAG","台",15600,15500,100,6.4516129032258064E-3,"1.UAS-6,HE2車廂已有話機,控盤內無按裝空間,不適用\n2.含安裝測試及配線\n3.遠隔監控及直話系統限擇一取付"]
[]
[null,"4C8750","P.B.F",199,"天井加裝空氣清淨器(標準型)","P6~P24人","台",8900,8900,{"$f":"H766-I766","v":0},0,"標準殺菌型: J POWER 600型 (循環式不可選用)"]
[null,"4C8760","P.B.F",199,"天井加裝空氣清淨器+奈米光觸媒","P6~P24人","台",11600,11600,{"$f":"H767-I767","v":0},0,"J POWER 600型 + 奈米光觸媒"]
[null,"7C9350","P.B.F",199,"天井加裝(夏普)空氣清淨器","P6~P24人","台",40000,39800,{"$f":"H768-I768","v":200},{"$f":"IF(I768>0,(H768-I768)/I768,-(H768-I768)/I768)","v":5.0251256281407036E-3},"型號:IG-002DCT 除菌離子"]
[null,"P003","P.B.F",199,"第二年起空氣清淨器\n保養保固費用　　　　　　　　　　　　　　",null,"年",5500,5500,{"$f":"H769-I769","v":0},0,"以年為單位, 僅看保養月數(不含借用), 四捨五入.\n例:(1)保養月數:18個月~29個月以1年計(5,500元)\n     (2)保養月數:30個月~41個月以2年計(5,500元*2年)"]
[]
[null,"4C8850","P.B.F",200,"車廂加裝冷氣　　　　　　　　　　　　　　","P12人以上","台",90500,89300,{"$f":"H771-I771","v":1200},1.3437849944008958E-2,"含冷氣集水盤(SH)等&\nFlat Cable 48C(附同軸)→48C,60C加價"]
[null,"P004","P.B.F",200,"第二年起冷氣,保養保固費用　　　　　　　　　　　　　　",null,"年",13800,13800,{"$f":"H772-I772","v":0},0,"以年為單位, 僅看保養月數(不含借用), 四捨五入.\n例:(1)保養月數:18個月~29個月以1年計(13,800元)\n     (2)保養月數:30個月~41個月以2年計(13,800元*2年)"]
[]
[null,"7C5100","P",202,"自動水平調整",null,"台",2300,2200,{"$f":"H774-I774","v":100},{"$f":"IF(I774>0,(H774-I774)/I774,-(H774-I774)/I774)","v":4.5454545454545456E-2}]
[]
[null,"Y25000","B",205,"永大版病床梯急救專用",null,"案",13600,13600,{"$f":"H776-I776","v":0},{"$f":"IF(I776>0,(H776-I776)/I776,-(H776-I776)/I776)","v":0},"以(案)為單位加計,特殊程式軟體開發需3個月以上"]
[]
[null,"Y26400","P.B",206,"紫外線殺菌燈",null,"台",5700,5700,{"$f":"H778-I778","v":0},{"$f":"IF(I778>0,(H778-I778)/I778,-(H778-I778)/I778)","v":0},"廠商:祥全電子"]
[]
[null,"4C7700","P",253.25399999999999,"車廂附防撞板  SH","P6~P12人","台",27300,26500,{"$f":"H780-I780","v":800},3.0188679245283019E-2,"1.標準: 3側附防撞板\n2.SH防撞板: 2T(唐榮)板材"]
[null,"4C7750","P",253.25399999999999,"車廂附防撞板  SH","P13~P17人","台",33000,31600,1400,4.4303797468354431E-2]
[null,"4C7800","P",253.25399999999999,"車廂附防撞板  SH","P20~P24人","台",35200,34100,1100,3.2258064516129031E-2]
[null,"4F2000","F",253.25399999999999,"車廂附防撞板  (橡膠)","F-1000kg","台",47600,47600,0,0,"1.標準: 3側附防撞板\n2.橡膠防撞板: 9T(生膠)\n3.高度:900mm"]
[null,"4F2100","F",253.25399999999999,"車廂附防撞板  (橡膠)","F-1500kg~2000kg","台",54700,54700,0,0]
[null,"4F2200","F",253.25399999999999,"車廂附防撞板  (橡膠)","F-2500kg~3000kg","台",68100,68100,0,{"$f":"IF(I785>0,(H785-I785)/I785,-(H785-I785)/I785)","v":0}]
[null,"4F2300","F",253.25399999999999,"車廂附防撞板  (SH)","F-1000kg","台",43800,37800,6000,0.15873015873015872,"1.標準: 3側附防撞板\n2.SH防撞板: 2T(唐榮)板材"]
[null,"4F2400","F",253.25399999999999,"車廂附防撞板  (SH)","F-1500kg~2000kg","台",54500,47000,7500,0.15957446808510639]
[null,"4F2500","F",253.25399999999999,"車廂附防撞板  (SH)","F-2500kg~3000kg","台",68700,58800,9900,0.1683673469387755]
[]
[null,"3C7000","P",92,"OH ≧7.5M","P6~P11人","台",13900,13800,{"$f":"H790-I790","v":100},7.246376811594203E-3,"含RAIL,MAIN ROPE&電(纜)線材--等追加"]
[null,"3C7100","P",92,"OH ≧7.5M","P12~P15人","台",16000,15800,200,1.2658227848101266E-2]
[null,"3C7200","P",92,"OH ≧7.5M","P17~P24人","台",22500,22400,100,4.464285714285714E-3]
[null,"3B0500","B",92,"OH ≧7.5M","B-750~1000kg ","台",19700,19700,0,0,"含RAIL,MAIN ROPE&電(纜)線材--等追加"]
[null,"3F1000","F",92,"OH ≧7.5M","F-1000kg ","台",22100,22700,-600,-2.643171806167401E-2]
[null,"3F1100","F",92,"OH ≧7.5M","F-1500~2000kg ","台",27600,28400,-800,-2.8169014084507043E-2]
[null,"3F1200","F",92,"OH ≧7.5M","F-2500~3000kg ","台",40700,41700,{"$f":"H796-I796","v":-1000},-2.3980815347721823E-2]
[null,"B00700","P.B.F",92,"OH 超過6M",null,"台",5300,5300,0,0,"無機房,UAS-08,UAS1-06不需加計"]
[null,"3C7300","P",95,"樓高 ≧ 6M","P6~P11人","樓",11300,11100,200,1.8018018018018018E-2,"含RAIL,MAIN ROPE&電(纜)線材--等追加"]
[null,"3C7400","P",95,"樓高 ≧ 6M","P12~P15人","樓",13300,13200,100,7.575757575757576E-3]
[null,"3C7500","P",95,"樓高 ≧ 6M","P17~P24人","樓",19800,19700,100,5.076142131979695E-3]
[null,"3B0600","B",95,"樓高 ≧ 6M","B-750~1000kg ","樓",17000,17100,-100,-5.8479532163742687E-3,"含RAIL,MAIN ROPE&電(纜)線材--等追加"]
[null,"3F1300","F",95,"樓高 ≧ 6M","F-1000kg ","樓",19400,20000,-600,-0.03]
[null,"3F1400","F",95,"樓高 ≧ 6M","F-1500~2000kg ","樓",25000,25800,-800,-3.1007751937984496E-2]
[null,"3F1500","F",95,"樓高 ≧ 6M","F-2500~3000kg ","樓",38000,39000,{"$f":"H804-I804","v":-1000},-2.564102564102564E-2]
[]
[null,"0C0300","P",501,"CAGE RAIL T-8K→T-13K","3.4m/樓高計","樓",2400,2400,{"$f":"H806-I806","v":0},0,"1.T-5K RAIL: 自製(中鋼)素材\n2.T-8K RAIL: 進口(塞維拉)成品\n3.T-13K RAIL: 進口(塞維拉BE)成品\n4.T-18K RAIL: 進口(塞維拉BE)成品\n5.T-24K RAIL: 進口(塞維拉BE)成品"]
[null,"0C0600","P",501,"CAGE RAIL T-13K→T-18K","3.4m/樓高計","樓",3800,3900,-100,-2.564102564102564E-2]
[null,"0C0900","P",501,"CAGE RAIL T-18K→T-24K","3.4m/樓高計","樓",3200,3400,-200,-5.8823529411764705E-2]
[null,"0C1200","P",501,"CWT RAIL T-5K→T-8K","3.4m/樓高計","樓",1100,1100,0,0]
[null,"0C1500","P",501,"CWT RAIL T-8K→T-13K","3.4m/樓高計","樓",3200,3300,-100,-3.0303030303030304E-2]
[null,"0C1800","P",501,"CWT RAIL T-13K→T-18K","3.4m/樓高計","樓",3900,4100,-200,-4.878048780487805E-2]
[null,"0B0110","B",501,"CAGE RAIL T-13K→T-18K","4.0m/樓高計","樓",4500,4600,-100,-2.1739130434782608E-2]
[null,"0B0310","B",501,"CWT RAIL T-5K→T-8K","4.0m/樓高計","樓",1100,1100,0,0]
[null,"0B0330","B",501,"CWT RAIL T-8K→T-13K","4.0m/樓高計","樓",4000,4200,-200,-4.7619047619047616E-2]
[null,"0F0200","F",501,"CAGE RAIL T-13K→T-18K","4.0m/樓高計","樓",4500,4600,-100,-2.1739130434782608E-2]
[null,"0F0400","F",501,"CAGE RAIL T-18K→T-24K","4.0m/樓高計","樓",3800,4100,-300,-7.3170731707317069E-2]
[null,"0F1200","F",501,"CWT RAIL T-8K→T-13K","4.0m/樓高計","樓",4000,4200,-200,-4.7619047619047616E-2]
[null,"0F1400","F",501,"CWT RAIL T-13K→T-18K","4.0m/樓高計","樓",4600,4700,-100,-2.1276595744680851E-2]
[]
[null,"3C8200","P",502,"(10ψ×4)MAIN ROPE 指定進口","P6~11人(60~105m) ","樓",900,700,{"$f":"H820-I820","v":200},0.2857142857142857]
[null,"3C8300","P",502,"(10ψ×5)MAIN ROPE 指定進口","P12~15人(60~105m)  ","樓",1100,800,{"$f":"H821-I821","v":300},0.375]
[null,"3C8650","P",502,"ROPE 10ψ*4 →  10ψ*5","UAY3-15人使用","台",23100,22900,{"$f":"H822-I822","v":200},8.7336244541484712E-3,"車廂加重>250KG需加計.>400KG則需跳級為大載重"]
[null,"3C9430","P",502,"ROPE 12ψ×5 → 12ψ×6","P24人 (60m~150m)","台",31400,31200,{"$f":"H823-I823","v":200},{"$f":"IF(I823>0,(H823-I823)/I823,-(H823-I823)/I823)","v":6.41025641025641E-3}]
[]
[null,"3C9400","P",503,"GSD-MM1 → GSD-MM ","P6~11人 (60m~105m)","台",37000,31400,{"$f":"H825-I825","v":5600},{"$f":"IF(I825>0,(H825-I825)/I825,-(H825-I825)/I825)","v":0.17834394904458598},"含10ψ4→10ψ5加價, 主機跳級"]
[null,"3C9420","P",503,"GSD-ML1 → GSC-LL","P17~20人 (60m~150m)","台",149200,120500,{"$f":"H826-I826","v":28700},{"$f":"IF(I826>0,(H826-I826)/I826,-(H826-I826)/I826)","v":0.23817427385892115},"含10ψ6→12ψ5加價, 主機跳級"]
[null,"3C9440","P",503,"GSD-MM(Y04) → GSD-ML1(Y06)","P12~15人 (60m~120m)","台",245500,214000,{"$f":"H827-I827","v":31500},{"$f":"IF(I827>0,(H827-I827)/I827,-(H827-I827)/I827)","v":0.14719626168224298},"含(1)13K*8K→18K*8K(10停)(2)結構Y04→Y06(3)主機跳級"]
[]
[null,"0C1900","P.B",505,"OIL BUFFER","P6~13人,B-750~1000kg(60m)","台",2300,2300,{"$f":"H829-I829","v":0},0]
[]
[null,"4F4200","F",506,"廂門踏板 (鐵材)","F-1000kg 2S-1400W","台",14500,17900,{"$f":"H831-I831","v":-3400},-0.18994413407821228]
[null,"4F4300","F",506,"廂門踏板 (鐵材)","F-1500~2000kg 2S-1700W","台",15500,20500,-5000,-0.24390243902439024]
[null,"4F4000","F",506,"出入口門踏板 (鐵材)","F-1000kg 2S-1400W","停",19500,24400,-4900,-0.20081967213114754]
[null,"4F4100","F",506,"出入口門踏板 (鐵材)","F-1500~2000kg 2S-1700W","停",20000,26800,-6800,-0.2537313432835821]
[null,"3C8700","P.B.F",506,"乘場SILL下護板與車廂下護板同高","1.6t 鍍鋅鋼板","停",1400,1400,0,0]
[null,"3C8710","P.B.F",506,"乘場SILL下護板與車廂下護板同高","1.2t 髮紋不鏽鋼","停",2900,2500,400,0.16]
[]
[null,"F03900","PF.F",507,"貨梯出入口SILL支撐架 OP:1100mm 無持出",null,"停",5300,5300,{"$f":"H838-I838","v":0},0]
[null,"F04000","PF.F",507,"貨梯出入口SILL支撐架 OP:1400mm 無持出",null,"停",6500,6500,{"$f":"H839-I839","v":0},0]
[null,"F04100","PF.F",507,"貨梯出入口SILL支撐架 OP:1700mm 無持出",null,"停",7600,7600,{"$f":"H840-I840","v":0},0]
[null,"F04200","PF.F",507,"貨梯出入口SILL支撐架 OP:2300mm 無持出",null,"停",8800,8800,{"$f":"H841-I841","v":0},0]
[]
[null,"B00900","P",508,"速度150米(含)以上電纜側追加保護網　　　　　　",null,"停",2900,2900,{"$f":"H843-I843","v":0},0,"樓數一半"]
[null,"E01400","P",508,"CWT側落式(EAS人乘千鳥型需加計)　　　　　　　　　　　　　　",null,"樓",2900,2900,{"$f":"H844-I844","v":0},0]
[null,"7C6000","P.B.F",201,"機坑浸水運轉管制",null,"台",11300,10900,{"$f":"H845-I845","v":400},3.669724770642202E-2,"含液面控制器(ST-70AB)&CONN"]
[null,"7C8500","P.B.F",508,"PCB凡立水處理","硫磺區 or 外島地區","台",9000,8500,{"$f":"H846-I846","v":500},5.8823529411764705E-2,"硫磺區 or 外島地區 需加計"]
[]
[null,"0C2300","P.B.F",600,"追加機房支撐樑","H300*150*6.5*9","支",9600,9200,{"$f":"H848-I848","v":400},4.3478260869565216E-2,"長度: L=3m計"]
[null,"B02100","P",601,"補強樑(U125*65*6)","UAS1-06,UAS-08選用","停",3600,3600,0,{"$f":"IF(I849>0,(H849-I849)/I849,-(H849-I849)/I849)","v":0},"長度: L=1600mm計,含2只固定拖架"]
[null,"B02200","P",601,"補強樑(H100*100*6*8)","VAG機種選用","停",6900,6900,0,0,"長度: L=1870mm計,含2只固定拖架"]
[null,"B00400","P",601,"補強樑(H100*100*6*8)","EAS P-11人(含)以下","停",5900,5900,0,0,"長度: L=1950mm計,含2只固定拖架"]
[null,"B00500","P",601,"補強樑(H100*100*6*8)","EAS P-12~P15人","停",6300,6300,0,0,"長度: L=2100mm計,含2只固定拖架"]
[null,"B00600","P",601,"補強樑(H100*100*6*8)","EAS P-17人(含)以上","停",7400,7400,0,0,"長度: L=2550mm計,含2只固定拖架"]
[null,"Y04100","B",601,"補強樑(H150*150*7*10)","B-TYPE","停",16800,16800,0,0,"長度: L=3100mm計,含4只固定拖架"]
[null,"Y04200","F",601,"補強樑(H150*150*7*10)","F-2000(含)以下","停",18400,18400,{"$f":"H855-I855","v":0},{"$f":"IF(I855>0,(H855-I855)/I855,-(H855-I855)/I855)","v":0},"長度: L=3400mm計,含4只固定拖架"]
[null,"Y04300","F",601,"補強樑(H150*150*7*10)","F-2500~3000","停",21400,21400,{"$f":"H856-I856","v":0},{"$f":"IF(I856>0,(H856-I856)/I856,-(H856-I856)/I856)","v":0},"長度: L=4000mm計,含4只固定拖架"]
[null,"Y04400","F",601,"補強樑(H250*250*9*14)","F-3500(含)以上","停",73100,73100,{"$f":"H857-I857","v":0},{"$f":"IF(I857>0,(H857-I857)/I857,-(H857-I857)/I857)","v":0},"長度: L=5800mm計,含4只固定拖架及2塊12t鐵板"]
[]
[null,"1S0100","UAS",16.170000000000002,"小框 SH (非最上階)","P6人 2S-2P OP-800W","停",2100,1700,{"$f":"H859-I859","v":400},0.23529411764705882,"1.SH素材:為國內(唐榮)板材(不鉋溝)\n2.SM素材:為國內(日新)板於國內加工\n3.鍍鈦顏色: 金黃色(標準)\n4.寬型門框(其它階): 140W×50D(標準)"]
[null,"1S0200","UAS",16.170000000000002,"小框 SH鍍鈦(金色)(非最上階)","P6人 2S-2P OP-800W","停",7700,6300,1400,0.22222222222222221]
[null,"1S1000","UAS",16.170000000000002,"小框 SM (非最上階)","P6人 2S-2P OP-800W","停",6400,4900,1500,0.30612244897959184]
[null,"1S1100","UAS",16.170000000000002,"小框 SM鍍鈦(金色)(非最上階)","P6人 2S-2P OP-800W","停",9300,7700,1600,0.20779220779220781]
[null,"1S2000","UAS",16.170000000000002,"小框&Frame SH (最上階)","P6人 2S-2P OP-800W","停",11000,9400,1600,0.1702127659574468,"1.SH素材:為國內(唐榮)板材(不鉋溝)\n2.SM素材:為國內(日新)板於國內加工\n3.含最上階PANEL FRAME一併改為SH.SM.鍍鈦\n4.寬型門框(最上階): 50W×187D(標準)"]
[null,"1S2100","UAS",16.170000000000002,"小框&Frame SH鍍鈦(金色)(最上階)","P6人 2S-2P OP-800W","停",21500,17800,3700,0.20786516853932585]
[null,"1S3000","UAS",16.170000000000002,"小框&Frame SM (最上階)","P6人 2S-2P OP-800W","停",18400,14500,3900,0.26896551724137929]
[null,"1S3100","UAS",16.170000000000002,"小框&Frame SM鍍鈦(金色)(最上階)","P6人 2S-2P OP-800W","停",25500,21400,4100,0.19158878504672897]
[null,"1S0300","UAS",16.170000000000002,"小框 SH鍍鈦(遠東) (非最上階)","P6人 2S-2P OP-800W","停",13800,12200,1600,0.13114754098360656]
[null,"1S1200","UAS",16.170000000000002,"小框 SM鍍鈦(遠東) (非最上階)","P6人 2S-2P OP-800W","停",15300,13600,1700,0.125]
[null,"1S2200","UAS",16.170000000000002,"小框&Frame SH鍍鈦(遠東)(最上階)","P6人 2S-2P OP-800W","停",36600,32600,4000,0.12269938650306748]
[null,"1S3200","UAS",16.170000000000002,"小框&Frame SM鍍鈦(遠東)(最上階)","P6人 2S-2P OP-800W","停",40500,36200,4300,0.11878453038674033]
[null,"1S3300","UAS",16.170000000000002,"其他階比照最上階寬直框(CE)","P6人 2S-2P OP-800W","停",2000,1900,{"$f":"H871-I871","v":100},{"$f":"IF(I871>0,(H871-I871)/I871,-(H871-I871)/I871)","v":5.2631578947368418E-2}]
[null,"1S3400","UAS",16.170000000000002,"其他階比照最上階寬直框(量A值)(CE)","P6人 2S-2P OP-800W","停",5600,5400,{"$f":"H872-I872","v":200},{"$f":"IF(I872>0,(H872-I872)/I872,-(H872-I872)/I872)","v":3.7037037037037035E-2}]
[null,"1S3500","UAS",16.170000000000002,"最上階寬直框(量A值)(CE)","P6人 2S-2P OP-800W","停",4100,3900,{"$f":"H873-I873","v":200},{"$f":"IF(I873>0,(H873-I873)/I873,-(H873-I873)/I873)","v":5.128205128205128E-2}]
[null,"Y10400","UAS",16.170000000000002,"其他階比照最上階大框製作(SH)","P6人 2S-2P OP-800W","停",4800,4500,{"$f":"H874-I874","v":300},{"$f":"IF(I874>0,(H874-I874)/I874,-(H874-I874)/I874)","v":6.6666666666666666E-2},"106.09.04(方啟智課長MAIL提供)"]
[null,"Y24600","UAS",16.170000000000002,"大框寬斜型製作(IP,CE)","P6人 2S-2P OP-800W","停",6100,6000,{"$f":"H875-I875","v":100},{"$f":"IF(I875>0,(H875-I875)/I875,-(H875-I875)/I875)","v":1.6666666666666666E-2},"參考BQ-E7300"]
[null,"4S3000","UAS","12,13","2S-800→2S-900 (台)","標準為2S:800W*EH-2000","台",3500,3300,200,6.0606060606060608E-2,"標準仕樣: 標準2S-800W*EH-2000\n                 門框AS-1X(CE),出入口門(CE or IP),"]
[null,"4S3100","UAS","12,13","2S-800→2S-900 (停)","標準為2S:800W*EH-2000","停",800,700,100,0.14285714285714285]
[null,"4S3200","UAS","12,13","EH-2000→EH-2200 (台)","標準為2S:800W*EH-2000","台",7000,6800,200,2.9411764705882353E-2,"1.車廂側板&廂門(CE or IP),天井型式(標準)\n2.含天井加高⊕200mm加計"]
[null,"4S3300","UAS","12,13","EH-2000→EH-2200 (停)","標準為2S:800W*EH-2000","停",1200,1100,100,9.0909090909090912E-2]
[null,"2S0300","UAS",81,"紅外線光幕+內縮型機械SHOE","CEDES SHOE","台",11600,11600,0,0,"光幕型號: Cegard/Mini"]
[null,"2S1000","UAS",26,"出入口門  SH","P6人 2S-2P OP-800W","停",6900,4900,2000,0.40816326530612246,"1.SH素材:為國內(唐榮)板材(不鉋溝)\n2.SM素材:為國內(日新)板於國內加工"]
[null,"2S1100","UAS",26,"出入口門  SH鍍鈦(金色)","P6人 2S-2P OP-800W","停",11800,9500,2300,0.24210526315789474]
[null,"2S1200","UAS",26,"出入口門  SH鍍鈦(遠東)","P6人 2S-2P OP-800W","停",20900,18400,2500,0.1358695652173913]
[null,"2S2000","UAS",266,"出入口門  SM","P6人 2S-2P OP-800W","停",10100,7800,2300,0.29487179487179488]
[null,"2S2100","UAS",266,"出入口門  SM鍍鈦(金色)","P6人 2S-2P OP-800W","停",14300,11900,2400,0.20168067226890757]
[null,"2S2200","UAS",266,"出入口門  SM鍍鈦(遠東)","P6人 2S-2P OP-800W","停",23400,20800,2600,0.125]
[null,"2S2300","UAS",86,"出入口門 (無取付三角key)","P6人 2S-2P OP-800W","停",2100,1700,{"$f":"H887-I887","v":400},{"$f":"IF(I887>0,(H887-I887)/I887,-(H887-I887)/I887)","v":0.23529411764705882}]
[null,"Y10600","UAS",26,"出入口門or廂門(追加透視窗)(UAS1-06)","UAS1-06適用","停",2500,2500,0,0]
[null,"3S0150","UAS",38.39,"大理石(或石英磚)貼付預留(UAS1-06)","UAS1-06適用","台",19800,19200,600,3.125E-2,"φ8-ROPE⊕1條及WT-3塊改鑄鐵"]
[null,"3S1000","UAS",282,"千鳥型",null,"台",91400,85800,5600,6.5268065268065265E-2,"1.需另計出入口防落網,UAS1-06帶鎖門刀無法對應\n2.(例) UAS-6*6/5-2S45m,      ⊕119,200/台+\n           17,100/停*1停(Through僅1停)=⊕136,300/台"]
[null,"4S0100","UAS","30.43.44.45","車廂側板&廂門  SH","不含OPB面板材質變更","台",33400,25800,7600,0.29457364341085274,"1.SH素材為國內(唐榮)板材.\n2.SM素材:為國內(日新)板於國內加工"]
[null,"4S0200","UAS","30.43.44.45","車廂側板&廂門  SH鍍鈦(金色)","不含OPB面板材質變更","台",53900,45700,8200,0.17943107221006566]
[null,"4S1000","UAS","30.43.44.45","車廂側板&廂門  SM","不含OPB面板材質變更","台",44900,36100,8800,0.24376731301939059]
[null,"4S1100","UAS","30.43.44.45","車廂側板&廂門  SM鍍鈦(金色)","不含OPB面板材質變更","台",63400,54300,9100,0.16758747697974216]
[null,"4S0300","UAS","30.43.44.45","車廂側板&廂門  SH鍍鈦(遠東)","不含OPB面板材質變更","台",92200,83900,8300,9.8927294398092974E-2]
[null,"4S1200","UAS","30.43.44.45","車廂側板&廂門  SM鍍鈦(遠東)","不含OPB面板材質變更","台",101800,92400,9400,0.10173160173160173]
[null,"8S0100","UAS",56.57,"US型式OPB面板  SH",null,"台",5800,5400,400,7.407407407407407E-2]
[null,"8S0200","UAS",56.57,"US型式OPB面板  SM",null,"台",8000,7600,400,5.2631578947368418E-2]
[null,"8S0300","UAS",56.57,"US型式OPB面板  SH鍍鈦(金)",null,"台",7600,7100,500,7.0422535211267609E-2]
[null,"8S0350","UAS",56.57,"US型式OPB面板  SM鍍鈦(金)",null,"台",9800,9300,{"$f":"H900-I900","v":500},5.3763440860215055E-2]
[null,"8S0400","UAS",56.57,"US型式OPB面板  SH鍍鈦(遠東)",null,"台",8800,8300,500,6.0240963855421686E-2]
[null,"8S0450","UAS",56.57,"US型式OPB面板  SM鍍鈦(遠東)",null,"台",11000,10400,{"$f":"H902-I902","v":600},5.7692307692307696E-2]
[null,"Y09000","UAS",157,"天井加高 ⊕200mm(UAS1-06)",null,"台",7000,6800,200,2.9411764705882353E-2,"參照OPTION項次4S3200"]
[null,"7S0300","UAS",176,"CCTV配線預留 ","5C FV線材(標準)","台",13100,12900,200,1.5503875968992248E-2,"1.標準長度:預留予CPI FRAME上,  2.長度L=50m計"]
[null,"7S0400","UAS",197,"車廂預留刷卡機接點","僅接點預留","台",11900,11700,200,1.7094017094017096E-2,"不含刷卡機&磁卡 [BY(工務or業主)]"]
[null,"4S4000","UAS",101,"意匠非套餐(UAS1-06)",null,"台",5500,4800,{"$f":"H906-I906","v":700},0.14583333333333334,"最多加計5台"]
[null,"Y01700","UAS",155,"CWT附WEDGE(台)","UAS1-P6人","台",50600,50600,{"$f":"H907-I907","v":0},0,"1.含CWT RAIL T-5K → T-8K.(參考BQ-E7101)\n2.含SUB WT採混用(複合式+鑄鐵式)."]
[null,"9S0100","UAS",60.61,"FOX IND→DIG-SE1","UAS1-P6人","停",500,400,{"$f":"H908-I908","v":100},{"$f":"IF(I908>0,(H908-I908)/I908,-(H908-I908)/I908)","v":0.25}]
[null,"Y03400","UAS",60.61,"DIG-SE1→DIG-C(SH)","UAS1-P6人","停",800,800,{"$f":"H909-I909","v":0},{"$f":"IF(I909>0,(H909-I909)/I909,-(H909-I909)/I909)","v":0},"參考BQ-E7256"]
[]
[null,"A00500","P.B.F",601,"預埋機房吊鉤　　　　　　　　　　　　　　　　",null,"台",5500,5500,{"$f":"H911-I911","v":0},{"$f":"IF(I911>0,(H911-I911)/I911,-(H911-I911)/I911)","v":0}]
[null,"Y08700","P",601,"小型門框門框保護",null,"停",1400,1400,0,0,"含後續拆除及清運費用"]
[null,"Y08800","P",601,"大型門框門框保護",null,"停",1600,1600,0,0,"含後續拆除及清運費用"]
[null,"C00100","P.B.F",601,"IND填縫工程　　　　　　　　　　　　　",null,"停",1000,1000,0,0]
[null,"C02100","P.B.F",601,"小型門框填縫２０ＣＭ以下 (永大出料)　　　　　　　　　　　　　　　　",null,"停",1400,1400,0,0,"不含IND填縫費"]
[null,"C02200","P.B.F",601,"大型門框填縫２０－２９ＣＭ (永大出料)　　　　　　　　　　　　　　　　",null,"停",2000,2000,0,0,"不含IND填縫費"]
[null,"C02300","P.B.F",601,"大型門框填縫３０ＣＭ以上 (永大出料)　　　　　　　　　　　　　　　",null,"停",2500,2500,0,0,"不含IND填縫費"]
[null,"Y05100","P.B.F",601,"小型門框填縫２０ＣＭ以下 (業主供料)　　　　　　　　　　　　　　　　",null,"停",1100,1100,0,0,"不含IND填縫費"]
[null,"Y05200","P.B.F",601,"大型門框填縫２０－２９ＣＭ (業主供料)　　　　　　　　　　　　　　　　",null,"停",1500,1500,0,0,"不含IND填縫費"]
[null,"Y05300","P.B.F",601,"大型門框填縫３０ＣＭ以上 (業主供料)　　　　　　　　　　　　　　　",null,"停",1800,1800,0,0,"不含IND填縫費"]
[null,"A00200","P.B.F",601,"機房打水泥　　",null,"台",27300,27300,0,0]
[null,"D00200","P.B.F",601,"機坑打水泥　　　　　　　　　　　　　　",null,"台",8200,8200,0,0]
[null,"E00300","P.B.F",601,"車廂內夾板保護板含拆除至垃圾場　　　　　　　",null,"台",35000,32300,2700,8.3591331269349839E-2]
[null,"E01000","P.B.F",601,"車廂內保護板(內襯保麗龍)含拆除至垃圾場                            ",null,"台",37800,35000,2800,0.08]
[null,"E01200","P.B.F",601,"車廂內耐力板保護板含拆除至垃圾場　                            ",null,"台",48500,45800,2700,5.8951965065502182E-2]
[null,"E01300","P.B.F",601,"車廂保護板拆除再復原費用",null,"台",13600,10900,{"$f":"H926-I926","v":2700},0.24770642201834864]
[null,"D00100","P.B.F",601,"不銹鋼鐵爬梯SH　　　　　　　　　　　　　",null,"台",5500,5500,0,0]
[null,"D00300","P.B.F",601,"機坑隔開網－二台共用　　　　　　　　　　",null,"台",4500,4500,0,0]
[null,"D00900","P.B.F",601,"機坑水泥台施作(一體式)",null,"台",3800,3800,0,0]
[null,"D01400","P.B.F",601,"機坑水泥台施作(水泥台式)",null,"台",9000,9000,0,0]
[null,"Y08200","P.B.F",601,"RAIL以3.5M長度出貨",null,"台",18800,18800,{"$f":"H931-I931","v":0},{"$f":"IF(I931>0,(H931-I931)/I931,-(H931-I931)/I931)","v":0}]
[null,"7C9310","P",601,"追加 AGV改造(自動導引車)","P8~24人","台",106900,104300,{"$f":"H932-I932","v":2600},{"$f":"IF(I932>0,(H932-I932)/I932,-(H932-I932)/I932)","v":2.4928092042186004E-2}]
[]
[null,"A00100","P.B.F",null,"機房安全欄杆",null,"台",19600,19600,{"$f":"H934-I934","v":0},0]
[null,"A00300","P.B.F",null,"機房溫控排風扇                          ",null,"台",6800,6800,0,0]
[null,"A00400","P.B.F",null,"機房混凝土施工　　　　　　　　　　　　　",null,"台",27300,27300,0,0]
[null,"A00600","P.B.F",null,"電源開關箱及NFB                    ",null,"台",10200,10200,0,0]
[null,"A00700","P.B.F",null,"機房主鋼索及調速機加裝安全蓋　　　　　　",null,"台",4600,4600,0,0]
[null,"A00800","P.B.F",null,"車廂塑膠碰墊三側　　　　　　　　　　　　",null,"台",12300,12300,0,0]
[null,"A00900","P.B.F",null,"定時開關抽風扇                          ",null,"台",6800,6800,0,0]
[null,"A01000","P.B.F",null,"高速梯ＴＨ　Ｍ/Ｃ機房器具安置　　　　　 ",null,"台",10600,10600,0,0]
[null,"A01100","P.B.F",null,"高速梯ＴＨ　Ｍ/Ｃ機房ＢＥＡＭ　　　　　 ",null,"台",5300,5300,0,0]
[null,"A01200","P.B.F",null,"高速梯ＴＨ　Ｍ/Ｃ機房配線槽　　　　　　 ",null,"台",5300,5300,0,0]
[null,"A01300","P.B.F",null,"機房洞口及線槽溝修打(含清潔)",null,"台",5300,5300,0,0]
[null,"A01400","P.B.F",null,"地板灌水泥(4--5公分),但需補平粉光",null,"台",10500,10500,0,0]
[null,"A01500","P.B.F",null,"機房RC施作(10公分高) 需補平粉光",null,"台",27300,27300,0,0]
[null,"A01600","P.B.F",null,"主機機座打除及清潔(以鋼樑為基座,)",null,"台",9000,9000,0,0]
[null,"A01700","P.B.F",null,"主機水泥機座打除及清潔",null,"台",4500,4500,0,0]
[null,"A01800","P.B.F",null,"OH高度不足,機房地板重新施作",null,"台",30000,30000,0,0]
[null,"A01900","P.B.F",null,"SUS材質機房門(含門框及門弓器)換新",null,"停",18000,18000,0,0]
[null,"A02000","P.B.F",null,"IP材質機房門(含門框及門弓器)換新",null,"停",15000,15000,0,0]
[null,"A02100","P.B.F",null,"機房門追加門弓器",null,"扇",1500,1500,0,0]
[null,"A02200","P.B.F",null,"機房通風窗遮雨棚",null,"組",4500,4500,0,0]
[null,"A02300","P.B.F",null,"機房門遮雨棚",null,"組",4500,4500,0,0]
[null,"A02400","P.B.F",null,"百葉窗開孔及按裝(含百葉窗)",null,"孔",11300,11300,0,0]
[null,"A02500","P.B.F",null,"百葉窗換裝",null,"扇",8300,8300,0,0]
[null,"A02600","P.B.F",null,"抽風扇開孔及按裝(含抽風扇)",null,"孔",6800,6800,0,0]
[null,"A02700","P.B.F",null,"抽風扇換裝",null,"組",3800,3800,0,0]
[null,"A02800","P.B.F",null,"抽風扇百葉窗開孔及按裝",null,"扇",12000,12000,0,0]
[null,"A02900","P.B.F",null,"玻璃窗加百葉窗開孔及按裝",null,"扇",15000,15000,0,0]
[null,"A03000","P.B.F",null,"機房頂抽風扇換新",null,"組",21000,21000,0,0]
[null,"A03100","P.B.F",null,"電源開關箱移位及配線",null,"組",8300,8300,0,0]
[null,"A03200","P.B.F",null,"照明燈具追加",null,"台",1200,1200,0,0]
[null,"A03300","P.B.F",null,"機房地面磁磚剔除",null,"台",3000,3000,0,0]
[null,"A03400","P.B.F",null,"機房地面貼付PVC地磚",null,"坪",3000,3000,0,0]
[null,"A03500","P.B.F",null,"機房地面貼付鋼磚",null,"坪",6000,6000,0,0]
[null,"A03600","P.B.F",null,"機房地面PU處理",null,"坪",12000,12000,0,0]
[null,"A03700","P.B.F",null,"配合吊運機房重新開孔",null,"孔",6000,6000,0,0]
[null,"B00300","P.B.F",601,"昇降路托架需熱浸鍍鋅處理　　　　　　　　",null,"樓",1600,1600,0,0]
[null,"B01000","P.B.F",null,"昇降道中間隔板　　　　　　　　　　　　　",null,"停",3400,3400,0,0]
[null,"B01100","P.B.F",null,"導軌用化學螺栓",null,"停",5000,5000,0,0]
[null,"B01300","P.B.F",null,"鋼骨結構防火披覆清潔　　　　　　　　　　",null,"停",600,600,0,0]
[null,"B01400","P.B.F",null,"RAIL接頭位置,昇降路牆面修打",null,"處",500,500,0,0]
[null,"B01500","P.B.F",null,"昇降路接線盒至IND配線處打溝",null,"停",500,500,0,0]
[null,"B01600","P.B.F",null,"誘導板處,昇降路牆面修打",null,"停",700,700,0,{"$f":"IF(I975>0,(H975-I975)/I975,-(H975-I975)/I975)","v":0}]
[null,"B01700","P.B.F",null,"昇降路傾斜, 昇降路牆面修打",null,"停",3800,3800,0,0]
[null,"B01800","P.B.F",null,"昇降路消防箱背面水泥修補",null,"處",1800,1800,0,0]
[null,"B01900","P.B.F",null,"昇降路鋼筋修補",null,"停",1200,1200,0,0]
[null,"B02000","P.B.F",null,"昇降路PIT及OH處孔洞封閉",null,"處",3000,3000,0,0]
[null,"C00200","P.B.F",null,"出入口門SILL防落板　　　　　　　　　　　　　",null,"停",9000,9000,0,0]
[null,"C00300","P.B.F",null,"出入口地板施工保護板　　　                      ",null,"停",700,700,0,0]
[null,"C00400","P.B.F",null,"S門框留用噴漆　　　　　　　　　　　　　 ",null,"台",1500,1500,0,0]
[null,"C00500","P.B.F",null,"T門框留用噴漆　　　　　　　　　　　　　 ",null,"停",1900,1900,0,0]
[null,"C00600","P.B.F",null,"臨時施工出入口設置　　　　　　　　　　　　　",null,"停",1000,1000,0,0]
[null,"C00700","P.B.F",null,"ＳＩＬＬ持出補強樑(貨梯)　　　　　　　　　　　",null,"停",5700,5700,0,0]
[null,"C00800","P.B.F",null,"隱藏式對講機　　　　　　　　　　　　　　",null,"組",5300,5300,0,0]
[null,"C00900","P.B.F",null,"更換H.SILL",null,"停",8000,8000,0,0]
[null,"C01000","P.B.F",null,"更換H.SILL除外工程",null,"停",2000,2000,0,0]
[null,"C01200","P.B.F",null,"更換T型門框",null,"停",6300,6300,0,0]
[null,"C01300","P.B.F",null,"更換T型門框除外工程",null,"停",4800,4800,0,0]
[null,"C01400","P.B.F",null,"Ｔ型門框(含幕板)留用噴漆　　　　　　　　　　　  ",null,"台",3100,3100,0,0]
[null,"C01500","P.B.F",null,"ＩＮＤ大理石修打　　　　　　　　　　　　",null,"停",1600,1600,0,0]
[null,"C01600","P.B.F",null,"出入口L型轉向                           ",null,"停",2100,2100,0,0]
[null,"C01700","P.B.F",null,"鋼骨結構工程SILICON門框填縫　　　　　　 ",null,"停",2700,2700,0,0]
[null,"C01800","P.B.F",null,"鋼骨結構門框立柱與橫柱　　　　　　　　　",null,"停",5300,5300,0,0]
[null,"C01900","P.B.F",null,"鋼骨結構ＳＩＬＬ橫樑　　　　　　　　　　",null,"停",1300,1300,0,0]
[null,"C02400","P.B.F",null,"Ｈ.ＤＯＯＲ－２Ｕ　　　　　　　　　　",null,"停",13300,13300,0,0]
[null,"C02500","P.B.F",null,"Ｈ.ＤＯＯＲ－３Ｕ　　　　　　　　　　　 ",null,"停",16600,16600,{"$f":"H998-I998","v":0},0]
[null,"C02600","P.B.F",null,"Ｈ.ＤＯＯＲ－３Ｓ　　　　　　　　　　　 ",null,"停",2700,2700,0,0]
[null,"C02700","P.B.F",null,"Ｈ.ＤＯＯＲ－４Ｐ　　　　　　　　　　　 ",null,"停",2700,2700,0,0]
[null,"C02800","P.B.F",null,"出入口地板大理石復原　　　　　　　　　　",null,"停",3000,3000,0,0]
[null,"C02900","P.B.F",null,"出入口地板磁磚復原　　　　　　　　　　  ",null,"停",1200,1200,0,0]
[null,"C03000","P.B.F",null,"H.SILL牛腿整片修打",null,"停",2300,2300,0,0]
[null,"C03100","P.B.F",null,"IND修打(含修剪鋼筋)",null,"孔",1100,1100,0,0]
[null,"C03200","P.B.F",null,"IND大理石切割",null,"孔",500,500,0,0]
[null,"C03300","P.B.F",null,"出入口地板切割不銹鋼復原",null,"停",1800,1800,0,0]
[null,"C03400","P.B.F",null,"新開出入口(含清潔)",null,"停",12000,12000,0,0]
[null,"C03500","P.B.F",null,"開門尺寸不足,昇降路牆面打溝",null,"停",1100,1100,0,0]
[null,"C03600","P.B.F",null,"出入口地板磨石子加銅條復原",null,"停",1200,1200,0,0]
[null,"C03700","P.B.F",null,"出入口地板大理石復原",null,"停",2300,2300,0,0]
[null,"C03800","P.B.F",null,"出入口地板PVC復原",null,"停",900,900,0,0]
[null,"C03900","P.B.F",null,"出入口三面修打",null,"停",3000,3000,0,0]
[null,"C04000","P.B.F",null,"門框三面大理石切割及修打",null,"停",2300,2300,0,0]
[null,"C04100","P.B.F",null,"出入口大理石脫落復原",null,"停",1500,1500,0,0]
[null,"C04200","P.B.F",null,"門內牆修打",null,"停",1500,1500,0,0]
[null,"C04300","P.B.F",null,"POCKET BRKT修打",null,"停",500,500,0,0]
[null,"C04400","P.B.F",null,"POCKET修打",null,"停",800,800,0,0]
[null,"D00400","P.B.F",null,"機坑隔開網－三台共用　　　　　　　　　　",null,"台",6800,6800,0,0]
[null,"D00500","P.B.F",null,"機坑防水工程　　　　　　　　　　　　　",null,"台",15000,15000,0,0]
[null,"D00600","P.B.F",null,"機坑超過深度回填  (30公分)                    ",null,"台",9000,9000,0,0]
[null,"D00700","P.B.F",null,"機坑超過深度回填  (60公分)                    ",null,"台",12000,12000,0,0]
[null,"D00800","P.B.F",null,"機坑處中間牆隔離板                    ",null,"台",3800,3800,0,0]
[null,"D01000","P.B.F",null,"機坑水泥台打除及清潔",null,"台",3800,3800,0,0]
[null,"D01100","P.B.F",null,"機坑防水工程(僅PIT底部或PIT局部)",null,"台",12000,12000,0,0]
[null,"D01200","P.B.F",null,"機坑防水PU工程",null,"台",12000,12000,0,0]
[null,"D01300","P.B.F",null,"機坑深度不足修打",null,"處",9000,9000,0,0]
[null,"D01500","P.B.F",null,"兩台以上電梯同機坑,PIT處中間磚牆隔離",null,"牆",9000,9000,0,0]
[null,"F00400","P.B.F",null,"彩色攝影機含人工費　　　　　　　",null,"台",22500,22500,0,0]
[null,"F00700","P.B.F",null,"電話配線至監控室　　　　　　　　　　　　",null,"台",3100,3100,0,0]
[null,"F00800","P.B.F",null,"雙控電鎖及配線工程費　　　　　　　　　　",null,"台",20500,20500,0,0]
[null,"F00900","P.B.F",null,"單控電鎖及配線（Ｈ.ＤＲ）　　　　　　　 ",null,"台",13600,13600,0,0]
[null,"F01000","P.B.F",null,"遠隔電話線按裝申請　　　　　　　　　　　",null,"台",8600,8600,0,0]
[null,"F01100","P.B.F",null,"昇降路配線槽配置（含材料費用）　　　　　",null,"停",8700,8700,0,0]
[null,"F01200","P.B.F",null,"機坑移動式抽水機",null,"台",5500,5500,0,0]
[null,"F01300","P.B.F",null,"它牌電梯聯動分割　　　　　　　　　　　　",null,"台",10200,10200,0,0]
[null,"F01400","P.B.F",null,"追加黑白隱藏式攝影機　　　　　　　　　　　　",null,"台",11600,11600,0,0]
[null,"F01500","P.B.F",null,"追加彩色隱藏式攝影機　　　　　　　　　　　　",null,"台",22500,22500,0,0]
[null,"F01600","P.B.F",null,"冷氣機開口",null,"孔",5500,5500,0,0]
[null,"F02800","P.B.F",null,"HU油壓用作動油　　　　　　　　　　　",null,"台",27300,27300,0,{"$f":"IF(I1039>0,(H1039-I1039)/I1039,-(H1039-I1039)/I1039)","v":0}]
[null,"F02900","P.B.F",null,"舊品拆除一台  BASE=6F                          ",null,"台",40900,40900,0,0]
[null,"F03000","P.B.F",null,"舊品拆除每增一停                            ",null,"停",2700,2700,0,0]
[null,"F03100","P.B.F",null,"監視器復原",null,"台",6800,6800,0,0]
[null,"G00100","P.B.F",null,"更新機房照明燈具(含人工及燈具)",null,"台",2000,2000,0,0]
[null,"G00200","P.B.F",null,"更新機房主電源開關壹台(75A以下)",null,"台",6100,6100,0,0]
[null,"G00300","P.B.F",null,"更新機房主電源開關壹台(75A以上)",null,"台",7500,7500,0,0]
[null,"G00400","P.B.F",null,"追加樓停(原不停止階且未留孔)",null,"停",21900,21900,0,0]
[null,"G00500","P.B.F",null,"更新SILL",null,"停",5300,5300,0,0]
[null,"G00600","P.B.F",null,"SILL整理",null,"停",300,300,0,0]
[null,"G00700","P.B.F",null,"小型門框更新",null,"停",10900,10900,0,0]
[null,"G00800","P.B.F",null,"T型門框更新",null,"停",21800,21800,0,0]
[null,"G00900","P.B.F",null,"更新車廂外法",null,"台",13800,13800,0,0]
[null,"G01200","P.B.F",null,"車廂更新Guide Shoe導靴",null,"台",2700,2700,0,0]
[null,"G01300","P.B.F",null,"A3改造車廂門及安全履更新(調整人工費)",null,"台",2700,2700,0,0]
[null,"G01400","P.B.F",null,"車廂及CWT ROPE END吊板更新",null,"台",5300,5300,0,0]
[null,"G01500","P.B.F",null,"H.DOOR追加介面鐵板",null,"停",300,300,0,0]
[null,"G01900","P.B.F",null,"幕板指示器切孔",null,"停",2000,2000,0,0]
[null,"G02000","P.B.F",null,"平衡鐵製作(KG)",null,"KG",100,100,0,0]
[null,"G02100","P.B.F",null,"機房地板修補",null,"台",4800,4800,0,0]
[null,"G02200","P.B.F",null,"機坑修補及清潔",null,"台",3400,3400,0,0]

{"sheet":"附表一","index":2,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,0,0,6],[2,3,2,6],[3,3,3,6],[4,3,4,6],[12,3,12,6],[5,3,5,6],[6,3,6,6],[7,3,7,6],[8,3,8,6],[9,3,9,6],[10,3,10,6],[11,1,11,6],[25,3,25,6],[13,3,13,4],[14,3,14,4],[15,3,15,4],[16,3,16,4],[17,3,17,4],[18,3,18,4],[19,3,19,4],[20,3,20,4],[21,3,21,6],[22,3,22,6],[24,3,24,6],[26,3,26,6],[27,3,27,6],[28,3,28,6],[29,3,29,6],[30,3,30,6]]}
["附   表   一"]
[]
[1,"型式（Type Form）",":","MAH100-6*5-2S*1台"]
[2,"載重（Load/Passenger）",":"," 450 公斤/ 6 人"]
[3,"停止樓數（No. of Stop）",":","  5  停／ 5  樓（1- 4,RF)（No.1)"]
[4,"速度（Speed）",":"," 45 m/min"]
[5,"控制方式（Control）",":","交流變壓變頻選擇性集合式控制"]
[6,"電源（Power Source）",":","動力用交流單相，220伏特，60Hz"]
[7,"出人口門框（Jamb）",":","標準門框：髮紋不鏽鋼"]
[8,"出人口門（Hatch Door）",":","彩妝鋼板或烤漆鋼板"]
[9,"出人口寬度（Opening）",":","800  mm× 2100  mm（W*H)"]
[10,"出人口指示燈及按鈕（Hall Indicator&Button）：MF001"]
[11,"梯廂型號（Cage）",":"]
[null,null,null,"a.、天花板型式（Ceiling Type）",null,":","MB010、MB013~015擇一"]
[null,null,null,"b、側板（Enclosure Wall)",null,":","前側側板：髮紋不鏽鋼"]
[{"$nulls":6},"兩側：彩妝鋼板或烤漆鋼板"]
[null," ",{"$nulls":4},"後側：彩妝鋼板或烤漆鋼板"]
[null,null,null,"c、廂門（Cage Door)",null,":","彩妝鋼板或烤漆鋼板"]
[null,null,null,"d、地板（Flooring)",null,":","標準塑膠地磚或預留大理石貼附厚度"]
[null,null,null,"e、換氣（Ventilation)",null,":","天花板扇（Ceiling Fan)"]
[null,null,null,"f、操作盤（Operating Panel）",null,":","ME016"]
[12,"警報方式（Alarm）",":","g、梯廂位置指示器（Car Position Indicator)：附於OPB上"]
[null,null,null,"電鈴及對講機（Bell & Interphone）"]
[13,"升降路尺寸及各層樓高度（Hoist Way & Each Floor Height）：依計劃圖（As Per Layout Drawing）"]
[14,"其他（Other）",":"]