{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["部品計劃表","工作表1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"部品計劃表","index":0,"n_rows":74,"n_cols":17,"rows_kept":74,"cut":false,"hidden":false,"merged":[[69,12,69,14],[70,10,73,10],[70,11,73,11],[70,12,73,14],[45,9,52,9],[54,9,60,9],[67,10,67,14],[62,10,62,14],[63,10,63,14],[64,10,64,14],[65,10,65,14],[66,10,66,14],[11,9,28,9],[29,9,33,9],[34,9,44,9],[5,0,73,0],[5,1,52,1],[54,1,73,1],[5,8,52,8],[54,8,60,8],[62,8,62,9],[7,9,8,9],[9,9,10,9],[0,0,0,14],[4,0,4,1],[1,0,1,1],[2,0,2,1],[3,0,3,1],[4,8,4,9],[1,2,1,3],[2,2,2,3],[3,2,3,3]]}
["永佳捷出貨部品計畫表"]
["案件名稱",null,"金寶城糖業股份有限公司"]
["案件編號",null,"3MH00266"]
["預計出貨日",null,"2023.12.20"]
["品目區分",null,"部件名稱","規格 / 圖號說明","P社手配","M社手配","見特記",null,"品目區分",null,"部件名稱","規格 / 圖號說明","P社手配","M社手配","見特記"]
["轎廂部分","轎架&\n對重框箱","上樑(平頂式轿顶轮梁阻立)",null,"●",null,null,null,"井道部分","配重","對重塊 (裸装)","比重3.5 (35KG)","●"]
[null,null,"立樑左組件",null,"●"]
[null,null,"立樑右組件",null,"●",{"$nulls":4},"導軌","轎廂導軌(含連接板)",null,"●"]
[null,null,"轎頂檢修停止總裝圖",null,"●",{"$nulls":5},"配重導軌(含連接板)",null,"●"]
[null,null,"下樑",null,"●",{"$nulls":4},"鋼絲繩","曳引機鋼絲繩",null,"●"]
[null,null,"滑動導靴",null,"●",{"$nulls":5},"限速器鋼絲繩",null,"●"]
[null,null,"安全钳装置",null,"●",{"$nulls":4},"電氣部\n品"]
[null,null,"極限開關支架",null,"●",{"$nulls":5},"極限開關",null,"●"]
[null,null,"隔磁板",null,"●",{"$nulls":5},"井道照明燈",null,"●"]
[null,null,"平層光電支架",null,"●",{"$nulls":5},"聲光警報器",null,"●"]
[null,null,"随行電纜支架",null,"●",{"$nulls":5},"平層光電開關",null,"●"]
[null,null,"撞弓组件",null,"●",{"$nulls":5},"模擬量秤重傳感器",null,"●"]
[null,null,"對重架+對重導靴",null,"●"]
[null,null,"井道電纜架組件",null,"●"]
[]
[null,null,"對重防護欄","依現行法規不手配",{"$nulls":6},"ARD (含電池)","NP7-12 (12V,7.0AH) *2顆",null,"●"]
[null,null,"檢修停車檔板",null,"●",{"$nulls":5},"底坑檢修箱(含五方通话)",null,"●"]
[null,null,"主機機械台安裝组件",null,"●",{"$nulls":5},"固定电纜",null,"●"]
[null,null,"主機座焊組件",null,"●",{"$nulls":5},"随行电纜",null,"●"]
[null,null,"主機减震墊",null,"●",{"$nulls":5},"動力線",null,"●"]
[null,null,"張緊輪",null,"●",{"$nulls":5},"電氣輔料",null,"●"]
[null,null,"限速器",null,"●"]
[null,null,"限速器底座/(含入轎廂側繩頭)",null,"●"]
[null,null,"轎廂油杯組裝",null,"●"]
[null,null,"對重油杯",null,"●",{"$nulls":4},"門機","門機",null,"●"]
[null,null,"轎廂導軌壓導板",null,"●",{"$nulls":5},"門控器",null,"●"]
[null,null,"配重導軌壓導板",null,"●",{"$nulls":5},"轎廂地坎","AL材质","●"]
[null,null,"轎廂導軌支架","由現地工務手配","●"]
[null,null,"對重導軌支架","由現地工務手配","●"]
[null,null,"缓衝器加高台",null,"●",{"$nulls":4},"門頭","電梯鑰匙",null,"●",null,null,null,"  "]
[null,null,"缓衝器",null,"●",{"$nulls":5},"重錘組件",null,"●"]
[null,null,"缓衝器座板",null,"●",{"$nulls":5},"層门装置",null,"●"]
[null,null,"缓衝器枕墊",null,"●"]
[null,null,"集油盒",null,"●"]
[null,null,"導軌油",null,"●",{"$nulls":5},"層門支架散件包",null,"●"]
[null,null,"轎廂導軌座",null,"●",{"$nulls":5},"地坎支架散件包",null,"●"]
[null,null,"對重導軌座"]
[{"$nulls":10},"層門護腳板"]
[null,null,"對重繩頭","繩頭無縫鋼管直吊型","●"]
[null,null,"轎廂繩頭组件","繩頭無縫鋼管直吊型","●",{"$nulls":5},"地坎组件","AL材质","●"]
[null,null,"秤重装置",null,"●",{"$nulls":4},"門板"]
[null,null,"轎頂護板",null,"●",{"$nulls":5},"光幕装置","赛福特","●"]
[null,null,"電纜防鈎線安裝",null,"●",{"$nulls":5},"小門套 YL01022A-A02/A03","JJ=800x2100 ; A111","●"]
[null,null,"斜支撐组件","標配","●",{"$nulls":5},"轎門板",null,null,null,"●"]
[null,null,"轿架螺絲包(含膨脹螺栓",null,"●",{"$nulls":5},"大門套 (0°斜角) YL05006A-A02","JJ=800x2100 A=220 ; A111","●"]
[null,null,"固定式轎頂安全欄杆","高度750","●",{"$nulls":5},"層门板",null,null,null,"●"]
[null,null,"水平連動同步桿",null,"●"]
[null,null,"提拉杆",null,"●"]
[null,null,"底坑爬梯",null,"●",{"$nulls":4},"主機箱","曳引機",null,"●"]
[null,"轎底 & 轎壁\n","轎頂組件",null,"●",null,null,null,"機房部分","控制箱","轎頂檢修盒(轎頂板，24V电源盒）","默纳克NICE3000+(CTW-B3S)","●"]
[null,null,"隨機文件",null,"●",{"$nulls":5},"操作盤 COP"]
[null,null,"轎頂卡板",null,"●",{"$nulls":5},"乘場指示器"]
[null,null,"轎頂安全窗及開關",null,"●",{"$nulls":5},"控制櫃","NICE3000-W-2015S-B 15kw","●"]
[null,null,"轎底组件 (含轎廂地砍支架)",null,"●",{"$nulls":5},"機房對講主機","MBT-MI-A1","●"]
[null,null,"床地板",null,"●",{"$nulls":5},"主機急停盒","MBT-MSB-D3","●"]
[null,null,"固定式護腳板組件",null,"●",{"$nulls":5},"急停開關盒(第三代)","MBT-PSB-A12","●"]
[null,null,"踢脚板 (含入轎底)",null,"●"]
[null,null,"天花组件",null,"●",null,null,null,"特記說明",null," (1) 轎門板及層門板透視窗採用5t強化玻璃，不需凸台 (可接受板厚段差)，此由P社提供。"]
[null,null,"風扇組裝",null,"●"]
[null,null,"扶手",null,"●"]
[null,null,"門楣板",null,"●"]
[null,null,"組立螺絲包",null,"●"]
[null,null,"出入口擋板",null,"●"]
[null,null,"前側板",null,"●"]
[null,null,"側面兩端壁",null,"●",{"$nulls":6},"確認","作成"]
[null,null,"左側中間壁",null,"●"]
[null,null,"右面中間壁",null,"●"]
[null,null,"後側兩端壁",null,"●"]
[null,null,"後側中間壁",null,"●"]

{"sheet":"工作表1","index":1,"n_rows":2,"n_cols":2,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
[]
[null,"●"]