{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["目錄","A-1車廂意匠","A-2車廂內裝","A-3車廂外部","A-4控制與其他"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"目錄","index":0,"n_rows":5,"n_cols":1,"rows_kept":5,"cut":false,"hidden":false,"merged":[[0,0,0,1]]}
["目錄"]
["A-1車廂意匠"]
["A-2車廂內裝"]
["A-3車廂外部"]
["A-4控制與其他"]

{"sheet":"A-1車廂意匠","index":1,"n_rows":12,"n_cols":8,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,7]]}
["A-1 車廂意匠"]
["序號","名稱","編號","規格/備註","配置","成本(NT)","定價","單位"]
[1,"車廂意匠","MA002","吊頂：MB005(鑽石銀烤漆+發紋不銹鋼+乳白透光板)\n兩側側板：彩妝鋼板ML001+彩妝鋼板ML002\n後側側板：彩妝鋼板ML001+彩妝鋼板ML002\n前側側板：發紋不銹鋼\n轎門：彩妝鋼板ML002\n地板：PVC(MD001)","標配",8527.68,0,"台"]
[2,"車廂意匠","MA006","吊頂：MB010(鏡面不銹鋼、透光軟膜)\n兩側側板：鏡面不銹鋼蝕刻鍍黑鈦\n後側側板：鏡面不銹鋼鍍黑鈦+彩妝鋼板 ML005\n前側側板：鏡面不銹鋼鍍黑鈦\n轎門：鏡面不銹鋼蝕刻鍍黑鈦\n地板：大理石(MD011)","選配",67840.125724644298,120000,"台"]
[3,"車廂意匠","MA005","吊顶：MB009(钻石银烤漆+乳白透光板)\n两侧侧板：彩妆钢板ML002\n后侧侧板：发纹不锈钢+镜面不锈钢\n前侧侧板：发纹不锈钢\n轿门：彩妆钢板ML002\n地板：PVC(MD001)","選配",1532.0237777284799,16000,"台"]
[4,"車廂意匠","MA007","吊顶：MB012(镜面不锈钢、乳白透光板)\n两侧侧板：发纹不锈钢+镜面不锈钢\n后侧侧板：发纹不锈钢+镜面不锈钢\n前侧侧板：发纹不锈钢\n轿门：发纹不锈钢\n地板：PVC(MD005)","選配",12502.538739821835,33600,"台"]
[5,"車廂意匠","MA008","吊顶：MB011(镜面不锈钢镀黑钛、乳白透光板)\n两侧侧板：镜面不锈钢镀黑钛+防火板\n后侧侧板：镜面不锈钢镀黑钛+防火板\n前侧侧板：镜面不锈钢镀黑钛\n轿门：镜面不锈钢镀黑钛\n地板：PVC(MD013)","選配",0,150000,"台"]
[6,"車廂意匠","MA017","吊顶：MB010(RAL9005砂纹+乳白透光板)\n两侧侧板：烤漆RAL9003砂纹+镜面不锈钢镀黑钛\n后侧侧板：烤漆RAL9003砂纹+镜面不锈钢镀黑钛\n前侧侧板：烤漆RAL9003砂纹\n轿门：烤漆RAL9003砂纹\n地板：PVC(MD005)","選配",2640.96,27300,"台"]
[7,"車廂意匠","MA018","吊顶：MB013(RAL9003砂纹+LED灯板)\n两侧侧板：烤漆RAL9005砂纹+烤漆RAL9003砂纹+\n          镜面不锈钢镀黑钛\n后侧侧板：烤漆RAL9003砂纹+镜面不锈钢镀黑钛\n前侧侧板：烤漆RAL9003砂纹\n轿门：烤漆RAL9003砂纹\n地板：PVC(MD005)","選配",0,10000,"台"]
[8,"車廂意匠","MA019","吊顶：MB014(RAL9003砂纹+LED灯板)\n两侧侧板：彩妆钢板ML002+镜面不锈钢\n后侧侧板：彩妆钢板ML002+镜面不锈钢\n前侧侧板：发纹不锈钢\n轿门：彩妆钢板ML002\n地板：PVC(MD006)","標配",17842.5,36000,"台"]
[9,"車廂意匠","MA020","吊顶：MB015(烤漆RAL1015+烤漆RAL9005+\n      LED方灯)\n两侧侧板：彩妆钢板ML006\n后侧侧板：彩妆钢板ML006+镜面饰条\n前侧侧板：发纹不锈钢\n轿门：彩妆钢板ML006\n地板：PVC(MD001)","標配",19651.5,40000,"台"]
[10,"車廂意匠","MA021","吊顶：MB011(镜面不锈钢镀黑钛+乳白透光板)\n两侧侧板：镜面不锈钢镀黑钛+蚀刻香槟金镀色\n后侧侧板：镜面不锈钢镀黑钛+蚀刻香槟金镀色\n前侧侧板：镜面不锈钢镀黑钛\n轿门：镜面不锈钢镀黑钛\n地板：PVC(MD006)","選配",45692.639999999999,92000,"台"]

{"sheet":"A-2車廂內裝","index":2,"n_rows":201,"n_cols":9,"rows_kept":201,"cut":false,"hidden":false,"merged":[[0,0,0,8],[140,1,145,1],[146,1,151,1],[133,1,134,1],[94,1,101,1],[102,1,111,1],[115,1,122,1],[123,1,132,1]]}
["A-2 車廂內裝"]
["序號","名稱","編號","規格/備註","配置",null,"成本(NT)","定價","單位"]
["A-2-1天井"]
[1,"天井","MB001","黑色烤漆、乳白透光板","標配",null,1440,5000,"台"]
[2,"天井","MB002","黑色烤漆、乳白透光板","標配",null,1438.4393541501165,5000,"台"]
[3,"天井","MB003","烤漆鋼板、深灰烤漆鋼板、LED方燈","標配",null,0,null,"台"]
[4,"天井","MB004","香檳色烤漆鋼板、乳白透光板、筒燈","標配",null,1400.0485685259646,2800,"台"]
[5,"天井","MB005","鑽石銀烤漆鋼板邊框、發紋不銹鋼、乳白透光板、筒燈","選配",null,5203.4237003112748,10500,"台"]
[6,"天井","MB006","鏡面不銹鋼、乳白透光板","選配",null,4676.1646505490453,10000,"台"]
[7,"天井","MB007","黑色烤漆鋼板邊框、黑鈦鏡面不銹鋼、乳白透光板、筒燈","選配",null,6145.9174873843649,13000,"台"]
[8,"天井","MB008","鑽石銀烤漆鋼板邊框、鏡面不銹鋼、乳白透光板、筒燈","選配",null,6145.9174873843649,13000,"台"]
[9,"天井","MB009","鑽石銀烤漆鋼板、乳白透光板","選配",null,4006.4048561946911,8400,"台"]
[10,"天井","MB010","鏡面不銹鋼、透光軟膜","選配",null,23924.241924541471,45000,"台"]
[11,"天井","MB011","鏡面不銹鋼鍍黑鈦、乳白透光板","選配",null,20217.992217850304,45000,"台"]
[12,"天井","MB012","鏡面不銹鋼、乳白透光板","標配",null,4006.4048561946911,8400,"台"]
[13,"天井","MB002","SUS304-1.2t發紋不銹鋼（標準：依巨龍標準）","加價",null,4006.4048561946911,8400,"台"]
[14,"天井","MB009","SUS304-1.3t發紋不銹鋼（標準：依巨龍標準）","加價",null,4006.4048561946911,8400,"台"]
[15,"天井","MB003","SUS304-1.4t發紋不銹鋼（標準：依巨龍標準）","加價",null,7251.4115044248147,12500,"台"]
[16,"天井","MB001","SUS304-1.5t發紋不銹鋼（標準：依巨龍標準）","加價",null,4006.4048561946911,8400,"台"]
[17,"天井","MB004","SUS304-1.6t發紋不銹鋼（標準：依巨龍標準）","加價",null,5628.9081803097597,9500,"台"]
[18,"天井","MB002","材質-SUS304-1.5t發紋不銹鋼\n（標準：依巨龍標準）","加價",null,4927.8779731194754,9500,"台"]
[19,"天井","MB009","材質-SUS304-1.6t發紋不銹鋼\n（標準：依巨龍標準）","加價",null,4927.8779731194754,9500,"台"]
[20,"天井","MB003","材質-SUS304-1.7t發紋不銹鋼\n（標準：依巨龍標準）","加價",null,8919.2361504424953,15500,"台"]
[21,"天井","MB001","材質-SUS304-1.8t發紋不銹鋼\n（標準：依巨龍標準）","加價",null,4927.8779731194754,9500,"台"]
[22,"天井","MB004","材質-SUS304-1.9t發紋不銹鋼\n（標準：依巨龍標準）","加價",null,6923.5570617809854,12500,"台"]
[23,"天井","MB002","材質-SUS304-1.5t鏡面不銹鋼\n（標準：依巨龍標準）","加價",null,5363.41587660396,11500,"台"]
[24,"天井","MB009","材質-SUS304-1.6t鏡面不銹鋼\n（標準：依巨龍標準）","加價",null,5363.41587660396,11500,"台"]
[25,"天井","MB003","材質-SUS304-1.7t鏡面不銹鋼\n（標準：依巨龍標準）","加價",null,9698.7628871681391,17500,"台"]
[26,"天井","MB001","材質-SUS304-1.8t鏡面不銹鋼\n（標準：依巨龍標準）","加價",null,5363.41587660396,11500,"台"]
[27,"天井","MB004","材質-SUS304-1.9t鏡面不銹鋼\n（標準：依巨龍標準）","加價",null,7042.9334236725599,12500,"台"]
["A-2-2地板"]
[28,"地板","MD001","PVC","標配",null,0,null,"台"]
[29,"地板","MD002","PVC","標配",null,0,null,"台"]
[30,"地板","MD003","PVC","標配",null,0,null,"台"]
[31,"地板","MD004","PVC","選配",null,2720.7295964601794,5200,"台"]
[32,"地板","MD005","PVC","選配",null,2720.7295964601794,5200,"台"]
[33,"地板","MD006","PVC","選配",null,2720.7295964601794,5200,"台"]
[34,"地板","MD007","PVC","選配",null,2720.7295964601794,5200,"台"]
[35,"地板","MD008","PVC","選配",null,2720.7295964601794,5200,"台"]
[36,"地板","MD009","PVC","選配",null,1999.158371681418,4200,"台"]
[37,"地板","MD010","PVC","選配",null,3147.112592920359,6500,"台"]
[38,"地板","MD011","大理石","選配",null,16910.073744807556,35000,"台"]
[39,"地板","MD012","大理石","選配",null,16910.073744807556,35000,"台"]
[40,"地板地磚貼付BY業主","客梯","P6~P24人 ",null,null,null,0,"台"]
[41,"地板 花紋不鏽鋼板 ","客梯","P6~P13人 (一片式)",null,null,{"$f":"H45*0.6","v":13080},21800,"台"]
[42,"地板 花紋不鏽鋼板 ","客梯","P15人 (一片式)",null,null,{"$f":"H46*0.6","v":15060},25100,"台"]
[43,"地板 花紋不鏽鋼板 ","客梯","P17~P24人 (僅接合式)",null,null,23220,38700,"台"]
[44,"地板_大理石貼付預留","小電梯","P6~P8人",null,null,6000,10000,"台"]
[45,"地板_大理石貼付預留","客梯","P9人",null,null,9000,15000,"台"]
[46,"地板_大理石貼付預留","客梯","P10人(10停)(120M(含)以下)",null,null,23580,39300,"台"]
[47,"地板_大理石貼付預留","客梯","P11人(10停)(120M(含)以下)",null,null,24240,40400,"台"]
[48,"地板_大理石貼付預留","客梯","P12~15人(10停)(60~105m)",null,null,21780,36300,"台"]
[49,"地板_大理石貼付預留","客梯","P17人(60~105m)",null,null,8940,14900,"台"]
[50,"地板_大理石貼付預留","客梯","P20~24人(任何速度)",null,null,9420,15700,"台"]
[51,"地板_大理石貼付預留","客梯","P13人(120M)",null,null,8520,14200,"台"]
[52,"地板_大理石貼付預留","客梯","P15人(20停)(120M)",null,null,75840,126400,"台"]
[53,"地板_大理石貼付預留","客梯","P17人(120M)",null,null,8280,13800,"台"]
[54,"地板_大理石貼付預留","客梯","P13~17人(150M)",null,null,9240,15400,"台"]
[55,"地板_石英磚貼付預留(10mm)","客梯","P6~P24人 ",null,null,6540,10900,"台"]
[56,"地板_大理石貼付預留","客梯","P6~P24人(無機房用)",null,null,6120,10200,"台"]
[57,"地板 花紋不鏽鋼板 (SH)","貨梯","1000kg以內 ",null,null,13680,22800,"台"]
[58,"地板 花紋不鏽鋼板 (SH)","貨梯","1500~2000kg ",null,null,30900,51500,"台"]
[59,"地板 花紋不鏽鋼板 (SH)","貨梯","2500~3000kg ",null,null,64380,107300,"台"]
[60,"地板_車廂地毯(P-11人(含)以下)","客梯",null,null,null,2040,3400,"台"]
[61,"地板_車廂地毯(P-12人(含)以上)","客梯",null,null,null,2460,4100,"台"]
[62,"地板_3M地毯(P-11人(含)以下)","客梯",null,null,null,2460,4100,"台"]
[63,"地板_3M地毯(P-12人(含)以上)","客梯",null,null,null,3300,5500,"台"]
["A-2-3操縱盤"]
[64,"操縱盤","ME001","主操縱盤","標配",null,0,null,"台"]
[65,"操縱盤","ME002","主操縱盤","選配",null,0,2500,"台"]
[66,"操縱盤","ME003","主操縱盤","選配",null,57.982300884955805,2500,"台"]
[67,"操縱盤","ME004","主操縱盤","選配",null,151.64601769911465,2500,"台"]
[68,"操縱盤","ME005","主操縱盤在ME001基礎上追加語音呼梯","選配",null,2029.3805309734485,3990,"台"]
[69,"操縱盤","ME006","側邊一體式操縱盤","選配",null,4370.9734513274352,8820,"台"]
[70,"操縱盤","ME007","側邊一體式操縱盤在ME006基礎上追加盲文點字板","選配",null,4518.1592920354051,9030,"台"]
[71,"操縱盤","ME008","一體式前側板用","選配",null,4616.2831858406998,9240,"台"]
[72,"操縱盤","ME009","一體式前側板用在ME008基礎上追加盲文點字板","選配",null,4767.84,9600,"台"]
[73,"操縱盤","ME010","外掛式殘障用","選配",null,4089.9823008849539,8300,"台"]
[74,"操縱盤","ME011","嵌入式殘障用","選配",null,4140.382300884954,8800,"台"]
[75,"操縱盤","ME012","外掛式附顯示殘障用","選配",null,4971.9823008849453,10000,"台"]
[76,"操縱盤","ME013","嵌入式附顯示殘障用","選配",null,4921.5823008849457,10000,"台"]
[77,"操縱盤","ME014","在ME002基礎上追加盲文點字板","選配",null,154.9911504424779,1000,"台"]
[78,"操縱盤","ME015","在ME003基礎上追加盲文點字板","選配",null,54.191150442477003,3500,"台"]
[79,"操縱盤","ME016","在ME001基礎上追加電話機鍵盤","選配",null,1033.2,2500,"台"]
[80,"操縱盤","ME017","在ME002基礎上追加電話機鍵盤","選配",null,1036.9911504424815,2500,"台"]
[81,"操縱盤","ME018","在ME003基礎上追加電話機鍵盤","選配",null,1087.3911504424814,3500,"台"]
["A-2-4扶手"]
[82,"扶手","MC001","不銹鋼扁平扶手","選配",null,1789.4230088495578,3500,"支"]
[83,"扶手","MC002","不銹鋼圓形扶手","選配",null,1342.0672566371684,3500,"支"]
[84,"扶手","MC003","不銹鋼彎管扶手","選配",null,1789.4230088495578,3500,"支"]
[85,"扶手","MC004","不銹鋼紅木扶手","選配",null,2236.7787610619475,5000,"支"]
[86,"扶手","MC005","鏡面黑鈦扶手","選配",null,2268,7000,"支"]
["A-2-5 車廂門與層門(轎門/層門)"]
[87,"轎門2100mm （標準：噴塗或彩粧鋼板）",null,"SUS304-1.5t發紋不銹鋼","加價",null,2754,5200,"停"]
[88,"轎門2100mm\n（標準：噴塗或彩粧鋼板）",null,"SUS304-1.2t發紋不銹鋼","加價",null,2292,4800,"停"]
[89,null,null,"SUS304-1.5t發紋不銹鋼 鍍鈦","加價",null,7106.3343716814179,11000,"停"]
[90,null,null,"SUS304-1.5t鏡面不銹鋼","加價",null,3110.9925663716817,9470,"停"]
[91,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",null,7590.6542867256449,13250,"停"]
[92,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",null,6517.2966371681441,13250,"停"]
[93,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",null,8775.2746194690153,16500,"停"]
[94,null,null,"四周包邊玻璃轎門SUS304-1.2t發紋不銹鋼","加價",null,12343.380530973482,30500,"停"]
[95,null,null,"四周包邊玻璃轎門SUS304-1.5t鏡面不銹鋼","加價",null,15376.300884955755,39500,"停"]
[96,"層門2100mm\n（標準：噴塗Q235A-1.5t）",null,"SUS304-1.5t發紋不銹鋼","加價",null,3396.7842690265516,5200,"停"]
[97,null,null,"噴塗Q235A-1.2t","加價",null,-239.05752212389365,0,"停"]
[98,null,null,"SUS304-1.2t發紋不銹鋼","加價",null,2729.2081699115056,4500,"停"]
[99,null,null,"SUS304-1.5t發紋不銹鋼 鍍鈦","加價",null,6224.1653946902406,9500,"停"]
[100,null,null,"SUS304-1.5t鏡面不銹鋼","加價",null,3527.6815433628312,7800,"停"]
[101,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",null,6708.4853097344849,12000,"停"]
[102,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",null,5654.76225132744,12000,"停"]
[103,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",null,7893.1056424778544,15000,"停"]
[104,null,null,"四周包邊玻璃層門SUS304-1.2t發紋不銹鋼","加價",null,15610.619469026518,29000,"停"]
[105,null,null,"四周包邊玻璃層門SUS304-1.5t鏡面不銹鋼","加價",null,21587.256637168182,38000,"停"]
[106,"廂門/層門加高200(標準：SUS304-1.5t發紋不銹鋼，高：2100)",null,"SUS304-1.2t發紋不銹鋼","加價",null,-212.49557522123894,2500,"台"]
[107,"廂門/層門加高200(標準：SUS304-1.5t發紋不銹鋼，高：2100)",null,"SUS304-1.5t發紋不銹鋼","加價",null,392.69182300884944,2500,"台"]
[108,"轎門2300mm （標準：噴塗或彩粧鋼板）",null,"SUS304-1.5t發紋不銹鋼","加價",null,3147,7700,"停"]
[109,"轎門2300mm\n（標準：噴塗或彩粧鋼板）",null,"SUS304-1.2t發紋不銹鋼","加價",null,2685,7300,"停"]
[110,null,null,"SUS304-1.5t發紋不銹鋼 鍍鈦","加價",null,7499,13500,"停"]
[111,null,null,"SUS304-1.5t鏡面不銹鋼","加價",null,3531,11970,"停"]
[112,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",null,8011,15750,"停"]
[113,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",null,6910,15750,"停"]
[114,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",null,9168,19000,"停"]
[115,null,null,"四周包邊玻璃轎門SUS304-1.2t發紋不銹鋼","加價",null,12736,33000,"停"]
[116,null,null,"四周包邊玻璃轎門SUS304-1.5t鏡面不銹鋼","加價",null,15769,42000,"停"]
[117,"層門2300mm\n（標準：噴塗Q235A-1.5t）",null,"SUS304-1.5t發紋不銹鋼","加價",null,3396.7842690265516,7700,"停"]
[118,null,null,"噴塗Q235A-1.2t","加價",null,3158,0,"停"]
[119,null,null,"SUS304-1.2t發紋不銹鋼","加價",null,6126.208169911506,7000,"停"]
[120,null,null,"SUS304-1.5t發紋不銹鋼 鍍鈦","加價",null,9621.1653946902406,12000,"停"]
[121,null,null,"SUS304-1.5t鏡面不銹鋼","加價",null,6924.6815433628308,10300,"停"]
[122,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",null,10105.485309734486,14500,"停"]
[123,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",null,9051.76225132744,14500,"停"]
[124,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",null,11290.105642477854,17500,"停"]
[125,null,null,"四周包邊玻璃層門SUS304-1.2t發紋不銹鋼","加價",null,19007.619469026518,31500,"停"]
[126,null,null,"四周包邊玻璃層門SUS304-1.5t鏡面不銹鋼","加價",null,24984.256637168182,40500,"停"]
[127,"臨時層門",null,"冷軋板噴塗1.2t高度：2100","加價",null,1498.7737911504421,5200,"停"]
[128,null,null,"冷軋板噴塗1.2t高度：2300","加價",null,1590.4018831858425,5400,"停"]
[129,"追加臨時廂門 (烤漆)",null,"冷軋板噴塗1.2t高度：2100","加價",null,{"$f":"H136*0.6","v":3120},5200,"台"]
[130,"追加臨時廂門 (烤漆)",null,"冷軋板噴塗1.2t高度：2300","加價",null,{"$f":"H137*0.6","v":3240},5400,"台"]
[131,"廂門層門加高200(標準：噴塗Q235A-1.5t)",null,"冷軋板噴塗1.2t","加價",null,-148.7469026548674,2500,"停"]
[132,"廂門層門加高200(標準：噴塗Q235A-1.5t)",null,"冷軋板噴塗1.5t","加價",null,130.89727433628315,2500,"停"]
["A-2-6 轎壁(車廂側板)"]
[133,"轎壁_P6-P9人乘\n（前側+左右側+後側+車廂門）\n（標準：烤漆/彩妝）\n",null,"SUS304-1.5t 髮紋不銹鋼",null,null,{"$f":"H133*0.6","v":24300},25200]
[134,null,null,"SUS304-1.5t 髮紋不銹鋼 鍍鈦",null,null,{"$f":"H134*0.6","v":3120},57750]
[135,null,null,"SUS304-1.5t鏡面不銹鋼","加價",null,1570.7672920353959,40000,"台"]
[136,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",null,14856.840637168139,66000,"台"]
[137,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",null,13393.171115044244,53000,"台"]
[138,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",null,20187.929628318554,86000,"台"]
[139,"轎壁_大梯\n（前側+左右側+後側+車廂門）\n（標準：烤漆/彩妝）",null,"SUS304-1.5t 髮紋不銹鋼","加價",null,{"$f":"H147*0.6","v":16695},27825]
[140,null,null,"SUS304-1.5t 髮紋不銹鋼 鍍鈦","加價",null,{"$f":"H148*0.6","v":54180},90300]
[141,null,null,"SUS304-1.5t鏡面不銹鋼","加價",null,35280,58800]
[142,null,null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",null,57600,96000]
[143,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",null,44730,74550]
[144,null,null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",null,71190,118650]
[145,"轎廂淨高加高200（含加重） （標準：SUS304-1.5t發紋不銹鋼，淨高：2300）",null,"SUS304-1.5t發紋不銹鋼","加價",null,2772,4620,"停"]
[146,"車廂特殊裝潢\n（標準：SUS304-1.5t發紋不銹鋼，淨高：2300）",null,"3側板中間片鏡面不銹鋼SUS304-1.5t，\n其中後側板鏡面不銹鋼SUS304-1.5t需及閘同寬","加價",null,13250.374088495581,22000,"台"]
[147,"側板單片特殊(烤漆→不鏽鋼)",null,"(烤漆→不鏽鋼髮紋)",null,null,{"$f":"H155*0.6","v":3300},5500,"片"]
[148,"側板單片特殊(烤漆→不鏽鋼)",null,"(烤漆→鏡面不鏽鋼)",null,null,{"$f":"H156*0.6","v":3900},6500,"片"]
[149,"側板單片特殊",null,"(烤漆→不鏽鋼髮紋 鍍鈦)",null,null,4440,7400,"片"]
[150,"側板單片特殊",null,"(烤漆→鏡面 不鏽鋼 鍍鈦)",null,null,5220,8700,"片"]
[151,"側板單片特殊",null,"(烤漆→鏡面 不鏽鋼 蝕刻)",null,null,6120,10200,"片"]
[152,"車廂前側 RT PANEL(髮紋不鏽鋼)",null,"P6~24人(不含廂門)",null,null,4200,7000,"台"]
[153,"車廂前側 RT PANEL(髮紋不鏽鋼鍍鈦)",null,"P6~24人(不含廂門)",null,null,10680,17800,"台"]
[154,"車廂前側 RT PANEL(鏡面不鏽鋼)",null,"P6~24人(不含廂門)",null,null,8460,14100,"台"]
[155,"OPB(前)側&CPI  烤漆→髮紋不鏽鋼",null,"P6~24人(不含廂門)",null,null,4440,7400,"台"]
[156,"OPB(前)側&CPI 烤漆→仿鍍鈦",null,"P6~24人(不含廂門)",null,null,3360,5600,"台"]
["A-2-7 其他車廂內裝配件"]
[157,"二合一光幕(標準門高2100)",null,null,"加價",null,4906.1946902654699,11000,"台"]
[158,"紫外線殺菌燈（型號：TL-16W）P社已有",null,null,"加價",null,2217.6,5700,"個"]
[159,"風扇出風口",null,null,"加價",null,252,1500,"台"]
[160,"SHARP清淨機（臺灣）",null,null,"加價",null,27512,45000,"台"]
[161,"冷氣（臺灣）",null,null,"加價",null,38024,95000,"套"]
[162,"副操作盤",null,null,"加價",null,5095.4399999999996,13000,"套"]
[163,"語音合成裝置",null,"語音報站器","加價",null,1033.2,4200,"套"]
[164,"車廂攝影機",null,null,"加價",null,1338.0530973451337,12000,"套"]
[165,"CCTV配線預留",null,"5C FV線材(標準)","加價",null,null,13000,"台"]
[166,"無線遠端對講系統",null,null,"加價",null,3978,7500,"套"]
[167,"殘障電梯(殘障OPB、殘障IND、殘障扶手、後側鏡面、語音合成)",null,"二、超過十層樓之各層樓地板面積之和達500平方公尺者需設置。","加價",null,7627.5,35000,"套"]
[168,"開門延長",null,"三、超過十層樓之部分為樓梯間、昇降機間、機械室、裝飾塔、屋頂窗及其他類似用途之建築物不需設置。","加價",null,80.64,1000,"套"]
[169,"刷卡機系統",null,"MCTC-IC-A2","加價",null,4430.16,12000,"套"]
[170,"多媒體屏",null,"13寸","加價",null,14616,53000,"套"]
[171,"車廂側板附壁鉤",null,"P6~P24人","加價",null,{"$f":"H180*0.6","v":6000},10000,"台"]
[172,"側板附壁鉤及保護掛毯(牛仔布)",null,"P6~P12人","加價",null,{"$f":"H181*0.6","v":16620},27700,"台"]
[173,"側板附壁鉤及保護掛毯(牛仔布)",null,"P13~P20人","加價",null,19080,31800,"台"]
[174,"側板附壁鉤及保護掛毯(牛仔布)",null,"P24人","加價",null,21540,35900,"台"]
[175,"明鏡嵌入式(僅車廂後側)預留10mm",null,"P6~P24人(不包含鏡子,單純因應側板特殊所需加工及設計費)","加價",null,4860,8100,"台"]
[176,"明鏡嵌入式(車廂三側)預留10mm",null,"P6~P24人(不包含鏡子,單純因應側板特殊所需加工及設計費)","加價",null,9600,16000,"台"]
[177,"凸面鏡",null,"千鳥,展望有殘障時加計","加價",null,960,1600,"面"]
[178,"半身明鏡　　　　　　　　　　",null,null,"加價",null,3480,5800,"面"]
[179,"中間片全身明鏡　　　",null,null,"加價",null,4740,7900,"面"]
[180,"車廂內法特殊",null,"客梯P6~P24人","加價",null,10200,17000,"台"]
[181,"車廂內法特殊",null,"貨梯-1000kg~2000kg","加價",null,16800,28000,"台"]
[182,"車廂內法特殊",null,"貨梯-2500kg~3000kg","加價",null,21000,35000,"台"]
[183,"車廂附防撞板  不鏽鋼",null,"P6~P12人","加價",null,16200,27000,"台"]
[184,"車廂附防撞板  不鏽鋼",null,"P13~P17人","加價",null,20400,34000,"台"]
[185,"車廂附防撞板  不鏽鋼",null,"P20~P24人","加價",null,21000,35000,"台"]
[186,"車廂附防撞板  (橡膠)",null,"F-1000kg","加價",null,36000,60000,"台"]
[187,"車廂附防撞板  (橡膠)",null,"F-1500kg~2000kg","加價",null,42000,70000,"台"]
[188,"車廂附防撞板  (橡膠)",null,"F-2500kg~3000kg","加價",null,51000,85000,"台"]
[189,"車廂附防撞板  不鏽鋼",null,"F-1000kg","加價",null,24000,40000,"台"]
[190,"車廂附防撞板  不鏽鋼",null,"F-1500kg~2000kg","加價",null,30000,50000,"台"]
[191,"車廂附防撞板  不鏽鋼",null,"F-2500kg~3000kg","加價",null,35400,59000,"台"]
[192,"車廂預留裝潢重量",null,null,"加價",null,null,150,"KG"]

{"sheet":"A-3車廂外部","index":3,"n_rows":91,"n_cols":8,"rows_kept":91,"cut":false,"hidden":false,"merged":[[0,0,0,7],[76,1,77,1],[78,1,79,1]]}
["A-3 車廂外部"]
["序號","名稱","編號","規格/備註","配置","成本(NT)","定價","單位"]
["A-3-1 小門框"]
[1,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t發紋不銹鋼","加價",641.3966442477855,1500,"停"]
[2,"小門框(標準：噴塗Q235A-1.5t)\n",null,"噴塗Q235A-1.2t","加價",-42.499115044247787,0,"停"]
[3,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.2t發紋不銹鋼","加價",556.31341592920353,1300,"停"]
[4,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t鏡面不銹鋼","加價",844.28741946902403,2300,"停"]
[5,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t鏡面不銹鋼 鍍鈦","加價",1433.3251539823018,3500,"停"]
[6,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t鏡面不銹鋼 蝕刻","加價",1164.9857415929189,5000,"停"]
[7,"小門框(標準：噴塗Q235A-1.5t)\n",null,"SUS304-1.5t鏡面不銹鋼 蝕刻 鍍鈦","加價",1727.844021238941,7500,"停"]
[8,"小型門框 髮紋不鏽鋼 鍍鈦",null,"2P-CO ≦OP-800~1100",null,{"$f":"G11*0.6","v":2280},3800,"停"]
[9,"小型門框 鏡面不鏽鋼",null,"2P-CO ≦OP-800~1100",null,{"$f":"G12*0.6","v":2220},3700,"停"]
[10,"小型門框 鏡面不鏽鋼 鍍鈦",null,"2P-CO ≦OP-800~1100",null,2760,4600,"停"]
[11,"小型門框 髮紋不鏽鋼",null,"2P-CO≦OP-800~1100*2300H",null,1320,2200,"停"]
[12,"小型門框 仿鍍鈦烤漆",null,"2P-CO ≦OP-800~1100",null,2400,4000,"停"]
[13,"大型門框 髮紋不鏽鋼HH=2100 A=240",null,"OP-800~1100  A值≦380",null,8040,13400,"停"]
[14,"大型門框 髮紋不鏽鋼鍍鈦 HH=2100 A=240",null,"OP-800~1100  A值≦380",null,12540,20900,"停"]
[15,"大型門框 鏡面不鏽鋼 HH=2100 A=240",null,"OP-800~1100  A值≦380",null,10380,17300,"停"]
[16,"大型門框 鏡面不鏽鋼 鍍鈦 HH=2100 A=240",null,"OP-800~1100  A值≦380",null,15420,25700,"停"]
[17,"大型門框 仿鍍鈦烤漆 HH=2100 A=240",null,"OP-800~1100  A值≦380",null,7140,11900,"停"]
[18,"小型門框附幕板 髮紋不鏽鋼",null,"OP-800~1100 全高≦3000",null,9000,15000,"停"]
[19,"小型門框附幕板 髮紋不鏽鋼 鍍鈦",null,"OP-800~1100 全高≦3000",null,13260,22100,"停"]
[20,"小型門框附幕板 鏡面不鏽鋼",null,"OP-800~1100 全高≦3000",null,10980,18300,"停"]
[21,"小型門框附幕板 鏡面不鏽鋼 鍍鈦",null,"OP-800~1100 全高≦3000",null,15060,25100,"停"]
[22,"小框附幕板  仿鍍鈦烤漆",null,"OP-800~1100 全高≦3000",null,9600,16000,"停"]
[23,"大型門框附幕板 髮紋不鏽鋼",null,"OP-800~1100 全高≦3000",null,18360,30600,"停"]
[24,"大型門框附幕板 髮紋不鏽鋼 鍍鈦",null,"OP-800~1100 全高≦3000",null,23880,39800,"停"]
[25,"大型門框附幕板 鏡面不鏽鋼",null,"OP-800~1100 全高≦3000",null,20280,33800,"停"]
[26,"大型門框附幕板 鏡面不鏽鋼 鍍鈦",null,"OP-800~1100 全高≦3000",null,25740,42900,"停"]
[27,"大框附幕板  仿鍍鈦烤漆",null,"OP-800~1100  A值≦380",null,15180,25300,"停"]
[28,"一體式門框",null,"OP-800~1100全高≦3000",null,12000,18000,"停"]
[29,"小型門框 髮紋不鏽鋼 鍍鈦",null,"2S-2P  OP-1100~1200W",null,{"$f":"G32*0.6","v":3540},5900,"停"]
[30,"小型門框 鏡面不鏽鋼",null,"2S-2P  OP-1100~1200W",null,{"$f":"G33*0.6","v":3180},5300,"停"]
[31,"小型門框 髮紋不鏽鋼 鍍鈦",null,"2S-2P  OP-1100~1200W",null,4440,7400,"停"]
[32,"大型門框 髮紋不鏽鋼",null,"2S-1100.1200  A值≦380",null,7980,13300,"停"]
[33,"大型門框 髮紋不鏽鋼 鍍鈦",null,"2S-1100.1200  A值≦380",null,13140,21900,"停"]
[34,"大型門框 鏡面不鏽鋼",null,"2S-1100.1200  A值≦380",null,12000,20000,"停"]
[35,"大型門框 鏡面不鏽鋼　鍍鈦",null,"2S-1100.1200  A值≦380",null,15780,26300,"停"]
[36,"大型門框 髮紋不鏽鋼",null,"2S-1400~1700W  A值≦380",null,9360,15600,"停"]
[37,"大型門框 髮紋不鏽鋼",null,"4C-1700~2300W  A值≦380",null,13980,23300,"停"]
["A-3-2 外呼(乘場指示器)"]
[38,"外呼","MF001","不銹鋼有底盒","標配",0,null,"停"]
[39,"外呼","MF002","並聯不銹鋼有底盒","選配",789.45132743362797,1600,"停"]
[40,"外呼","MF003","不銹鋼無底盒","選配",0,null,"停"]
[41,"外呼","MF004","並聯不銹鋼無底盒","選配",227.46902654867264,525,"停"]
[42,"外呼","MF005","液晶無底盒","選配",762.6902654867265,1600,"停"]
[43,"外呼","MF006","液晶無底盒","選配",762.6902654867265,1800,"停"]
[44,"外呼","MF007","殘障有底盒附盲文點字板","選配",414.79646017699127,1000,"停"]
[45,"外呼","MF008","殘障並聯有底盒附盲文點字板","選配",1239.9292035398205,2500,"停"]
[46,"外呼","MF009","殘障並聯手勢呼梯有底盒附盲文點字板","選配",1342.5132743362847,2700,"停"]
[47,"外呼","MF010","手勢呼梯有底盒","選配",499.539823008849,1050,"停"]
[48,"外呼","MF011","殘障無底盒附盲文點字板和MF012搭配用","選配",13.380530973451334,500,"停"]
[49,"外呼","MF012","殘障無底盒和MF011搭配用","選配",303.29203539823015,500,"停"]
[50,"外呼","MF013","無接觸式外呼","選配",3269.3097345132733,4500,"停"]
[51,"外呼","MF014","殘障+手勢呼梯有底盒附盲文點字板","選配",517.38053097344846,1500,"停"]
[52,"外呼","MF015","殘障有底盒和MF001搭配用","選配",334.51327433628313,1000,"停"]
[53,"外呼","MF016","殘障有底盒","選配",365.73451327433611,1000,"停"]
[54,"外呼","MF017","殘障手勢呼梯有底盒","選配",463.85840707964553,1000,"停"]
[55,"外呼","MF018","手勢呼梯有底盒附盲文點字板","選配",102.5840707964604,400,"停"]
[56,"外呼","MF019","並聯殘障有底盒附盲文點字板，左側","選配",1373.7345132743371,2800,"停"]
[57,"外呼","MF020","並聯殘障有底盒附盲文點字板，右側","選配",1373.7345132743371,2800,"停"]
[58,"外呼","MF021","無底盒","選配",160.56637168141577,400,"停"]
[59,"外呼","MF022","無底盒帶手勢呼梯","選配",182.86725663716851,400,"停"]
[60,"群管裡(2台聯動)",null,null,"選配",{"$f":"G64*0.6","v":4740},7900,"群"]
[61,"群管理 (3~8台/群)",null,"3~8台群管理(無群管理盤)","選配",{"$f":"G65*0.6","v":33780},56300,"群"]
[62,"人流管控(群)",null,"僅限一層樓(一般為大廳)","選配",null,"特殊詢價","群"]
["A-3-3 到站燈"]
[63,"到站燈","MG001",null,"選配",1110.5840707964594,2500,"停"]
[64,"到站燈","MG002",null,"選配",1110.5840707964594,2500,"停"]
[65,"到站燈","MG003",null,"選配",2872.3539823008882,6000,"停"]
[66,"到站燈","MG004",null,"選配",1436.1769911504421,2900,"停"]
[67,"到站燈","MG005",null,"選配",1855.4336283185864,4000,"停"]
[68,"到站燈","MG006",null,"選配",2368.3539823008882,5500,"停"]
["A-3-4 門開方式與門"]
[69,"2P-CO→2S-2P(台)",null,"P6~24人(OP≦1100)","加價",{"$f":"G75*0.6","v":4800},8000,"台"]
[70,"2P-CO→2S-2P(停)",null,"P6~24人(OP≦1100)","加價",{"$f":"G76*0.6","v":3000},5000,"停"]
[71,"貫通門-轎廂（轎門標準SUS304-1.5t）",null,"SUS304-1.5t","加價",15469.677876106171,85000,"台"]
[72,null,null,"冷軋板噴塗1.5t","加價",13089.727433628315,80000,"台"]
[73,"貫通門-乘場（層門門框標準Q235A-1.5t）",null,"冷軋板噴塗1.5t","加價",4164.9132743362798,9000,"停"]
[74,null,null,"SUS304-1.5t","加價",8151.3302654867402,15000,"停"]
[75,"千鳥型",null,"P9人","加價",{"$f":"G81*0.6","v":78000},130000,"台"]
[76,"千鳥型",null,"P10~P11人","加價",{"$f":"G82*0.6","v":96000},160000,"台"]
[77,"千鳥型",null,"P12~P15人","加價",90000,150000,"台"]
[78,"千鳥型",null,"P17~P24人","加價",79200,132000,"台"]
[79,"L型千鳥",null,"P9人","加價",195000,325000,"台"]
[80,"L型千鳥",null,"P10~P11人","加價",216000,360000,"台"]
[81,"L型千鳥",null,"P12~P15人","加價",204000,340000,"台"]
[82,"千鳥型",null,"貨梯1000kg~2000kg ","加價",90000,150000,"台"]
[83,"千鳥型",null,"貨梯2500kg~3000kg","加價",120000,200000,"台"]
[87,"防火門(停)(2P-CO)",null,"不鏽鋼","加價",19200,32000,"停"]
[89,"防火門(停)(2S-2P)",null,"不鏽鋼","加價",24000,40000,"停"]

{"sheet":"A-4控制與其他","index":4,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[[0,0,0,7]]}
["A-4 控制與其他"]
["序號","名稱","編號","規格/備註","配置","成本(NT)","定價","單位"]
["A-4-1 功能與配置"]
[1,"專用運轉",null,"操作電梯，可提供客戶做專用運轉(例：看來車廂人滿了,直接經過外面叫車之樓層，直接到達服務樓層","加價",{"$f":"G4*0.6","v":720},1200,"台"]
[2,"車廂追加到樓鈴",null,"到樓鈴: 電子","加價",{"$f":"G5*0.6","v":1500},2500,"台"]
[3,"乘場追加到樓鈴",null,"到樓鈴: 電子","加價",780,1300,"停"]
[4,"對講機配線至管理員室以100M計(不含配管)　　　　　　　　　　",null,null,"加價",10500,17500,"台"]
[5,"對講機線材100M計　　　　　　　　　　",null,null,"加價",6720,11200,"台"]
[6,"車廂預留電話機接點",null,"僅接點預留","加價",8040,13400,"台"]
[7,"追加電話機(工廠配合留孔)",null,null,"加價",420,700,"台"]
[8,"追加電話機(工事現地配合鑽孔)",null,"針對現地配合的人工費用","加價",4200,7000,"台"]
[9,"車廂預留刷卡機接點",null,"僅接點預留","加價",7800,13000,"台"]
[10,"車廂預留刷卡機接點+面板開孔",null,"僅接點預留&面板留孔","加價",9480,15800,"台"]
[11,"遠隔監控 (組)",null,"1~7台/組 (配賦於第1台)","加價",9480,15800,"台"]
[12,"遠隔監控工事配線費(EAS)",null,null,"加價",3780,6300,"台"]
[13,"物聯網(BY工務購買)",null,"1~4台/組用, 5~8台/2組","加價",10860,18100,"組"]
[14,"廂內監控(需搭配物聯網)",null,"物聯網費用需另計","加價",116820,194700,"台"]
[15,"直話機系統",null,"與車廂內\"緊急呼叫\"共用按鈕\n1.按下3秒內,為一般緊急呼叫,可與升降道外對講\n2.按著超過3秒以上,則直接撥通電話至設定的第一組號碼(一般來說可設置6組號碼)，無人接聽時往下一組號碼撥號\n(需請客戶申請市話，方能用電話線接進去，需預先錄製語音)\n適用:EAS,VAG","加價",10560,17600,"台"]
[16,"火警受信運轉",null,"WL432","加價",4334.4000000000005,6300,"套"]
[17,"火災管制",null,"火災管制：當兩台電梯聯動時，其中一台為緊急用電梯，則隔壁台需有火災管制功能","加價",{"$f":"G20*0.6","v":2880},4800,"台"]
[18,"緊急用",null,"緊急用：一、建築物高度超過十層樓以上部分之最大一層樓地板面積，在1500平方公尺以下者，至少應設置一座：超過1500平方公尺時，每達3000平方公尺，增設一座。","加價",{"$f":"G21*0.6","v":10200},17000,"台"]
[19,"ARD",null,"四、超過十層樓之各層樓地板面積之和未達500平方公尺者不需設置。","加價",7156.8,39000,"套"]
[20,"停機操作",null,null,"加價",100.8,500,"套"]
[21,"滿載直駛",null,"操作盤檢修增加直駛開關非標加價","加價",1008,3000,"套"]
[22,"能量回饋",null,null,"加價",14822.64,42000,"套"]
[23,"對重附安全鉗（包含限速器等）",null,"P8-P15","加價",15610.619469026518,42000,"組"]
[24,"對重附安全鉗（包含限速器等）",null,"P17",null,{"$f":"G27*0.6","v":37800},63000]
[25,"對重附安全鉗（包含限速器等）",null,"P24",null,{"$f":"G28*0.6","v":44100},73500]
[26,"井道頂部追加防沖梁",null,null,"加價",2520,6500,"台"]
[27,"人臉識別",null,null,"加價",{"$f":"G30*0.6","v":39000},65000,"套"]
[null,"地震感知器"]
["A-4-2 OH與樓高"]
[28,"OH ≧7.5M",null,"P6~P11人","加價",{"$f":"G33*0.6","v":9300},15500,"台"]
[29,"OH ≧7.5M",null,"P12~P15人","加價",{"$f":"G34*0.6","v":10140},16900,"台"]
[30,"OH ≧7.5M",null,"P17~P24人","加價",12120,20200,"台"]
[31,"OH ≧7.5M",null,"B-750~1000kg ","加價",11040,18400,"台"]
[32,"OH ≧7.5M",null,"F-1000kg ","加價",12420,20700,"台"]
[33,"OH ≧7.5M",null,"F-1500~2000kg ","加價",15300,25500,"台"]
[34,"OH ≧7.5M",null,"F-2500~3000kg ","加價",21180,35300,"台"]
[35,"OH 超過6M",null,null,"加價",3780,6300,"台"]
[36,"OH>5M,追加吊樑施工",null,"僅VAG無機房機種","加價",3780,6300,"台"]
[37,"樓高 ≧ 6M",null,"P6~P11人","加價",8280,13800,"樓"]
[38,"樓高 ≧ 6M",null,"P12~P15人","加價",9060,15100,"樓"]
[39,"樓高 ≧ 6M",null,"P17~P24人","加價",11160,18600,"樓"]
[40,"樓高 ≧ 6M",null,"B-750~1000kg ","加價",10080,16800,"樓"]
[41,"樓高 ≧ 6M",null,"F-1000kg ","加價",11520,19200,"樓"]
[42,"樓高 ≧ 6M",null,"F-1500~2000kg ","加價",14340,23900,"樓"]
[43,"樓高 ≧ 6M",null,"F-2500~3000kg ","加價",20280,33800,"樓"]