{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["工作表1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"工作表1","index":0,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[18,0,21,2]]}
["強驅梯  MAQ100",null,null,null,"單位:萬元"]
[" 規                格","產品系列","樓層","標準價","(±1S) "]
["MAQ100-4*-4PCO24","G5",4,70,2]
["MAQ100-4*-4PCO24","G6",4,70,2]
["MAQ100-4*-4PCO24","G10",4,72.5,2]
["MAQ100-4*-4PCO24","G20",4,72.5,2]
["MAQ100-4*-4PCO24","A2",4,77.5,2]
["MAQ100-4*-4PCO24","A3",4,78.7,2]
["MAQ100-4*-4PCO24","A6",4,77.5,2]
["MAQ100-4*-4PCO24","A8",4,78.7,2]
["MAQ100-4*-2PCO24","G5",4,68,2]
["MAQ100-4*-2PCO24","G6",4,68,2]
["MAQ100-4*-2PCO24","G10",4,70.5,2]
["MAQ100-4*-2PCO24","G20",4,70.5,2]
["MAQ100-4*-2PCO24","A2",4,75.5,2]
["MAQ100-4*-2PCO24","A3",4,76.5,2]
["MAQ100-4*-2PCO24","A6",4,75.5,2]
["MAQ100-4*-2PCO24","A8",4,76.5,2]
["註\n1、處長權限為發佈價之80%\n2、開門改2PCO，井道不變時，出入口寬需由800mm變成為600mm；或井道需加寬400mm"]